(footprint "Valve_Noval_G"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Valve NOVAL G")
	(tags "Valve NOVAL G")
	(property "Reference" "REF**"
		(at 7.11 4.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Valve_Noval_G"
		(at 8.38 19.56 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "d=18,0mm"
		(at -7.62 17.41 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -7.62 10.16 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 6.99 10.16)
		(size 4.5 4.5)
		(drill 4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -22.23 10.16)
		(size 4.5 4.5)
		(drill 4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -7.62 -2.54)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -15.24 0)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -20.32 3.81)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -20.32 16.51)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -15.24 20.32)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -7.62 22.86)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 20.32)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 5.08 16.51)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Valve.3dshapes/Valve_Noval_G.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
