(footprint "RV_Rect_V25S440P_L26.5mm_W8.2mm_P12.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Varistor, V25S440P, https://www.littelfuse.com/media?resourcetype=datasheets&itemid=b410c42c-51d1-460e-b1d9-d105d93c9679&filename=littelfuse-varistor-ultramov25s-datasheet")
	(tags "varistor")
	(property "Reference" "REF**"
		(at 0.3 -8.15 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RV_Rect_V25S440P_L26.5mm_W8.2mm_P12.7mm"
		(at 1.7 6.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.2 5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 4.3 12.7)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Varistor.3dshapes/RV_Rect_V25S440P_L26.5mm_W8.2mm_P12.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
