(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BAC05S05DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "BAC05S05DC"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Murata_BAC05SxxDC_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8809982558238/KAC-BAC05.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "5V, 1A, 5W, Isolated, AC-DC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply muRataPs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Murata*BAC05S*DC*THT*"
			(at 0 0 0)
		)
		(symbol "BAC05S05DC_0_1")
		(symbol "BAC05S05DC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLK-12M05A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M05A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
		(symbol "HLK-12M05A_0_1")
		(symbol "HLK-12M05A_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLK-30M05"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M05"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
		(symbol "HLK-30M05_0_1")
		(symbol "HLK-30M05_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "6")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLK-PM01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM01"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
		(symbol "HLK-PM01_0_1")
		(symbol "HLK-PM01_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HS-40003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40003"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/de/Document/d4b3c52125889c3435af182c9515c76b/HS40003.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "3.3V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "3.3V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
		(symbol "HS-40003_0_1")
		(symbol "HS-40003_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "7")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-02-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-3.3"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "3.3V, 600mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-02-3.3_0_1")
		(symbol "IRM-02-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-02-3.3S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-3.3S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 600mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
		(symbol "IRM-02-3.3S_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "24")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "12")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-03-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "3.3V, 900mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-03-3.3_0_1")
		(symbol "IRM-03-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "16")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-03-3.3S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-3.3S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "3.3V, 900mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
		(symbol "IRM-03-3.3S_0_1")
		(symbol "IRM-03-3.3S_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "16")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-05-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-05-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-05-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-05/IRM-05-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "3.3V, 1.25A, 4.125W, Isolated, AC-DC, 222A(IRM05)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*05*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-05-3.3_0_1")
		(symbol "IRM-05-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-10-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-10-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-10/IRM-10-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "3.3V, 2.5A, 8.25W, Isolated, AC-DC, 222A(IRM10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*10*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-10-3.3_0_1")
		(symbol "IRM-10-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-20-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-20-3.3"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-20-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.meanwell.com/Upload/PDF/IRM-20/IRM-20-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "3.3V, 4.5A, 14.85W, Isolated, AC-DC, 219A(IRM20)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*20*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-20-3.3_0_1")
		(symbol "IRM-20-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRM-60-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 7.62 0)
		)
		(property "Value" "IRM-60-5"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-60-xx_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.meanwellusa.com/productPdf.aspx?i=687"
			(at 0 0 0)
		)
		(property "Description" "5V, 10A, 50W, Isolated, AC-DC, IRM60"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*60*THT*"
			(at 0 0 0)
		)
		(symbol "IRM-60-5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MFM-10-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-10-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell-web.com/content/files/pdfs/productPdfs/MW/MFM-10/MFM-10-spec.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 3.3V, 10 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*10*THT*"
			(at 0 0 0)
		)
		(symbol "MFM-10-3.3_0_1")
		(symbol "MFM-10-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MFM-15-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-15-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-15-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 3.3V, 15 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*15*THT*"
			(at 0 0 0)
		)
		(symbol "MFM-15-3.3_0_1")
		(symbol "MFM-15-3.3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PBO-3-S3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S3.3"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 0.6A 1.98W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
		(symbol "PBO-3-S3.3_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "AC(L)")
				(number "3")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "+V(CAP)")
				(number "5")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "-V(CAP)")
				(number "7")
			)
			(pin power_in line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "+Vo")
				(number "12")
			)
			(pin power_out line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "-Vo")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC01-xxSGB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC01-xxSGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC01-xxSGB_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC01-GB.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "1 Watt Single Output EMC Class B AC/DC power supply with regulated and short-circuit-proof isolated DC outputs and low standby power consumption."
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC01*SGB*THT*"
			(at 0 0 0)
		)
		(symbol "RAC01-xxSGB_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC04-xxSGA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-xxSGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
		(symbol "RAC04-xxSGA_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC04-xxSGB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-xxSGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
		(symbol "RAC04-xxSGB_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC05-3.3SK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC05-3.3SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC05-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC05-K.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "5W Single Output EMC Class B 3.3V 1515mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC05*SK*"
			(at 0 0 0)
		)
		(symbol "RAC05-3.3SK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC20-05SK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-05SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "20 Watt Single Output AC/DC power supply 5V 4000mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*SK*THT*"
			(at 0 0 0)
		)
		(symbol "RAC20-05SK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAC20-12DK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-12DK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxDK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at 0 0 0)
		)
		(property "Description" "20 Watt Dual Output AC/DC power supply ±12V ±833mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*DK*THT*"
			(at 0 0 0)
		)
		(symbol "RAC20-12DK_0_1")
		(symbol "RAC20-12DK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Com")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMF05105"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF05105"
			(at 3.048 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_051xx_THT"
			(at 0.254 0 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf05.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "5W AC/DC power supply, 5V fixed output voltage, 1A output, 4.0kVAC isolation"
			(at 0 -8.636 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*051xx*THT*"
			(at 0 0 0)
		)
		(symbol "TMF05105_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMF10105"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF10105"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_101xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf10.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "10W AC/DC power supply, 5V fixed output voltage, 2A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 10W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*101xx*THT*"
			(at 0 0 0)
		)
		(symbol "TMF10105_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMF20105"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF20105"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_201xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf20.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "18W AC/DC power supply, 5V fixed output voltage, 3.6A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 18W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*201xx*THT*"
			(at 0 0 0)
		)
		(symbol "TMF20105_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMF30105"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF30105"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_301xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf30.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "25W AC/DC power supply, 5V fixed output voltage, 5A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 25W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*301xx*THT*"
			(at 0 0 0)
		)
		(symbol "TMF30105_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vout")
				(number "5")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMLM04103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04103"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1200mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
		(symbol "TMLM04103_0_1")
		(symbol "TMLM04103_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout+")
				(number "2")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vout-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMLM04225"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04225"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 250mA / 5V 120mA AC/DC dual output, low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
		(symbol "TMLM04225_0_1")
		(symbol "TMLM04225_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AC(L)")
				(number "5")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "AC(N)")
				(number "6")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout1")
				(number "2")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "Common")
				(number "3")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Vout2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMLM05103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM05103"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-05_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 1250mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 5W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*05*"
			(at 0 0 0)
		)
		(symbol "TMLM05103_0_1")
		(symbol "TMLM05103_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout+")
				(number "2")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vout-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMLM10103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM10103"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 2500mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
		(symbol "TMLM10103_0_1")
		(symbol "TMLM10103_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout+")
				(number "2")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vout-")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPP-15-103-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-103-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "3.3V, 4000mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
		(symbol "TPP-15-103-D_0_1")
		(symbol "TPP-15-103-D_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AC/L")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AC/N")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "+Vo")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "Trim")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "-Vo")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTX-214-010-103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-103"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "3V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "3V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
		(symbol "VTX-214-010-103_0_1")
		(symbol "VTX-214-010-103_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "N")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DC+")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DC-")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTX-214-015-103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-103"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "3V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "3V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
		(symbol "VTX-214-015-103_0_1")
		(symbol "VTX-214-015-103_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "L")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "N")
				(number "2")
			)
			(pin no_connect line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "FG")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DC+")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DC-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLK-10M03"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M03"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-10M05"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M05"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-10M09"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-10M12"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-10M15"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-10M24"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-10M24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-10Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9710W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9110W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.8.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 10W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?10M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-12M03A"
		(extends "HLK-12M05A")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M03A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-12M09A"
		(extends "HLK-12M05A")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M09A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-12M12A"
		(extends "HLK-12M05A")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M12A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-12M15A"
		(extends "HLK-12M05A")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M15A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-12M24A"
		(extends "HLK-12M05A")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-12M24A"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-12MxxA"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9712W%E7%B3%BB%E5%88%97/1/12W%E7%B3%BB%E5%88%97%E8%A7%84%E6%A0%BC%E4%B9%A6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 12W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?12M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-20M05"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-20M05"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-20Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9720W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9120W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 20W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?20M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-20M09"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-20M09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-20Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9720W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9120W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 20W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?20M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-20M12"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-20M12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-20Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9720W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9120W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 20W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?20M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-20M15"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-20M15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-20Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9720W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9120W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 20W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?20M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-20M24"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-20M24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-20Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9720W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9120W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 20W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?20M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M03"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M03"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M05"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M05"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M09"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M12"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M15"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-2M24"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-2M24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-2Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%972W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%912W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%AF%B4%E6%98%8E%E4%B9%A6V2.6.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 2W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?2M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M05C"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M05C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130WC%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M09"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M09C"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M09C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130WC%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M12"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M12C"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M12C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130WC%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M15"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M15C"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M15C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130WC%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M24"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.6.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-30M24C"
		(extends "HLK-30M05")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-30M24C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-30Mxx"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%9730W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%9130WC%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V1.2.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 30W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?30M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M03"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M03"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 3.3V 1.5A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M05"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M05"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 5V 1A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M09"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 9V 0.560A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M12"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 12V 0.420A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M15"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 15V 0.333A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-5M24"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-5M24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-5Mxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Compact AC/DC board mount power module 5W, 24V 0.208A"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?5M*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-PM03"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM03"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 3V3"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-PM09"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM09"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 9V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-PM12"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-PM15"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
	)
	(symbol "HLK-PM24"
		(extends "HLK-PM01")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HLK-PM24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 24V"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC/DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hi?Link*HLK?PM*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40005"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40005"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/de/Document/996b08915f81126361ce1f9c12d2f8b9/HS40005.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "5V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40009"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40009"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/de/Document/cd3ff0c74e0c3bb183174aa10baf8730/HS40009.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "9V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "9V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40012"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40012"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/de/Document/221b247820f4fbb72e0cbc1ee10acb85/HS40012.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "12V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40015"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40015"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.schukat.com/schukat/pdf.nsf/index/956F3869A8D071A1C1257B810041B129/$file/HS-40015-Serie%20Schemazeichnung-A3%20(1).pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "15V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40018"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40018"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.schukat.com/schukat/pdf.nsf/index/6A4EEAC16DA84B74C1257B810041DC7B/$file/HS-40018-Serie%20Schemazeichnung-A3%20(1).pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "18V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "18V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "HS-40024"
		(extends "HS-40003")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "HS-40024"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hahn_HS-400xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.schukat.com/schukat/pdf.nsf/index/17647BA7403E2D39C1257B810041F34E/$file/HS-40024-Serie%20Schemazeichnung-A3%20(1).pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "24V, 3W, AC-DC module power supply, Hahn"
			(at 0 0 0)
		)
		(property "ki_keywords" "24V 3W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Hahn*HS*400xx*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-12"
		(extends "IRM-02-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "12V, 167mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-12S"
		(extends "IRM-02-3.3S")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-12S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "12V, 167mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-15"
		(extends "IRM-02-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "15V, 133mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-15S"
		(extends "IRM-02-3.3S")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-15S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "15V, 133mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-24"
		(extends "IRM-02-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "24V, 83mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-24S"
		(extends "IRM-02-3.3S")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-24S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "24V, 83mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-5"
		(extends "IRM-02-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-5"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "5V, 400mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-5S"
		(extends "IRM-02-3.3S")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-5S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "5V, 400mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-9"
		(extends "IRM-02-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-9"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "9V, 222mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-02-9S"
		(extends "IRM-02-3.3S")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-02-9S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_SMD"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 0)
		)
		(property "Description" "9V, 222mA, 2W, Isolated, AC-DC, IRM02-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*02*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-12"
		(extends "IRM-03-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-12"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "12V, 250mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-12S"
		(extends "IRM-03-3.3S")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-12S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "12V, 250mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-15"
		(extends "IRM-03-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-15"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "15V, 200mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-15S"
		(extends "IRM-03-3.3S")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-15S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "15V, 200mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-24"
		(extends "IRM-03-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-24"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "24V, 125mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-24S"
		(extends "IRM-03-3.3S")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-24S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "24V, 125mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-5"
		(extends "IRM-03-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "5V, 600mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-5S"
		(extends "IRM-03-3.3S")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-5S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "5V, 600mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-9"
		(extends "IRM-03-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-9"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "9V, 333mA, 3W, Isolated, AC-DC, IRM03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-03-9S"
		(extends "IRM-03-3.3S")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-03-9S"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_SMD"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "9V, 333mA, 3W, Isolated, AC-DC, IRM03-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*SMD*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-05-12"
		(extends "IRM-05-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-05-12"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-05-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-05/IRM-05-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "12V, 420mA, 5.04W, Isolated, AC-DC, 222A(IRM05)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*05*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-05-15"
		(extends "IRM-05-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-05-15"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-05-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-05/IRM-05-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "15V, 330mA, 4.95W, Isolated, AC-DC, 222A(IRM05)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*05*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-05-24"
		(extends "IRM-05-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-05-24"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-05-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-05/IRM-05-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "24V, 230mA, 5.52W, Isolated, AC-DC, 222A(IRM05)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*05*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-05-5"
		(extends "IRM-05-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-05-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-05-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-05/IRM-05-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "5V, 1A, 5W, Isolated, AC-DC, 222A(IRM05)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*05*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-10-12"
		(extends "IRM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-10-12"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-10/IRM-10-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "12V, 850mA, 10.2W, Isolated, AC-DC, 222A(IRM10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-10-15"
		(extends "IRM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-10-15"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-10/IRM-10-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "15V, 670mA, 10.05W, Isolated, AC-DC, 222A(IRM10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-10-24"
		(extends "IRM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-10-24"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-10/IRM-10-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "24V, 420mA, 10.08W, Isolated, AC-DC, 222A(IRM10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-10-5"
		(extends "IRM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "IRM-10-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-10/IRM-10-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "5V, 2A, 10W, Isolated, AC-DC, 222A(IRM10)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-20-12"
		(extends "IRM-20-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-20-12"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-20-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.meanwell.com/Upload/PDF/IRM-20/IRM-20-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "12V, 1.8A, 21.6W, Isolated, AC-DC, 219A(IRM20)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*20*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-20-15"
		(extends "IRM-20-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-20-15"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-20-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.meanwell.com/Upload/PDF/IRM-20/IRM-20-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "15V, 1.4A, 21W, Isolated, AC-DC, 219A(IRM20)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*20*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-20-24"
		(extends "IRM-20-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-20-24"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-20-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.meanwell.com/Upload/PDF/IRM-20/IRM-20-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "24V, 900mA, 21.6W, Isolated, AC-DC, 219A(IRM20)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*20*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-20-5"
		(extends "IRM-20-3.3")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "IRM-20-5"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-20-xx_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.meanwell.com/Upload/PDF/IRM-20/IRM-20-SPEC.PDF"
			(at 10.16 -8.89 0)
		)
		(property "Description" "5V, 4A, 20W, Isolated, AC-DC, 219A(IRM20)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*20*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-60-12"
		(extends "IRM-60-5")
		(property "Reference" "PS"
			(at 0 7.62 0)
		)
		(property "Value" "IRM-60-12"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-60-xx_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.meanwellusa.com/productPdf.aspx?i=687"
			(at 0 0 0)
		)
		(property "Description" "12V, 5A, 60W, Isolated, AC-DC, IRM60"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*60*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-60-15"
		(extends "IRM-60-5")
		(property "Reference" "PS"
			(at 0 7.62 0)
		)
		(property "Value" "IRM-60-15"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-60-xx_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.meanwellusa.com/productPdf.aspx?i=687"
			(at 0 0 0)
		)
		(property "Description" "15V, 4A, 60W, Isolated, AC-DC, IRM60"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*60*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-60-24"
		(extends "IRM-60-5")
		(property "Reference" "PS"
			(at 0 7.62 0)
		)
		(property "Value" "IRM-60-24"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-60-xx_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.meanwellusa.com/productPdf.aspx?i=687"
			(at 0 0 0)
		)
		(property "Description" "24V, 2.5A, 60W, Isolated, AC-DC, IRM60"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*60*THT*"
			(at 0 0 0)
		)
	)
	(symbol "IRM-60-48"
		(extends "IRM-60-5")
		(property "Reference" "PS"
			(at 0 7.62 0)
		)
		(property "Value" "IRM-60-48"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-60-xx_THT"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.meanwellusa.com/productPdf.aspx?i=687"
			(at 0 0 0)
		)
		(property "Description" "48V, 1.25A, 50W, Isolated, AC-DC, IRM60"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*60*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-10-12"
		(extends "MFM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-10-12"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell-web.com/content/files/pdfs/productPdfs/MW/MFM-10/MFM-10-spec.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 12V, 10 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-10-15"
		(extends "MFM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-10-15"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell-web.com/content/files/pdfs/productPdfs/MW/MFM-10/MFM-10-spec.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 15V, 10 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-10-24"
		(extends "MFM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-10-24"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell-web.com/content/files/pdfs/productPdfs/MW/MFM-10/MFM-10-spec.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 24V, 10 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-10-5"
		(extends "MFM-10-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-10-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-10-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell-web.com/content/files/pdfs/productPdfs/MW/MFM-10/MFM-10-spec.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 5V, 10 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*10*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-15-12"
		(extends "MFM-15-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-15-12"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-15-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 12V, 15 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-15-15"
		(extends "MFM-15-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-15-15"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-15-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 15V, 15 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-15-24"
		(extends "MFM-15-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-15-24"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-15-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 24V, 15 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "MFM-15-5"
		(extends "MFM-15-3.3")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "MFM-15-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_MFM-15-xx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF"
			(at 0 -10.16 0)
		)
		(property "Description" "Meanwell AC/DC converter, 80-264VAC, output 5V, 15 watts"
			(at 0 0 0)
		)
		(property "ki_keywords" "Miniature Module-type Power Supply MeanWell"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*MeanWell*MFM*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "PBO-3-S12"
		(extends "PBO-3-S3.3")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S12"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 0.25A 3W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "PBO-3-S15"
		(extends "PBO-3-S3.3")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S15"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 0.2A 3W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "PBO-3-S24"
		(extends "PBO-3-S3.3")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S24"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V 0.125A 3W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "PBO-3-S5"
		(extends "PBO-3-S3.3")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S5"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 0.6A 3W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "PBO-3-S9"
		(extends "PBO-3-S3.3")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "PBO-3-S9"
			(at 0 11.43 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_CUI_PBO-3-Sxx_THT_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cui.com/product/resource/pbo-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V 0.333A 3W miniature AC-DC module-type power supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*CUI*PBO*3*Sxx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC01-05SGB"
		(extends "RAC01-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC01-05SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC01-xxSGB_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC01-GB.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "1 Watt Single Output EMC Class B AC/DC 5V 200mA power supply with regulated and short-circuit-proof isolated DC outputs and low standby power consumption."
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC01*SGB*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC01-12SGB"
		(extends "RAC01-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC01-12SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC01-xxSGB_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC01-GB.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "1 Watt Single Output EMC Class B AC/DC 12V 83mA power supply with regulated and short-circuit-proof isolated DC outputs and low standby power consumption."
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC01*SGB*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC01-24SGB"
		(extends "RAC01-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC01-24SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC01-xxSGB_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC01-GB.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "1 Watt Single Output EMC Class B AC/DC 24V 42mA power supply with regulated and short-circuit-proof isolated DC outputs and low standby power consumption."
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC01*SGB*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC01-3.3SGB"
		(extends "RAC01-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC01-3.3SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC01-xxSGB_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC01-GB.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "1 Watt Single Output EMC Class B AC/DC 3.3V 303mA power supply with regulated and short-circuit-proof isolated DC outputs and low standby power consumption."
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC01*SGB*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-05SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-05SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 5V 800mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-05SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-05SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 5V 800mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-09SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-09SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 9V 440mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-09SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-09SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 9V 440mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-12SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-12SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 12V 330mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-12SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-12SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 12V 330mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-15SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-15SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 15V 270mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-15SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-15SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 15V 270mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-24SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-24SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 24V 170mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-24SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-24SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 24V 170mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-3.3SGA"
		(extends "RAC04-xxSGA")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-3.3SGA"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GA.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class A - 3.3V 1210mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC04-3.3SGB"
		(extends "RAC04-xxSGB")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC04-3.3SGB"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC04-xxSGx_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC04-GB.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "4 Watt Single Output EMC Class B - 3.3V 1210mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC04*SG*"
			(at 0 0 0)
		)
	)
	(symbol "RAC05-05SK"
		(extends "RAC05-3.3SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC05-05SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC05-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC05-K.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "5W Single Output EMC Class B 5V 1000mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC05*SK*"
			(at 0 0 0)
		)
	)
	(symbol "RAC05-12SK"
		(extends "RAC05-3.3SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC05-12SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC05-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC05-K.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "5W Single Output EMC Class B 12V 416mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC05*SK*"
			(at 0 0 0)
		)
	)
	(symbol "RAC05-15SK"
		(extends "RAC05-3.3SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC05-15SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC05-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC05-K.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "5W Single Output EMC Class B 15V 333mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC05*SK*"
			(at 0 0 0)
		)
	)
	(symbol "RAC05-24SK"
		(extends "RAC05-3.3SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC05-24SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_RECOM_RAC05-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.recom-power.com/pdf/Powerline-AC-DC/RAC05-K.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "5W Single Output EMC Class B 24V 210mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*RECOM*RAC05*SK*"
			(at 0 0 0)
		)
	)
	(symbol "RAC20-12SK"
		(extends "RAC20-05SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-12SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "20 Watt Single Output AC/DC power supply 12V 1670mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*SK*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC20-15DK"
		(extends "RAC20-12DK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-15DK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxDK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at 0 0 0)
		)
		(property "Description" "20 Watt Dual Output AC/DC power supply ±15V ±670mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*DK*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC20-15SK"
		(extends "RAC20-05SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-15SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "20 Watt Single Output AC/DC power supply 15V 1333mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*SK*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC20-24SK"
		(extends "RAC20-05SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-24SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "20 Watt Single Output AC/DC power supply 24V 840mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*SK*THT*"
			(at 0 0 0)
		)
	)
	(symbol "RAC20-48SK"
		(extends "RAC20-05SK")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "RAC20-48SK"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Recom_RAC20-xxSK_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Powerline_AC-DC/RAC20-K.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "20 Watt Single Output AC/DC power supply 48V 420mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "ac dc power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Recom*RAC20*SK*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF05112"
		(extends "TMF05105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF05112"
			(at 3.048 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_051xx_THT"
			(at 0.254 0 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf05.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "5W AC/DC power supply, 12V fixed output voltage, 417mA output, 4.0kVAC isolation"
			(at 0 -8.636 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*051xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF05115"
		(extends "TMF05105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF05115"
			(at 3.048 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_051xx_THT"
			(at 0.254 0 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf05.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "5W AC/DC power supply, 15V fixed output voltage, 333mA output, 4.0kVAC isolation"
			(at 0 -8.636 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*051xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF05124"
		(extends "TMF05105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF05124"
			(at 3.048 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_051xx_THT"
			(at 0.254 0 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf05.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "5W AC/DC power supply, 24V fixed output voltage, 208mA output, 4.0kVAC isolation"
			(at 0 -8.636 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 5W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*051xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF10112"
		(extends "TMF10105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF10112"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_101xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf10.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "10W AC/DC power supply, 12V fixed output voltage, 833mA output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 10W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*101xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF10115"
		(extends "TMF10105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF10115"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_101xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf10.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "10W AC/DC power supply, 15V fixed output voltage, 666mA output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 10W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*101xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF10124"
		(extends "TMF10105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF10124"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_101xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf10.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "10W AC/DC power supply, 24V fixed output voltage, 417mA output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 10W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*101xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF20112"
		(extends "TMF20105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF20112"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_201xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf20.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "20W AC/DC power supply, 12V fixed output voltage, 1.667A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 20W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*201xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF20115"
		(extends "TMF20105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF20115"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_201xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf20.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "20W AC/DC power supply, 15V fixed output voltage, 1.333A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 20W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*201xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF20124"
		(extends "TMF20105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF20124"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_201xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf20.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "20W AC/DC power supply, 24V fixed output voltage, 833mA output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 20W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*201xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF30112"
		(extends "TMF30105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF30112"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_301xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf30.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "30W AC/DC power supply, 12V fixed output voltage, 2.5A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 30W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*301xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF30115"
		(extends "TMF30105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF30115"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_301xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf30.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "30W AC/DC power supply, 15V fixed output voltage, 2A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 30W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*301xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMF30124"
		(extends "TMF30105")
		(property "Reference" "PS"
			(at -6.604 6.096 0)
		)
		(property "Value" "TMF30124"
			(at 2.794 6.096 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMF_301xx_THT"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmf30.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "30W AC/DC power supply, 24V fixed output voltage, 1.25A output, 4.0kVAC isolation"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco isolated isolation ac-dc AC/DC medical power-supply 30W"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMF*301xx*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04105"
		(extends "TMLM04103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04105"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 800mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04109"
		(extends "TMLM04103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04109"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "9V 444mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04112"
		(extends "TMLM04103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04112"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 333mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04115"
		(extends "TMLM04103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04115"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 267mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04124"
		(extends "TMLM04103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04124"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V 167mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM04253"
		(extends "TMLM04225")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM04253"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-04_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 600mA / 3.3V 150mA AC/DC dual output, low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 4W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*04*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM05105"
		(extends "TMLM05103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM05105"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-05_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 1000mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 5W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*05*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM05112"
		(extends "TMLM05103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM05112"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-05_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 420mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 5W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*05*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM05115"
		(extends "TMLM05103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM05115"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-05_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 333mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 5W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*05*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM05124"
		(extends "TMLM05103")
		(property "Reference" "PS"
			(at 0 6.35 0)
		)
		(property "Value" "TMLM05124"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-05_THT"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V 230mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 5W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*05*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM10105"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM10105"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 2000mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM10112"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM10112"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 833mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM10115"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM10115"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V 667mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM10124"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM10124"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V 417mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM20103"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM20103"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 3600mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 20W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM20105"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM20105"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V 3600mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 20W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM20112"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM20112"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 1660mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 20W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM20115"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM20115"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V 1330mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 20W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TMLM20124"
		(extends "TMLM10103")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TMLM20124"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TMLM-10-20_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/products/tmlm.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V 833mA AC/DC low noise power module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Traco Power 20W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TMLM*10*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-105-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-105-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "5V, 3000mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-109-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-109-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "9V, 1670mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-112-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-112-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "12V, 1250mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-115-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-115-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "15V, 1000mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-124-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-124-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "24V, 625mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-136-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-136-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "36V, 417mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "TPP-15-148-D"
		(extends "TPP-15-103-D")
		(property "Reference" "PS"
			(at 0 5.08 0)
		)
		(property "Value" "TPP-15-148-D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_TRACO_TPP-15-1xx-D_THT"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.tracopower.com/sites/default/files/products/datasheets/tpp15_d_datasheet.pdf"
			(at 10.16 -8.89 0)
		)
		(property "Description" "48V, 313mA, 15W, Isolated, AC-DC, Traco"
			(at 0 0 0)
		)
		(property "ki_keywords" "Medical Power Supply Traco"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*TRACO*TPP*15*THT*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-105"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-105"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "5V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-106"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-106"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "6V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "6V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-107"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-107"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "7.5V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "7.5V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-108"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-108"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "8V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "8V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-109"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-109"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "9V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "9V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-110"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-110"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "10V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "10V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-112"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-112"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "12V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-115"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-115"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "15V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-118"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-118"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "18V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "18V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-124"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-124"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "24V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "24V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-010-148"
		(extends "VTX-214-010-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-010-148"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-010-xxx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/10WattACDCPCBPowerModule.aspx"
			(at 27.94 -20.32 0)
		)
		(property "Description" "48V Vigortronix 10W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "48V 10W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*010*xxx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-105"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-105"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "5V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "5V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-106"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-106"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "6V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "6V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-107"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-107"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "7V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "7V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-109"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-109"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "9V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "9V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-112"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-112"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "12V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "12V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-115"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-115"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "15V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "15V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-118"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-118"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "18V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "18V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-124"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-124"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "24V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "24V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
	(symbol "VTX-214-015-148"
		(extends "VTX-214-015-103")
		(property "Reference" "PS"
			(at 0 8.89 0)
		)
		(property "Value" "VTX-214-015-148"
			(at 0 6.35 0)
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Vigortronix_VTX-214-015-1xx_THT"
			(at 0 11.43 0)
		)
		(property "Datasheet" "http://www.vigortronix.com/15WattSMPSPCBModuleAC-DC"
			(at 27.94 -20.32 0)
		)
		(property "Description" "48V Vigortronix 15W ACDC Converters"
			(at 0 0 0)
		)
		(property "ki_keywords" "48V 15W AC-DC module power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*ACDC*Vigortronix*VTX*214*015*1xx*"
			(at 0 0 0)
		)
	)
)
