(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "1.5KExxA"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1.5KExxA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1500W unidirectional TVS diode, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor TRANSZORB®"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
		(symbol "1.5KExxA_0_1")
		(symbol "1.5KExxA_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1.5KExxCA"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1.5KExxCA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500W bidirectional TVS diode, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor TRANSZORB®"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
		(symbol "1.5KExxCA_0_1")
		(symbol "1.5KExxCA_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1N4001"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4001"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
		(symbol "1N4001_0_1")
		(symbol "1N4001_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1N5711UR"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5711UR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/131890-lds-0040-1-datasheet"
			(at 0 0 0)
		)
		(property "Description" "70V 33mA Schottky diode, MELF(DO-213AA)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?MELF*"
			(at 0 0 0)
		)
		(symbol "1N5711UR_0_1")
		(symbol "1N5711UR_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1N5820"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5820"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88526/1n5820.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 3A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
		(symbol "1N5820_0_1")
		(symbol "1N5820_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1N6263"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N6263"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/1n6263.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 15mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
		(symbol "1N6263_0_1")
		(symbol "1N6263_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2BZX84Cxx"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.81 2.54 0)
		)
		(property "Value" "2BZX84Cxx"
			(at 3.81 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bzx84c2v4.pdf"
			(at -2.54 0 90)
		)
		(property "Description" "300mW Double Zener Diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "2BZX84Cxx_0_1")
		(symbol "2BZX84Cxx_1_1"
			(pin passive line
				(at -2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B120-E3"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B120-E3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
		(symbol "B120-E3_0_1")
		(symbol "B120-E3_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B220"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B220"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
		(symbol "B220_0_1")
		(symbol "B220_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B320"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B320"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 3A Schottky Barrier Rectifier Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMC*"
			(at 0 0 0)
		)
		(symbol "B320_0_1")
		(symbol "B320_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAR42FILM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAR42FILM"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/bar42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.1A Small signal Schottky diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAR42FILM_0_1")
		(symbol "BAR42FILM_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at 1.27 1.27 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAS16TW"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS16TW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30154.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAS16TW_0_1")
		(symbol "BAS16TW_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "BAS16TW_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(symbol "BAS16TW_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAS16W"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS16W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "BAS16W_0_1")
		(symbol "BAS16W_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAS40-04"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -1.27 0)
		)
		(property "Value" "BAS40-04"
			(at -6.35 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at -6.35 7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85701/bas40v.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "40V 0.2A Dual Small Signal Schottky Diodes"
			(at 0 0 0)
		)
		(property "ki_keywords" "Schottky, Diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAS40-04_0_1")
		(symbol "BAS40-04_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT160A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT160A"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT160_SERIES.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual schottky barrier diode, common anode, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BAT160A_0_1")
		(symbol "BAT160A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at 0 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT160C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT160C"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT160_SERIES.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual schottky barrier diode, common cathode, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BAT160C_0_1")
		(symbol "BAT160C_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at 0 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT160S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT160S"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT160_SERIES.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual schottky barrier diode, in series, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BAT160S_0_1")
		(symbol "BAT160S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at 0 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT54A"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at -3.048 0 0)
		)
		(property "Description" "schottky barrier diode"
			(at 0 0 0)
		)
		(property "ki_keywords" "schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAT54A_0_1")
		(symbol "BAT54A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54ADW"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT54ADW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30152.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Schottky diode array 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAT54ADW_0_1")
		(symbol "BAT54ADW_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "BAT54ADW_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "BAT54ADW_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "BAT54ADW_4_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54AW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT54AW"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT54W_SER.pdf"
			(at -3.048 0 0)
		)
		(property "Description" "Dual schottky barrier diode, common anode, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "BAT54AW_0_1")
		(symbol "BAT54AW_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT54C"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at -2.032 0 0)
		)
		(property "Description" "dual schottky barrier diode, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "schottky diode common cathode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAT54C_0_1")
		(symbol "BAT54C_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54CW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT54CW"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT54W_SER.pdf"
			(at -2.032 0 0)
		)
		(property "Description" "Dual schottky barrier diode, common cathode, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "BAT54CW_0_1")
		(symbol "BAT54CW_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54S"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 -5.08 0)
		)
		(property "Value" "BAT54S"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds11005.pdf"
			(at -3.048 0 0)
		)
		(property "Description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAT54S_0_1")
		(symbol "BAT54S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 5.08)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54SDW"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT54SDW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/BAT54TW_ADW_CDW_SDW_BRW.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Schottky diode array 2 pair Com A, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAT54SDW_0_1")
		(symbol "BAT54SDW_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "BAT54SDW_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "BAT54SDW_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(symbol "BAT54SDW_4_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAT54W"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT54W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT54W_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "Schottky barrier diode, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "BAT54W_0_1")
		(symbol "BAT54W_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at 0 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV70"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -2.54 0)
		)
		(property "Value" "BAV70"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 100V 215mA high-speed switching diodes, common cathode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAV70_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV70S"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.635 -2.54 0)
		)
		(property "Value" "BAV70S"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 250mA high-speed switching diodes, dual common cathode, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAV70S_0_1")
		(symbol "BAV70S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "A")
				(number "2")
			)
		)
		(symbol "BAV70S_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "A")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV756S"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV756S"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV756S_BAW56_SER.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "High-speed switching diodes, dual common anode/common cathode, SOT-363"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAV756S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "CK")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "A4")
				(number "5")
			)
		)
		(symbol "BAV756S_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "K2")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "K3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV99"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "BAV99"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "BAV99 High-speed switching diodes, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BAV99_0_1")
		(symbol "BAV99_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV99S"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV99S"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-speed switching diodes, dual series, SOT-363"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BAV99S_0_1")
		(symbol "BAV99S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K3A4")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "K2")
				(number "2")
			)
		)
		(symbol "BAV99S_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "K1A2")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "K4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BZX84Cxx"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 3.81 0)
		)
		(property "Value" "BZX84Cxx"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bzx84c2v4.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mW Zener Diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BZX84Cxx_0_1")
		(symbol "BZX84Cxx_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at 1.27 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3D02060F"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D02060F"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/35/C3D02060F.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 2A, SiC Schottky Diode, TO-220F"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*"
			(at 0 0 0)
		)
		(symbol "C3D02060F_0_1")
		(symbol "C3D02060F_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3D06060G"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06060G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/137/C3D06060G.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 6A, SiC Schottky Diode, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin1*"
			(at 0 0 0)
		)
		(symbol "C3D06060G_0_1")
		(symbol "C3D06060G_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3D16060D"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C3D16060D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/98/C3D16060D.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 16A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
		(symbol "C3D16060D_0_1")
		(symbol "C3D16060D_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3D1P7060Q"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D1P7060Q"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_QFN_3.3x3.3mm_P0.65mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/846/C3D1P7060Q.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 1.7A, SiC Schottky Diode, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*QFN*3.3x3.3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "C3D1P7060Q_0_1")
		(symbol "C3D1P7060Q_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C4D10120H"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D10120H"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/1189/C4D10120H.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 10A, SiC Schottky Diode, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
		(symbol "C4D10120H_0_1")
		(symbol "C4D10120H_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD01060E"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CSD01060E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/87/CSD01060.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 1A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
		(symbol "CSD01060E_0_1")
		(symbol "CSD01060E_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB3"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 3.81 0)
		)
		(property "Value" "DB3"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -5.715 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A100/DB%203%23st.pdf"
			(at 0 0 0)
		)
		(property "Description" "32V 2A Bidirectional trigger diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC diode DIAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
		(symbol "DB3_0_1")
		(symbol "DB3_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESD9B5.0ST5G"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESD9B5.0ST5G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-923"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "ESD protection diode, 5.0Vrwm, SOD-923"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?923*"
			(at 0 0 0)
		)
		(symbol "ESD9B5.0ST5G_0_1")
		(symbol "ESD9B5.0ST5G_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDDD04G65C6"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD04G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD04G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628f749daa0e03"
			(at 0 0 0)
		)
		(property "Description" "650V, 4A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
		(symbol "IDDD04G65C6_0_1")
		(symbol "IDDD04G65C6_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "10")
			)
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "7")
			)
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "8")
			)
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(hide yes)
				(name "K")
				(number "9")
			)
			(pin no_connect line
				(at 1.27 1.27 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 1.27 -1.27 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LL41"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LL41"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85659/bat41.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.1A Small Signal Schottky diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
		(symbol "LL41_0_1")
		(symbol "LL41_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MBR735"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR735"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBR735-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "35V 7.5A Schottky Barrier Rectifier Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "MBR735_0_1")
		(symbol "MBR735_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMEG2005EJ"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2005EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
		(symbol "PMEG2005EJ_0_1")
		(symbol "PMEG2005EJ_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMEG2010AET"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010AET"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010AEH_PMEG2010AET.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "PMEG2010AET_0_1")
		(symbol "PMEG2010AET_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at 0 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMEG4050EP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4050EP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-128"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4050EP.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 5A low Vf Schottky barrier rectifier, SOD-128"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?128*"
			(at 0 0 0)
		)
		(symbol "PMEG4050EP_0_1")
		(symbol "PMEG4050EP_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMEG40T10ER"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG40T10ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG40T10ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A low Vf Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
		(symbol "PMEG40T10ER_0_1")
		(symbol "PMEG40T10ER_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMEG45A10EPD"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG45A10EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG45A10EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 10A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
		(symbol "PMEG45A10EPD_0_1")
		(symbol "PMEG45A10EPD_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Rohm_UMN1N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Rohm_UMN1N"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/diode/switching/umn1ntr-e.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High-speed switching diodes 2 pair Com K"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "Rohm_UMN1N_0_1")
		(symbol "Rohm_UMN1N_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "Rohm_UMN1N_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "Rohm_UMN1N_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(symbol "Rohm_UMN1N_4_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Rohm_UMP11N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Rohm_UMP11N"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/diode/switching/ump11ntn-e.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High-speed switching diodes 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "Rohm_UMP11N_0_1")
		(symbol "Rohm_UMP11N_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "Rohm_UMP11N_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "Rohm_UMP11N_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "4")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(symbol "Rohm_UMP11N_4_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SB120"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB120"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds23022.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
		(symbol "SB120_0_1")
		(symbol "SB120_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SD05_SOD323"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SD05_SOD323"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sd_c_datasheet.pdf.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 450W Discrete Bidirectional TVS Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323*"
			(at 0 0 0)
		)
		(symbol "SD05_SOD323_0_1")
		(symbol "SD05_SOD323_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SD103ATW"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -1.27 2.54 0)
		)
		(property "Value" "SD103ATW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30374.pdf"
			(at 0 0 0)
		)
		(property "Description" "Schottky Barrier Diode Array, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "schottky barrier diode array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "SD103ATW_0_1")
		(symbol "SD103ATW_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "SD103ATW_2_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "5")
			)
		)
		(symbol "SD103ATW_3_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SM6T6V8A"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T6V8A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 6.8Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
		(symbol "SM6T6V8A_0_1")
		(symbol "SM6T6V8A_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SM712_SOT23"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 4.445 0)
		)
		(property "Value" "SM712_SOT23"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sm712_datasheet.pdf.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "7V/12V, 600W Asymmetrical TVS Diode Array, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SM712_SOT23_0_0")
		(symbol "SM712_SOT23_0_1")
		(symbol "SM712_SOT23_1_1"
			(pin passive line
				(at -8.89 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at 0 -3.81 90)
				(length 2.54)
				(name "common")
				(number "3")
			)
			(pin passive line
				(at 8.89 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STTH2002D"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "STTH2002D"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stth2002.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "200V 20A Ultrafast Recovery Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*2*"
			(at 0 0 0)
		)
		(symbol "STTH2002D_0_0"
			(pin no_connect line
				(at 0 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
		)
		(symbol "STTH2002D_0_1")
		(symbol "STTH2002D_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STTH2002G"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "STTH2002G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stth2002.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "200V 20A Ultrafast Recovery Diode, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "STTH2002G_0_0"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
		)
		(symbol "STTH2002G_0_1")
		(symbol "STTH2002G_1_1"
			(pin no_connect line
				(at 0 0 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STTH212S"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "STTH212S"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stth212.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V 2A High Voltage Ultrafast Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMC*"
			(at 0 0 0)
		)
		(symbol "STTH212S_0_1")
		(symbol "STTH212S_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VS-6ESU06"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "VS-6ESU06"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-277A"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/94987/vs-6esu06hm3.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 6.0A Ultrafast Rectifier, TO-277A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode fred"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?277A*"
			(at 0 0 0)
		)
		(symbol "VS-6ESU06_0_1")
		(symbol "VS-6ESU06_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZPYxx"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZPYxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85790/zpy3v9.pdf"
			(at 0 0 0)
		)
		(property "Description" "1300mW Zener Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
		(symbol "ZPYxx_0_1")
		(symbol "ZPYxx_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1.5SMCxxA"
		(extends "1.5KExxA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1.5SMCxxA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88303/15smc.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1500W unidirectional TVS diode, SMC (DO-201AB)"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor TRANSZORB®"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMC*"
			(at 0 0 0)
		)
	)
	(symbol "1.5SMCxxCA"
		(extends "1.5KExxCA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1.5SMCxxCA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88303/15smc.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500W bidirectional TVS diode, SMC (DO-201AB)"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor TRANSZORB®"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMC*"
			(at 0 0 0)
		)
	)
	(symbol "1N4002"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4002"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4003"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4003"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4004"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4004"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4005"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4005"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4006"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4006"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4007"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4007"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4148"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4148"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N4148W"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4148W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85748/1n4148w.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast Switching Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "1N4148WS"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4148WS"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85751/1n4148ws.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "1N4148WT"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4148WT"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "1N4149"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4149"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_view/11580-lds-0239"
			(at 0 0 0)
		)
		(property "Description" "75V Vrm 0.5A Ifsm standard switching diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N4151"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4151"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_view/11580-lds-0239"
			(at 0 0 0)
		)
		(property "Description" "75V 0.5A standard switching diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N4448"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4448"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A High-speed standard diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N4448W"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4448W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85722/1n4448w.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A High-speed standard diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "1N4448WS"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4448WS"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81387/1n4448ws.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Small Signal Fast switching Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "1N4448WT"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4448WT"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/149/1N4148WT-461550.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "1N47xxA"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N47xxA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85816/1n4728a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1300mW Silicon planar power Zener diodes, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4933"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4933"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88508/1n4933.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast Switching Plastic Rectifier, VRRM 50V, IF(AV) 1.0A, trr 200ns, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N53xxB"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N53xxB"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/1n5345b.pdf"
			(at 0 0 0)
		)
		(property "Description" "5000mW Zener Diode, DO-201"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201*"
			(at 0 0 0)
		)
	)
	(symbol "1N5400"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5400"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5401"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5401"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5402"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5402"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5403"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5403"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "300V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5404"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5404"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5405"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5405"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "500V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5406"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5406"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5407"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5407"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5408"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5408"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5711"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5711"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "70V 33mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N5712"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5712"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 75mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N5712UR"
		(extends "1N5711UR")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5712UR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/131890-lds-0040-1-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 75mA Schottky diode, MELF(DO-213AA)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?MELF*"
			(at 0 0 0)
		)
	)
	(symbol "1N5817"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5817"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N5818"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5818"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N5819"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5819"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N5819WS"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5819WS"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204281430_Guangdong-Hottech-1N5819WS_C191023.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 600mV@1A 1A SOD-323 Schottky Barrier Diodes, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "1N5821"
		(extends "1N5820")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5821"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88526/1n5820.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 3A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5822"
		(extends "1N5820")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5822"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88526/1n5820.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "1N5908"
		(extends "1.5KExxA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N5908"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/1n5908.pdf"
			(at -1.016 -4.572 0)
		)
		(property "Description" "1500W (10/1000 μs) Unidirectional TVS Diode, VRM = 5V (IRM = 300 μA at 25°C), VBR = 6V, DO-201AE"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
	)
	(symbol "1N62xxA"
		(extends "1.5KExxA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N62xxA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1500W unidirectional TRANSZORB® Transient Voltage Suppressor, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
	)
	(symbol "1N62xxCA"
		(extends "1.5KExxCA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N62xxCA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500W bidirectional TRANSZORB® Transient Voltage Suppressor, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
	)
	(symbol "1N630xA"
		(extends "1.5KExxA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N630xA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "1500W unidirectional TRANSZORB® Transient Voltage Suppressor, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
	)
	(symbol "1N630xCA"
		(extends "1.5KExxCA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N630xCA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AE_P15.24mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88301/15ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500W bidirectional TRANSZORB® Transient Voltage Suppressor, DO-201AE"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?DO?201AE*"
			(at 0 0 0)
		)
	)
	(symbol "1N6857"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N6857"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 150mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N6857UR"
		(extends "1N5711UR")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N6857UR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/131890-lds-0040-1-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 150mA Schottky diode, MELF(DO-213AA)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?MELF*"
			(at 0 0 0)
		)
	)
	(symbol "1N6858"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N6858"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "70V 75mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N6858UR"
		(extends "1N5711UR")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N6858UR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/131890-lds-0040-1-datasheet"
			(at 0 0 0)
		)
		(property "Description" "70V 75mA Schottky diode, MELF(DO-213AA)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?MELF*"
			(at 0 0 0)
		)
	)
	(symbol "1N914"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N914"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85622/1n914.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.3A Small Signal Fast Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "1N914WT"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N914WT"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/149/1N4148WT-461550.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "1SS355VM"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1SS355VM"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/diode/switching/1ss355vmte-17-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "90V 0.1A high speed switching Diode, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "5KPxxA"
		(extends "1.5KExxA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "5KPxxA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_P600_R-6_P20.00mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/5kp65.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "5000W unidirectional Transient Voltage Suppressor, P-600"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?P600*"
			(at 0 0 0)
		)
	)
	(symbol "5KPxxCA"
		(extends "1.5KExxCA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "5KPxxCA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_P600_R-6_P20.00mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/5kp65.pdf"
			(at 0 0 0)
		)
		(property "Description" "5000W bidirectional Transient Voltage Suppressor, P-600"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?P600*"
			(at 0 0 0)
		)
	)
	(symbol "B130-E3"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B130-E3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "B140-E3"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B140-E3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "B150-E3"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B150-E3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "B160-E3"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B160-E3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "B230"
		(extends "B220")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B230"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "B240"
		(extends "B220")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B240"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "B250"
		(extends "B220")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B250"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "B260"
		(extends "B220")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B260"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "B330"
		(extends "B320")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B330"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 3A Schottky Barrier Rectifier Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "B340"
		(extends "B320")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B340"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "B350"
		(extends "B320")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B350"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 3A Schottky Barrier Rectifier Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "B360"
		(extends "B320")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "B360"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 3A Schottky Barrier Rectifier Diode, SMC"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "BA157"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA157"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88536/ba157.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V 1A Fast recovery Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "BA158"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA158"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88536/ba157.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 1A Fast recovery Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "BA159"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA159"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88536/ba157.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V 1A Fast recovery Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "BA243"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA243"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/BA243_TFK.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 0.1A silicon planar diode for VHF tuner band selection, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BA244"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA244"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/BA243_TFK.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 0.1A silicon planar diode for VHF tuner band selection, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BA282"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA282"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://docs-europe.electrocomponents.com/webdocs/1304/0900766b813040d6.pdf"
			(at 0 0 0)
		)
		(property "Description" "35V 0.1A Band Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BA283"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BA283"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://docs-europe.electrocomponents.com/webdocs/1304/0900766b813040d6.pdf"
			(at 0 0 0)
		)
		(property "Description" "35V 0.1A Band Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAR43FILM"
		(extends "BAR42FILM")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAR43FILM"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/bar43.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.1A Small signal Schottky diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BAS16VY"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS16VY"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BAS19"
		(extends "BAS16W")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS19"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/Ds12004.pdf"
			(at 0 0 0)
		)
		(property "Description" "120V, 0.4A, High-speed Switching Diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BAS20"
		(extends "BAS16W")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS20"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/Ds12004.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V, 0.4A, High-speed Switching Diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BAS21"
		(extends "BAS16W")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS21"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/Ds12004.pdf"
			(at 0 0 0)
		)
		(property "Description" "250V, 0.4A, High-speed Switching Diode, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BAS316"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS316"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 0.25A, High-speed Switching Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "BAS516"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAS516"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 0.25A, High-speed Switching Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "BAT41"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT41"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85659/bat41.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.1A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT42"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT42"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT42W-V"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT42W-V"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "BAT43"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT43"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT43W-V"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT43W-V"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "BAT46"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT46"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85662/bat46.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT48JFILM"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT48JFILM"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/bat48.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 0.35A Small Signal Schottky Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "BAT48RL"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT48RL"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/bat48.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 0.35A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT48ZFILM"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT48ZFILM"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/bat48.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 0.35A Small Signal Schottky Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "BAT54J"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT54J"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT54J.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 200mA Schottky diode, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "BAT54SW"
		(extends "BAT54S")
		(property "Reference" "D"
			(at 0.635 -3.81 0)
		)
		(property "Value" "BAT54SW"
			(at -6.35 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 1.905 3.175 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT54W_SER.pdf"
			(at -3.048 0 0)
		)
		(property "Description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual schottky diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BAT60A"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT60A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BAT60ASERIES-DS-v01_01-en.pdf?fileId=db3a304313d846880113def70c9304a9"
			(at 0 0 0)
		)
		(property "Description" "10V 3A High Current Recitifier Schottky Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "BAT85"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT85"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT85.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Schottky barrier single diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT86"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT86"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAT86.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAT86S"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAT86S"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85514/bat86s.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV16W"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV16W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30086.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Fast Switching Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "BAV17"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV17"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85543/bav17.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 0.25A Small Signal Switching Diode, High Voltage, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV18"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV18"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85543/bav17.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.25A Small Signal Switching Diode, High Voltage, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV19"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV19"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85543/bav17.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.25A Small Signal Switching Diode, High Voltage, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV199DW"
		(extends "BAV99S")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV199DW"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30417.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Surface Mount Low Leakage Diode, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BAV20"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV20"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85543/bav17.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 0.25A Small Signal Switching Diode, High Voltage, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV21"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV21"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85543/bav17.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 0.25A Small Signal Switching Diode, High Voltage, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAV300"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV300"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85545/bav300.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.25A Switching Diode, High Voltage, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BAV301"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV301"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85545/bav300.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.25A Switching Diode, High Voltage, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BAV302"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV302"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85545/bav300.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 0.25A Switching Diode, High Voltage, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BAV303"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAV303"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85545/bav300.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 0.25A Switching Diode, High Voltage, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BAV70M"
		(extends "BAV70")
		(property "Reference" "D"
			(at 0.635 -2.54 0)
		)
		(property "Value" "BAV70M"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-883"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 100V 150mA high-speed switching diodes, common cathode, SOT-883"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?883*"
			(at 0 0 0)
		)
	)
	(symbol "BAV70T"
		(extends "BAV70")
		(property "Reference" "D"
			(at 0.635 -2.54 0)
		)
		(property "Value" "BAV70T"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-416"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 100V 150mA high-speed switching diodes, common cathode, SOT-416"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?416*"
			(at 0 0 0)
		)
	)
	(symbol "BAV70W"
		(extends "BAV70")
		(property "Reference" "D"
			(at 0.635 -2.54 0)
		)
		(property "Value" "BAV70W"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual 100V 175mA high-speed switching diodes, common cathode, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BAW56DW"
		(extends "Rohm_UMP11N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAW56DW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30146.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Switching diode array 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BAW56S"
		(extends "Rohm_UMP11N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAW56S"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV756S_BAW56_SER.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High Speed Switching Diode Array 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BAW75"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAW75"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85550/baw75.pdf"
			(at 0 0 0)
		)
		(property "Description" "25V 0.45A Small Signal Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAW76"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAW76"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85551/baw76.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.3A Small Signal Fast Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BAY93"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BAY93"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://cdn-reichelt.de/documents/datenblatt/A400/BAY93_TFK.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 0.115A Very Fast Switching Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "BYV79-100"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BYV79-100"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/philips/BYV79-100.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 14A Ultrafast Rectifier Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BYV79-150"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BYV79-150"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/philips/BYV79-100.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 14A Ultrafast Rectifier Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BYV79-200"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BYV79-200"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/philips/BYV79-100.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 14A Ultrafast Rectifier Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BZD27Cxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZD27Cxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85153/bzd27series.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mW Zener Diode, 3.6-200V, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "BZM55Bxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZM55Bxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85597/bzm55.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mW Zener Diode, 2%, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZM55Cxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZM55Cxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85597/bzm55.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mW Zener Diode, 6%, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZT52Bxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZT52Bxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bzt52b2v4.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mW Zener Diode, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B10"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B10"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B11"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B11"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "11V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B12"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B12"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B13"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B13"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "13V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B15"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B15"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B16"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B16"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "16V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B18"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B18"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B20"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B20"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B22"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B22"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "22V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B24"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B24"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B27"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B27"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.4V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B2V4"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B2V4"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.4V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B2V7"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B2V7"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B30"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B30"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B33"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B33"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "33V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B36"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B36"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "36V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B39"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B39"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B3V0"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B3V0"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B3V3"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B3V3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B3V6"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B3V6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.6V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B3V9"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B3V9"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.9V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B43"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B43"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "43V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B47"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B47"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "47V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B4V3"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B4V3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.3V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B4V7"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B4V7"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.7V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B51"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B51"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "51V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B56"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B56"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "56V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B5V1"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B5V1"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.1V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B5V6"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B5V6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.6V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B62"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B62"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "62V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B68"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B68"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "68V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B6V2"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B6V2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "6.2V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B6V8"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B6V8"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "6.8V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B75"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B75"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B7V5"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B7V5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B8V2"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B8V2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "8.2V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55B9V1"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55B9V1"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "9.1V, 500mW, 2%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C10"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C10"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C11"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C11"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "11V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C12"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C12"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C13"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C13"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "13V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C15"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C15"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C16"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C16"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "16V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C18"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C18"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C20"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C20"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C22"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C22"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "22V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C24"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C24"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C27"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C27"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "27V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C2V4"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C2V4"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.4V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C2V7"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C2V7"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C30"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C30"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C33"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C33"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "33V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C36"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C36"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "36V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C39"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C39"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "39V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C3V0"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C3V0"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C3V3"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C3V3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C3V6"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C3V6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.6V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C3V9"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C3V9"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.9V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C43"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C43"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "43V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C47"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C47"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "47V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C4V3"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C4V3"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.3V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C4V7"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C4V7"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.7V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C51"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C51"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "51V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C56"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C56"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "56V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C5V1"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C5V1"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.1V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C5V6"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C5V6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.6V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C62"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C62"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "62V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C68"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C68"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "68V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C6V2"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C6V2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "6.2V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C6V8"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C6V8"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "6.8V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C75"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C75"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C7V5"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C7V5"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C8V2"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C8V2"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "8.2V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZV55C9V1"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZV55C9V1"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BZV55_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "9.1V, 500mW, 5%, Zener diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "BZX384xxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "BZX384xxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85764/bzx384.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mW Zener Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD*323*"
			(at 0 0 0)
		)
	)
	(symbol "C3D02060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D02060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/55/C3D02060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 2A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D02060E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D02060E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/116/C3D02060E.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 2A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D02065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D02065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/118/C3D02065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 2A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D03060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D03060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/57/C3D03060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 3A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D03060E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D03060E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/119/C3D03060E.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 3A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D03060F"
		(extends "C3D02060F")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D03060F"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/39/C3D03060F.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 3A, SiC Schottky Diode, TO-220F"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*"
			(at 0 0 0)
		)
	)
	(symbol "C3D03065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D03065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/121/C3D03065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 3A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D04060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D04060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/845/C3D04060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 4A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D04060E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D04060E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/122/C3D04060E.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 4A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D04060F"
		(extends "C3D02060F")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D04060F"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/41/C3D04060F.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 4A, SiC Schottky Diode, TO-220F"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*"
			(at 0 0 0)
		)
	)
	(symbol "C3D04065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D04065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/841/C3D04065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 4A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D04065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D04065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/124/C3D04065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 4A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D06060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/844/C3D06060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 6A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D06060F"
		(extends "C3D02060F")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06060F"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/43/C3D06060F.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 6A, SiC Schottky Diode, TO-220F"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*"
			(at 0 0 0)
		)
	)
	(symbol "C3D06065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/65/C3D06065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 6A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D06065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/125/C3D06065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 6A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D06065I"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D06065I"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/44/C3D06065I.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 6A, SiC Schottky Diode, Isolated TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D08060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D08060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/843/C3D08060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 8A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D08060G"
		(extends "C3D06060G")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D08060G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/141/C3D08060G.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 8A, SiC Schottky Diode, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D08065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D08065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/840/C3D08065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 8A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D08065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D08065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/839/C3D08065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 8A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D08065I"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D08065I"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/47/C3D08065I.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 8A, SiC Schottky Diode, Isolated TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/842/C3D10060A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 10A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10060G"
		(extends "C3D06060G")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10060G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/143/C3D10060G.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 10A, SiC Schottky Diode, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/73/C3D10065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 10A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10065E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10065E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/127/C3D10065E.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 10A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10065I"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10065I"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/49/C3D10065I.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 10A, SiC Schottky Diode, Isolated TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D10170H"
		(extends "C4D10120H")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D10170H"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/96/C3D10170H.pdf"
			(at 0 0 0)
		)
		(property "Description" "1700V, 10A, SiC Schottky Diode, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3D12065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D12065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/963/C3D12065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 12A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D16065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D16065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/964/C3D16065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 16A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C3D16065D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C3D16065D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/99/C3D16065D.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 16A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3D20060D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C3D20060D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/100/C3D20060D.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 20A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3D20065D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C3D20065D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/102/C3D20065D.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 20A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3D25170H"
		(extends "C4D10120H")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C3D25170H"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/103/C3D25170H.pdf"
			(at 0 0 0)
		)
		(property "Description" "1700V, 25A, SiC Schottky Diode, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3D30065D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C3D30065D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/969/C3D30065D.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 30A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D02120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D02120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/75/C4D02120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 2A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D02120E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D02120E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/128/C4D02120E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 2A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C4D05120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D05120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/77/C4D05120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 5A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D05120E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D05120E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/130/C4D05120E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 5A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C4D08120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D08120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/80/C4D08120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 8A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D08120E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D08120E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/132/C4D08120E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 8A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C4D10120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D10120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/82/C4D10120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 10A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D10120D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C4D10120D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/104/C4D10120D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 10A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D10120E"
		(extends "CSD01060E")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D10120E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2_TabPin1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/134/C4D10120E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 10A, SiC Schottky Diode, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin1*"
			(at 0 0 0)
		)
	)
	(symbol "C4D15120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D15120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/84/C4D15120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 15A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D15120D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C4D15120D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/848/C4D15120D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 15A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D15120H"
		(extends "C4D10120H")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D15120H"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/1190/C4D15120H.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 15A, SiC Schottky Diode, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D20120A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D20120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/85/C4D20120A.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 20A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "C4D20120D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C4D20120D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/106/C4D20120D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 20A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D20120H"
		(extends "C4D10120H")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "C4D20120H"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/1191/C4D20120H.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 20A, SiC Schottky Diode, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D30120D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C4D30120D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/108/C4D30120D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 30A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C4D40120D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C4D40120D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/109/C4D40120D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 40A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C5D50065D"
		(extends "C3D16060D")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "C5D50065D"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/111/C5D50065D.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 50A, SiC Schottky Diode, TO-247-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "CD4148W"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CD4148W"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.dccomponents.com/upload/product/original/623524775088.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.15A Switching Diode, 0805"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*0805*"
			(at 0 0 0)
		)
	)
	(symbol "CDBA3100-HF"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CDBA3100-HF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/CDBA340-HF%20Thru193640.%20CDBA3100-HF%20RevB.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 3A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "CDBA340-HF"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CDBA340-HF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/CDBA340-HF%20Thru193640.%20CDBA3100-HF%20RevB.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "CDBA360-HF"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CDBA360-HF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/CDBA340-HF%20Thru193640.%20CDBA3100-HF%20RevB.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 3A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "CDBU40-HF"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CDBU40-HF"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_0603_1608Metric"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/QW-G1012-CDBU40-HF-RevA321692.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 200mA Schottky Barrier Rectifier Diode, 0603"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*0603*"
			(at 0 0 0)
		)
	)
	(symbol "CSD01060A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CSD01060A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/87/CSD01060.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 1A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "CVFD20065A"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "CVFD20065A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/89/CVFD20065A.pdf"
			(at 0 0 0)
		)
		(property "Description" "650V, 20A, SiC Schottky Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "Central_Semi_CMKD4448"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Central_Semi_CMKD4448"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.centralsemi.com/PDFs/products/CMKD4448.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "High speed switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "Central_Semi_CMKD6001"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Central_Semi_CMKD6001"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.centralsemi.com/PDFs/products/CMKD6001.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Ultra low leakage switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "Comchip_ACDSV6-4448TI-G"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Comchip_ACDSV6-4448TI-G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.comchiptech.com/cms/UserFiles/ACDSV6-4448TI-G%20RevA285610.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Small signal switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "Comchip_CDSV6-4148-G"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Comchip_CDSV6-4148-G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.comchiptech.com/cms/UserFiles/CDSV6-16-G,4148-G%20RevA272279.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "Comchip_CDSV6-4448TI-G"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Comchip_CDSV6-4448TI-G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.comchiptech.com/cms/UserFiles/CDSV6-4448XX-G%20RevC285574.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High speed switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "DB4"
		(extends "DB3")
		(property "Reference" "D"
			(at 0 3.81 0)
		)
		(property "Value" "DB4"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -5.715 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A100/DB%203%23st.pdf"
			(at 0 0 0)
		)
		(property "Description" "34V 2A Bidirectional trigger diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC diode DIAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "DC34"
		(extends "DB3")
		(property "Reference" "D"
			(at 0 3.81 0)
		)
		(property "Value" "DC34"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -5.715 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A100/DB%203%23st.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 2A Bidirectional trigger diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC diode DIAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "DSB2810"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DSB2810"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 75mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "DSB5712"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DSB5712"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/8865-lds-0040-datasheet"
			(at 0 0 0)
		)
		(property "Description" "20V 75mA Schottky diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S030X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S030X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S03000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 3.0V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S033X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S033X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S03300L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 3.3V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S036X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S036X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S03600L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 3.6V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S039X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S039X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S03900L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 3.9V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S047X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S047X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S04700L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 4.7V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S051X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S051X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S05100L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 5.1V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S056X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S056X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S05600L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 5.6V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S068X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S068X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S06800L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 6.8V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S082X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S082X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S08200L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 8.2V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S100X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S100X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S10000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 10V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S110X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S110X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S11000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 11V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S120X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S120X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S12000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 12V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S130X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S130X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S13000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 13V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S150X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S150X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S15000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 15V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S160X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S160X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S16000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 16V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S180X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S180X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S18000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 18V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S200X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S200X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S20000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 20V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "DZ2S360X0L"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DZ2S360X0L"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/DZ2S36000L_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mW Silicon Planar Zener Diode, 36V, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "ESD131-B1-W0201"
		(extends "ESD9B5.0ST5G")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESD131-B1-W0201"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Infineon_SG-WLL-2-3_0.58x0.28_P0.36mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ESD131-B1-W0201-DataSheet-v02_00-EN.pdf?fileId=5546d4625cc9456a015ce94850964889"
			(at 0 0 0)
		)
		(property "Description" "Bidirectional ESD protection diode, ±5.5Vrwm, 0.23pF, SG-WLL-2-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SG?WLL?2?3*"
			(at 0 0 0)
		)
	)
	(symbol "ESD5Zxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESD5Zxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/esd5z2.5t1-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "ESD Protection Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "esd tvs unidirectional diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "ESD9B3.3ST5G"
		(extends "ESD9B5.0ST5G")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESD9B3.3ST5G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-923"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "ESD protection diode, 3.3Vrwm, SOD-923"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?923*"
			(at 0 0 0)
		)
	)
	(symbol "ESH2PB"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESH2PB"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMP_DO-220AA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/89016/esh2pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 2A High Voltage Ultrafast Diode, 25ns reverse recovery time, SMP"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D?SMP*"
			(at 0 0 0)
		)
	)
	(symbol "ESH2PC"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESH2PC"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMP_DO-220AA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/89016/esh2pb.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "150V 2A High Voltage Ultrafast Diode, 25ns reverse recovery time, SMP"
			(at 0 -7.62 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D?SMP*"
			(at 0 0 0)
		)
	)
	(symbol "ESH2PD"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ESH2PD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMP_DO-220AA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/89016/esh2pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 2A High Voltage Ultrafast Diode, 25ns reverse recovery time, SMP"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D?SMP*"
			(at 0 0 0)
		)
	)
	(symbol "HN2D02FU"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "HN2D02FU"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/HN2D02FUTW1T1-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Ultra high speed switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD06G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD06G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD06G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628f86ff8c0e09"
			(at 0 0 0)
		)
		(property "Description" "650V, 6A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD08G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD08G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD08G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628ff7d31a104b"
			(at 0 0 0)
		)
		(property "Description" "650V, 8A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD10G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD10G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD10G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628ff848ec1051"
			(at 0 0 0)
		)
		(property "Description" "650V, 10A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD12G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD12G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD12G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628f86ec3e0e06"
			(at 0 0 0)
		)
		(property "Description" "650V, 12A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD16G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD16G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD16G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628f8711b50e0c"
			(at 0 0 0)
		)
		(property "Description" "650V, 16A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IDDD20G65C6"
		(extends "IDDD04G65C6")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IDDD20G65C6"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IDDD20G65C6-DS-v02_00-EN.pdf?fileId=5546d462625a528f01628ff837cf104e"
			(at 0 0 0)
		)
		(property "Description" "650V, 20A, SiC Schottky Diode, CoolSiC, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "sic diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "LL4148"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LL4148"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85557/ll4148.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A standard switching diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "LL42"
		(extends "LL41")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LL42"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85672/ll42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "LL43"
		(extends "LL41")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LL43"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85672/ll42.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.2A Small Signal Schottky diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "LL4448"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LL4448"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85557/ll4148.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 0.15A standard switching diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0520"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0520"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0520LT"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0520LT"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBR0520LT1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "20V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0530"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0530"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0540"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0540"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0550"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0550"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0560"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0560"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0570"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0570"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "70V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR0580"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR0580"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.mccsemi.com/up_pdf/MBR0520~MBR0580(SOD123).pdf"
			(at 0 0 0)
		)
		(property "Description" "80V 0.5A Schottky Power Rectifier Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MBR1020VL"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR1020VL"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MBR1020VL-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A, 340 mV, Schottky Diode Rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "MBR340"
		(extends "1N5820")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR340"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBR340-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "MBR745"
		(extends "MBR735")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBR745"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-2_Vertical"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBR735-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "45V 7.5A Schottky Barrier Rectifier Diode, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MBRA340"
		(extends "B120-E3")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBRA340"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MBRA340T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "MCL4148"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MCL4148"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85566/mlc4148.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.2A Switching Diode, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "MCL4448"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MCL4448"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MicroMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85566/mlc4148.pdf"
			(at 0 0 0)
		)
		(property "Description" "75V 0.2A Switching Diode, MicroMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MicroMELF*"
			(at 0 0 0)
		)
	)
	(symbol "MM3Zxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MM3Zxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/mm3z2v4.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mW Zener Diode, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "MM5Zxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MM5Zxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/mm5z2v4.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mW Zener Diode, SOD-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?523*"
			(at 0 0 0)
		)
	)
	(symbol "MMBD4148TW"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMBD4148TW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30154.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMBD4448HADW"
		(extends "Rohm_UMP11N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMBD4448HADW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30153.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast Switching Diode Array 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMBD4448HCQW"
		(extends "Rohm_UMN1N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMBD4448HCQW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30153.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Quad Switching Diode Array Common Cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "MMBD4448HTW"
		(extends "BAS16TW")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMBD4448HTW"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/ds30153.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Fast switching diode array 3 independent"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMBZxx"
		(extends "2BZX84Cxx")
		(property "Reference" "D"
			(at 3.81 2.54 0)
		)
		(property "Value" "MMBZxx"
			(at 3.81 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBZ5V6ALT1-D.PDF"
			(at -2.54 0 90)
		)
		(property "Description" "Double Zener Diode, Common Anode, 225mW, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMSD4148"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMSD4148"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMSD4148T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100V 200mA Switching Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MMSD914"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MMSD914"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMSD914T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100V 0.2A Switching Diode, SOD-123"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123*"
			(at 0 0 0)
		)
	)
	(symbol "MRA4003T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MRA4003T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "300V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "MRA4004T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MRA4004T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "400V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "MRA4005T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MRA4005T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "600V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "MRA4006T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MRA4006T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "800V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "MRA4007T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MRA4007T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1000V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NRVA4003T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NRVA4003T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "300V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NRVA4004T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NRVA4004T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "400V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NRVA4005T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NRVA4005T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "600V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NRVA4006T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NRVA4006T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "800V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NRVA4007T3G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NRVA4007T3G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MRA4003T3-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1000V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "NSR0340HT1G"
		(extends "1N6263")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "NSR0340HT1G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NSR0340H-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "40V 0.25A Schottky Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG030V030EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG030V030EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG030V030EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 3A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG030V050EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG030V050EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG030V050EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 5A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG040V030EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG040V030EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG040V030EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 3A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG040V050EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG040V050EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG040V050EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 5A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045T050EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045T050EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045T050EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 5A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045T100EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045T100EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045T100EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 10A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045T150EIPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045T150EIPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045T150EIPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 15A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045T150EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045T150EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045T150EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 15A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045V050EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045V050EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045V050EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 5A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045V100EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045V100EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045V100EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 10A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG045V150EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG045V150EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG045V150EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 15A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG050T150EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG050T150EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG050T150EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V, 15A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG050V030EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG050V030EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG050V030EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V, 3A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG050V150EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG050V150EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG050V150EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V, 15A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG060V030EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG060V030EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG060V030EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 3A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG060V050EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG060V050EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG060V050EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 5A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG060V100EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG060V100EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG060V100EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 10A low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG10010ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG10010ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG10010ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 1A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG10020AELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG10020AELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG10020AELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 2A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG10020ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG10020ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG10020ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 2A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG100V060ELPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG100V060ELPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG100V060ELPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 6A low leakage current MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG100V080ELPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG100V080ELPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG100V080ELPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 8A low leakage current MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG100V100ELPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG100V100ELPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG100V100ELPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 10A low leakage current MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG1020EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG1020EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG1020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 2A ultra low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG1020EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG1020EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG1020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 2A ultra low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG1030EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG1030EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG1030EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 3A ultra low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG1030EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG1030EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG1030EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 3A ultra low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2005EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2005EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010AEH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010AEH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010AEH_PMEG2010AET.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010AEJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010AEJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010AEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010BER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010BER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010BER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2010ET"
		(extends "PMEG2010AET")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2010ET"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1A very low Vf MEGA Schottky barrier rectifier, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2015EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2015EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2015EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1.5A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2015EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2015EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2015EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 1.5A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2020EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2020EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 2A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG2020EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG2020EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG2020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 2A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3002EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3002EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3002EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 200mA low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3005EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3005EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3005EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3005EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010BER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010BER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010BER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010CEH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010CEH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010CEH_PMEG3010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010CEJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010CEJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010CEH_PMEG3010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3010ET"
		(extends "PMEG2010AET")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3010ET"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1A very low Vf MEGA Schottky barrier rectifier, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3015EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3015EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3015EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1.5A ultra low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3015EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3015EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3015EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 1.5A ultra low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3020BER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3020BER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3020BER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 2A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3020EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3020EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 2A ultra low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3020EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3020EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3020EH_EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 2A ultra low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG3020ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG3020ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG3020ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V, 2A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4002EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4002EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4002EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 200mA low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4005CEJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4005CEJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4005CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 500mA low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4005EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4005EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4005EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4005EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEGXX05EH_EJ_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 500mA very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010CEH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010CEH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010CEH_PMEG4010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010CEJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010CEJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010CEH_PMEG4010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010EH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010EH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4010ET"
		(extends "PMEG2010AET")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4010ET"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4010EH_EJ_ET.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 1A very low Vf MEGA Schottky barrier rectifier, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4020ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4020ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4020ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 2A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG4030ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG4030ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG4030ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 3A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG40T20ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG40T20ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG40T20ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 2A low Vf Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG40T30ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG40T30ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG40T30ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V, 3A low Vf Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG45T15EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG45T15EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG45T15EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 15A low Vf Trench MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG45U10EPD"
		(extends "PMEG45A10EPD")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG45U10EPD"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Nexperia_CFP15_SOT-1289"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG45U10EPD.pdf"
			(at 0 0 0)
		)
		(property "Description" "45V, 10A extremely low Vf MEGA Schottky barrier rectifier, SOT-1289"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP15*SOT?1289*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6002EJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6002EJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6002EJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 200mA very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6010CEH"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6010CEH"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6010CEH_PMEG6010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-123F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?123F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6010CEJ"
		(extends "PMEG2005EJ")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6010CEJ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323F"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6010CEH_PMEG6010CEJ.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 1A very low Vf MEGA Schottky barrier rectifier, SOD-323F"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323F*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6010ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6010ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6010ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 1A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6010ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6010ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6010ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 1A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6020AELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6020AELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6020AELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 2A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6020ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6020ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6020ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 2A low leakage current MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6020ER"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6020ER"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6020ER.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 2A low Vf MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6030EP"
		(extends "PMEG4050EP")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6030EP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-128"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6030EP.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 3A low Vf MEGA Schottky barrier rectifier, SOD-128"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?128*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG6045ETP"
		(extends "PMEG4050EP")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG6045ETP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-128"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG6045ETP.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 4.5A High-Temperature Schottky barrier rectifier, SOD-128"
			(at 0 0 0)
		)
		(property "ki_keywords" "forward voltage diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?128*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG60T10ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG60T10ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG60T10ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 1A low leakage current Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG60T20ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG60T20ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG60T20ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 2A low leakage current Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PMEG60T30ELR"
		(extends "PMEG40T10ER")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PMEG60T30ELR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_CFP3_SOD-123W"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMEG60T30ELR.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V, 3A low leakage current Trench MEGA Schottky barrier rectifier, SOD-123W"
			(at 0 0 0)
		)
		(property "ki_keywords" "ir diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nexperia*CFP3*SOD?123W*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS10VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS10VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS10VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "10V, 2000W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS12VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS12VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS12VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 1900W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS15VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS15VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS15VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 1900W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS18VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS18VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS18VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, 1800W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS20VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS20VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS20VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, 2000W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS22VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS22VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS22VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "22V, 1900W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS26VZ1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS26VZ1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS26VZ1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "26V, 1850W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS5V0Z1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS5V0Z1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS5V0Z1USKP"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS5V0Z1USKP"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USKP.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 2000W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "PTVS7V5Z1USK"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "PTVS7V5Z1USK"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS7V5Z1USK.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5V, 2200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TVS diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSN1608?2*"
			(at 0 0 0)
		)
	)
	(symbol "Panasonic_MA5J002E"
		(extends "Rohm_UMN1N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Panasonic_MA5J002E"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.semicon.panasonic.co.jp/ds4/MA5J002E_BED_discon.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Quad Ultra high Speed Switching Diode Array Com K"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "RF01VM2S"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "RF01VM2S"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/diode/fast_recovery/rf01vm2s.pdf"
			(at 0 0 0)
		)
		(property "Description" "250 V, 100 mA, Super Fast Recovery Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "S2JTR"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "S2JTR"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.smc-diodes.com/propdf/S2A-S2M%20N0562%20REV.A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 2A General Purpose Rectifier Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D?SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SB130"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB130"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds23022.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "SB140"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB140"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds23022.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "SB150"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB150"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds23022.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "SB160"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB160"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds23022.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "SB5H100"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB5H100"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88722/sb5h90.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 5A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "SB5H90"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SB5H90"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88722/sb5h90.pdf"
			(at 0 0 0)
		)
		(property "Description" "90V 5A Schottky Barrier Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "SD12_SOD323"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SD12_SOD323"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sd_c_datasheet.pdf.pdf"
			(at 0 0 0)
		)
		(property "Description" "12V, 450W Discrete Bidirectional TVS Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "SD15_SOD323"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SD15_SOD323"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sd_c_datasheet.pdf.pdf"
			(at 0 0 0)
		)
		(property "Description" "15V, 450W Discrete Bidirectional TVS Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "SD24_SOD323"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SD24_SOD323"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sd_c_datasheet.pdf.pdf"
			(at 0 0 0)
		)
		(property "Description" "24V, 450W Discrete Bidirectional TVS Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "SD36_SOD323"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SD36_SOD323"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sd_c_datasheet.pdf.pdf"
			(at 0 0 0)
		)
		(property "Description" "36V, 450W Discrete Bidirectional TVS Diode, SOD-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "transient voltage suppressor thyrector transil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SOD?323*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T6V8A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T6V8A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at -0.508 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Unidirectional TVS Diode, VRM = 5.8V (IRM = 500 μA at 25°C), VBR = 6.45 ... 7.14V, 'MDE' marking, SMC"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T6V8CA"
		(extends "1.5KExxCA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T6V8CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at 0 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Bidirectional TVS Diode, VRM = 5.8V (IRM = 500 μA at 25°C), VBR = 6.45 ... 7.14V, 'BDE' marking, SMC"
			(at 0.508 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM2000"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM2000"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4001"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4001"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4002"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4002"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4003"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4003"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4004"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4004"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4005"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4005"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4006"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4006"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM4007"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM4007"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM5059"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5059"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/sm5059.pdf"
			(at 0 -4.572 0)
		)
		(property "Description" "Standard Recovery SMD Rectifier Diodes, IFAV = 2A, IFSM = 50/55A (50/60Hz), trr = 1500ns, VRRM = 200V, DO-213AB (MELF)"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM513"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM513"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "130V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM516"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM516"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "1600V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM518"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM518"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A400/SMD1N400%23DIO.pdf"
			(at 0 0 0)
		)
		(property "Description" "1800V 1A General Purpose Rectifier Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T100A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T100A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 100Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T10A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T10A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 10Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T12A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T12A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 12Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T150A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T150A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 150Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T15A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T15A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 15Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T18A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T18A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 18Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T200A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T200A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 200Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T220A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T220A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 220Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T22A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T22A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 22Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T24A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T24A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 24Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T27A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T27A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 27Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T30A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T30A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 30Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T33A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T33A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 33Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T36A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T36A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 36Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T39A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T39A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 39Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T56A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T56A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 56Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T68A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T68A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 68Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T75A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T75A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 75Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SM6T7V5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM6T7V5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transil Transient Voltage Suppressor, 7.5Vrwm, DO-214AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ100A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ100A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 100.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ100CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ100CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 100.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ10A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ10A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ10CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ10CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ110A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ110A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 110.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ110CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ110CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 110.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ11A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ11A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 11.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ11CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ11CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 11.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ120A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ120A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 120.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ120CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ120CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 120.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ12A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ12A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 12.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ12CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ12CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 12.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ130A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ130A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 130.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ130CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ130CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 130.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ13A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ13A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 13.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ13CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ13CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 13.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ14A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ14A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 14.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ14CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ14CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 14.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ150A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ150A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 150.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ150CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ150CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 150.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ15A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ15A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 15.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ15CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ15CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 15.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ160A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ160A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 160.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ160CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ160CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 160.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ16A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ16A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 16.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ16CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ16CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 16.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ170A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ170A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 170.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ170CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ170CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 170.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ17A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ17A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 17.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ17CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ17CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 17.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ180A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ180A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 180.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ180CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ180CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 180.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ188A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ188A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 188.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ188CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ188CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 188.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ18A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ18A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ18CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ18CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ200A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ200A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 200.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ200CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ200CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 200.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ20A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ20A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 20.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ20CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ20CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 20.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ220A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ220A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 220.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ220CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ220CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 220.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ22A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ22A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 22.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ22CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ22CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 22.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ24A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ24A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 24.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ24CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ24CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 24.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ250A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ250A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 250.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ250CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ250CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 250.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ26A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ26A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 26.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ26CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ26CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 26.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ28A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ28A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 28.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ28CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ28CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 28.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ300A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ300A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transient Voltage Suppressor, 300.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ300CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ300CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 300.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ30A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ30A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 30.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ30CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ30CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 30.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ33A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ33A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 33.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ33CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ33CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 33.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ350A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ350A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transient Voltage Suppressor, 350.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ350CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ350CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 350.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ36A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ36A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 36.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ36CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ36CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 36.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ400A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ400A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transient Voltage Suppressor, 400.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ400CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ400CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 400.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ40A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ40A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 40.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ40CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ40CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 40.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ43A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ43A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 43.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ43CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ43CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 43.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ440A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ440A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "600W unidirectional Transient Voltage Suppressor, 440.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ440CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ440CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "600W bidirectional Transient Voltage Suppressor, 440.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ45A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ45A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 45.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ45CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ45CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 45.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ48A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ48A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 48.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ48CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ48CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 48.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ5.0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ5.0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 5.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ5.0CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ5.0CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 5.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ51A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ51A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 51.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ51CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ51CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 51.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ54A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ54A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 54.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ54CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ54CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 54.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ58A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ58A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 58.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ58CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ58CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 58.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ6.0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ6.0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 6.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ6.0CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ6.0CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 6.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ6.5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ6.5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 6.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ6.5CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ6.5CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 6.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ60A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ60A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 60.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ60CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ60CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 60.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ64A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ64A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 64.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ64CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ64CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 64.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ7.0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ7.0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 7.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ7.0CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ7.0CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 7.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ7.5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ7.5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 7.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ7.5CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ7.5CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 7.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ70A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ70A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 70.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ70CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ70CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 70.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ75A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ75A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 75.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ75CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ75CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 75.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ78A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ78A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 78.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ78CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ78CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 78.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ8.0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ8.0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 8.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ8.0CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ8.0CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 8.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ8.5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ8.5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 8.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ8.5CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ8.5CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 8.5Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ85A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ85A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 85.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ85CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ85CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 85.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ9.0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ9.0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 9.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ9.0CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ9.0CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 9.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ90A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ90A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at -1.27 0 0)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 90.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "unidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMAJ90CA"
		(extends "SD05_SOD323")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMAJ90CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 0)
		)
		(property "Description" "400W bidirectional Transient Voltage Suppressor, 90.0Vr, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SMF10A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF10A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 10Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF11A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF11A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 11Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF12A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF12A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 12Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF13A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF13A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 13Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF14A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF14A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 14Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF15A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF15A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 15Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF16A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF16A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 16Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF17A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF17A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 17Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF18A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF18A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 18Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF20A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF20A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 20Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF22A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF22A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 22Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF24A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF24A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 24Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF26A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF26A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 26Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF28A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF28A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 28Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF30A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF30A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 30Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF33A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF33A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 33Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF36A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF36A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 36Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF40A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF40A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 40Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF43A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF43A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 43Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF45A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF45A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 45Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF48A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF48A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 48Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF51A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF51A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 51Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF54A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF54A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 54Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF58A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF58A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 58Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF5V0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF5V0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 5Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF6V0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF6V0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 6Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF6V5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF6V5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 6.5Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF7V0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF7V0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 7Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF7V5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF7V5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 7.5Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF8V0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF8V0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 8Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF8V5A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF8V5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 8.5Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMF9V0A"
		(extends "SM6T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMF9V0A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?85881"
			(at -1.27 0 0)
		)
		(property "Description" "200W unidirectional Transil Transient Voltage Suppressor, 9Vrwm, SMF"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS voltage suppressor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMF*"
			(at 0 0 0)
		)
	)
	(symbol "SMZxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SMZxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/smz1.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000mW Zener Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SS110"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS110"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.smc-diodes.com/propdf/SS12-SS110%20N0229%20REV.C.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS1150"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS1150"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wontop.com/uploadfiles/56/sort_excel/pdf/ss1150.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS12"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS12"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88746/ss12.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS1200"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS1200"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wontop.com/uploadfiles/56/sort_excel/pdf/ss1150.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS13"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS13"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88746/ss12.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS14"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS14"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88746/ss12.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS15"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS15"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88746/ss12.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS16"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS16"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88746/ss12.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS18"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS18"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.smc-diodes.com/propdf/SS12-SS110%20N0229%20REV.C.pdf"
			(at 0 0 0)
		)
		(property "Description" "80V 1A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS210"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS210"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wontop.com/uploadfiles/56/sort_excel/pdf/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS2150"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS2150"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS22-THRU-SS2200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS22"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS22"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88748/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS2200"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS2200"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS22-THRU-SS2200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS23"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS23"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88748/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS24"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS24"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88748/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS25"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS25"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88748/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS26"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS26"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88748/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS28"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS28"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.wontop.com/uploadfiles/56/sort_excel/pdf/ss22.pdf"
			(at 0 0 0)
		)
		(property "Description" "80V 2A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS310"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS310"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS32-THRU-SS3200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS3150"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS3150"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS32-THRU-SS3200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "150V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS32"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS32"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88751/ss32.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS3200"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS3200"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS32-THRU-SS3200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS33"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS33"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88751/ss32.pdf"
			(at 0 0 0)
		)
		(property "Description" "30V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS34"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS34"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88751/ss32.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS35"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS35"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88751/ss32.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS36"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS36"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88751/ss32.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "SS38"
		(extends "SB120")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SS38"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.microdiode.com/uploadfiles//PDF/SS32-THRU-SS3200-SMA.pdf"
			(at 0 0 0)
		)
		(property "Description" "80V 3A Schottky Diode, SMA"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "STBR3008WY"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "STBR3008WY"
			(at 0 2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-247_Vertical"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stbr3008-y.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 30A, General Purpose Rectifier Diode, DO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO*247*"
			(at 0 0 0)
		)
	)
	(symbol "STBR3012WY"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "STBR3012WY"
			(at 0 2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-247_Vertical"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stbr3012-y.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 30A, General Purpose Rectifier Diode, DO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO*247*"
			(at 0 0 0)
		)
	)
	(symbol "STBR6008WY"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "STBR6008WY"
			(at 0 2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-247_Vertical"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stbr6008-y.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 60A, General Purpose Rectifier Diode, DO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO*247*"
			(at 0 0 0)
		)
	)
	(symbol "STBR6012WY"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 5.08 0)
		)
		(property "Value" "STBR6012WY"
			(at 0 2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-247_Vertical"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stbr6012-y.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V, 60A, General Purpose Rectifier Diode, DO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "AEC-Q101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO*247*"
			(at 0 0 0)
		)
	)
	(symbol "STTH212U"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "STTH212U"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stth212.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200V 2A High Voltage Ultrafast Diode, SMB"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D?SMB*"
			(at 0 0 0)
		)
	)
	(symbol "SZESD9B5.0ST5G"
		(extends "ESD9B5.0ST5G")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SZESD9B5.0ST5G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-923"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "ESD protection diode, 5.0Vrwm, SOD-923"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SOD?923*"
			(at 0 0 0)
		)
	)
	(symbol "Toshiba_HN1D01FU"
		(extends "Rohm_UMP11N")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Toshiba_HN1D01FU"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.toshiba.com/taec/components2/Datasheet_Sync/200901/DST_HN1D01FU-TDE_EN_1882.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Ultra High Speed Switching Diode Array 2 pair Com A"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "UF5400"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5400"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5401"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5401"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5402"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5402"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5403"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5403"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "300V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5404"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5404"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5405"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5405"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "500V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5406"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5406"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5407"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5407"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "UF5408"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "UF5408"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-201AD_P15.24mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88756/uf5400.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V 3A Soft Recovery Ultrafast Rectifier Diode, DO-201AD"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?201AD*"
			(at 0 0 0)
		)
	)
	(symbol "US1A"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "50V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1B"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1B"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "100V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1D"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1D"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "200V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1G"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1G"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "400V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1J"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1J"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "600V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1K"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1K"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "800V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US1M"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US1M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2AA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2AA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "50V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2BA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2BA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2DA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2DA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "200V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2FA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2FA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "300V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2GA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2GA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "400V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2JA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2JA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "600V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2KA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2KA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "800V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "US2MA"
		(extends "1N4001")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "US2MA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/US2AA-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1000V, 1.5A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Super Fast"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*SMA*"
			(at 0 0 0)
		)
	)
	(symbol "Z1SMAxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Z1SMAxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/z1sma1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000mW Zener Diode, SMA(DO-214AC)"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMA*"
			(at 0 0 0)
		)
	)
	(symbol "Z2SMBxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Z2SMBxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMB"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/z2smb1.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000mW Zener Diode, SMB(DO-214AA)"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMB*"
			(at 0 0 0)
		)
	)
	(symbol "Z3SMCxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "Z3SMCxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/z3smc1.pdf"
			(at 0 0 0)
		)
		(property "Description" "3000mW Zener Diode, SMC(DO-214AB)"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D?SMC*"
			(at 0 0 0)
		)
	)
	(symbol "ZMDxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZMDxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://diotec.com/tl_files/diotec/files/pdf/datasheets/zmd1"
			(at 0 0 0)
		)
		(property "Description" "1000mW Zener Diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "ZMMxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZMMxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/zmm1.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mW Zener Diode, MiniMELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MiniMELF*"
			(at 0 0 0)
		)
	)
	(symbol "ZMYxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZMYxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/85788/zmy3v9.pdf"
			(at 0 0 0)
		)
		(property "Description" "1300mW Zener Diode, MELF"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "ZPDxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZPDxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://diotec.com/tl_files/diotec/files/pdf/datasheets/zpd1"
			(at 0 0 0)
		)
		(property "Description" "500mW Zener Diode, DO-35"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?35*"
			(at 0 0 0)
		)
	)
	(symbol "ZYxxx"
		(extends "ZPYxx")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "ZYxxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/zy1"
			(at 0 0 0)
		)
		(property "Description" "2000mW Zener Diode, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "zener diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4934"
		(extends "1N4933")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4934"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88508/1n4933.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast Switching Plastic Rectifier, VRRM 100V, IF(AV) 1.0A, trr 200ns, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4935"
		(extends "1N4933")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4935"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88508/1n4933.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast Switching Plastic Rectifier, VRRM 200V, IF(AV) 1.0A, trr 200ns, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4936"
		(extends "1N4933")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4936"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88508/1n4933.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast Switching Plastic Rectifier, VRRM 400V, IF(AV) 1.0A, trr 200ns, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "1N4937"
		(extends "1N4933")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "1N4937"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88508/1n4933.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fast Switching Plastic Rectifier, VRRM 600V, IF(AV) 1.0A, trr 200ns, DO-41"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*DO?41*"
			(at 0 0 0)
		)
	)
	(symbol "MBRS340"
		(extends "MBR340")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "MBRS340"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/mbrs340t3-d.pdf"
			(at 0 -6.604 0)
		)
		(property "Description" "40V 3A Schottky Barrier Rectifier Diode, SMC (DO-214AB)"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "diode Schottky"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T36A"
		(extends "SM15T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T36A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at 0 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Unidirectional TVS Diode, VRM = 30.8V (IRM = 0.2 μA at 25°C), VBR = 34.2 ... 37.8V, 'MEV' marking, SMC"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T36CA"
		(extends "SM15T6V8CA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T36CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0.508 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at 0 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Bidirectional TVS Diode, VRM = 30.8V (IRM = 0.2 μA at 25°C), VBR = 34.2 ... 37.8V, 'BEV' marking, SMC"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T7V5A"
		(extends "SM15T6V8A")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T7V5A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at -0.508 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Unidirectional TVS Diode, VRM = 6.4V (IRM = 250 μA at 25°C), VBR = 7.13 ... 7.88V, 'MDG' marking, SMC"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM15T7V5CA"
		(extends "SM15T6V8CA")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM15T7V5CA"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sm15t36a.pdf"
			(at 0 -6.604 0)
		)
		(property "Description" "1500W (10/1000 μs) Bidirectional TVS Diode, VRM = 6.4V (IRM = 250 μA at 25°C), VBR = 7.13 ... 7.88V, 'BDG' marking, SMC"
			(at 0 -4.572 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
	(symbol "SM5060"
		(extends "SM5059")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5060"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/sm5059.pdf"
			(at 0 -4.572 0)
		)
		(property "Description" "Standard Recovery SMD Rectifier Diodes, IFAV = 2A, IFSM = 50/55A (50/60Hz), trr = 1500ns, VRRM = 400V, DO-213AB (MELF)"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM5061"
		(extends "SM5059")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5061"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/sm5059.pdf"
			(at 0 -4.572 0)
		)
		(property "Description" "Standard Recovery SMD Rectifier Diodes, IFAV = 2A, IFSM = 50/55A (50/60Hz), trr = 1500ns, VRRM = 600V, DO-213AB (MELF)"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM5062"
		(extends "SM5059")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5062"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/sm5059.pdf"
			(at 0 -4.572 0)
		)
		(property "Description" "Standard Recovery SMD Rectifier Diodes, IFAV = 2A, IFSM = 50/55A (50/60Hz), trr = 1500ns, VRRM = 800V, DO-213AB (MELF)"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM5063"
		(extends "SM5059")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5063"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:D_MELF"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/sm5059.pdf"
			(at 0 -4.572 0)
		)
		(property "Description" "Standard Recovery SMD Rectifier Diodes, IFAV = 2A, IFSM = 50/55A (50/60Hz), trr = 1500ns, VRRM = 1000V, DO-213AB (MELF)"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*MELF*"
			(at 0 0 0)
		)
	)
	(symbol "SM5908"
		(extends "1N5908")
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "SM5908"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Diode_SMD:ST_D_SMC"
			(at 0 -8.636 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/1n5908.pdf"
			(at -1.016 -4.572 0)
		)
		(property "Description" "1500W (10/1000 μs) Unidirectional TVS Diode, VRM = 5V (IRM = 300 μA at 25°C), VBR = 6V, 'MDC' marking, SMC"
			(at 0 -6.604 0)
		)
		(property "ki_keywords" "ESD protection transient voltage-suppressor transil thyrector transorb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*D*SMC*"
			(at 0 0 0)
		)
	)
)
