(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PLT5_450B"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LD"
			(at -1.27 4.445 0)
		)
		(property "Value" "PLT5_450B"
			(at -1.27 -2.54 0)
		)
		(property "Footprint" "OptoDevice:LaserDiode_TO56-3"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://look.ams-osram.com/m/711b74151583f43/original/PLT5-450B.pdf"
			(at 0.762 -5.08 0)
		)
		(property "Description" "100mW, Blue Laser Diode (450nm), TO-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto laserdiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LaserDiode*TO56*"
			(at 0 0 0)
		)
		(symbol "PLT5_450B_0_1")
		(symbol "PLT5_450B_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PLT5_488"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LD"
			(at 0 6.985 0)
		)
		(property "Value" "PLT5_488"
			(at 0 -5.715 0)
		)
		(property "Footprint" "OptoDevice:LaserDiode_TO56-3"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://look.ams-osram.com/m/451ee5087173918f/original/PLT5-488.pdf"
			(at 0.762 -5.08 0)
		)
		(property "Description" "60mW, Cyan Laser Diode (488nm), TO-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto laserdiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LaserDiode*TO56*"
			(at 0 0 0)
		)
		(symbol "PLT5_488_0_1")
		(symbol "PLT5_488_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPL_PL90"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LD"
			(at -1.27 4.445 0)
		)
		(property "Value" "SPL_PL90"
			(at -1.27 -2.54 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at -1.524 -4.572 0)
		)
		(property "Datasheet" "https://look.ams-osram.com/m/2e6f6e5edf55ddfe/original/SPL-PL90.pdf"
			(at 0.762 -5.08 0)
		)
		(property "Description" "Pulsed Laser Diode in Plastic Package 25W Peak Power"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto laserdiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*"
			(at 0 0 0)
		)
		(symbol "SPL_PL90_0_1")
		(symbol "SPL_PL90_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PL520"
		(extends "PLT5_450B")
		(property "Reference" "LD"
			(at -1.27 4.445 0)
		)
		(property "Value" "PL520"
			(at -1.27 -2.54 0)
		)
		(property "Footprint" "OptoDevice:LaserDiode_TO38ICut-3"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic7/00234693_0.pdf/PL%20520.pdf"
			(at 0.762 -5.08 0)
		)
		(property "Description" "Green Laser Diode (520nm), TO-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto laserdiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LaserDiode*TO38ICut*"
			(at 0 0 0)
		)
	)
	(symbol "PLT5_510"
		(extends "PLT5_450B")
		(property "Reference" "LD"
			(at -1.27 4.445 0)
		)
		(property "Value" "PLT5_510"
			(at -1.27 -2.54 0)
		)
		(property "Footprint" "OptoDevice:LaserDiode_TO56-3"
			(at 0 -4.445 0)
		)
		(property "Datasheet" "https://look.ams-osram.com/m/2562f8ca3a03a793/original/PLT5-510.pdf"
			(at 0.762 -5.08 0)
		)
		(property "Description" "10mW, Green Laser Diode (515nm), TO-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto laserdiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LaserDiode*TO56*"
			(at 0 0 0)
		)
	)
)
