(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XTR111AxDGQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "XTR111AxDGQ"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP2.2x3.1mm_Mask1.83x1.89mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/xtr111.pdf"
			(at 0 0 0)
		)
		(property "Description" "0-20mA/4-20mA Current Loop Transmitter, Precision Voltage-To-Current, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "0-20mA 4-20mA Current Loop Transmitter Voltage To Current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XTR111AxDGQ_0_1")
		(symbol "XTR111AxDGQ_1_1"
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "REGF")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "REGS")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VSP")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OD")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{EF}")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IS")
				(number "2")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VG")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XTR115U"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "XTR115U"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/xtr115.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-20mA Current Loop Transmitter, VREF 2.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-20mA Current Loop Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "XTR115U_0_1")
		(symbol "XTR115U_1_1"
			(pin output line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VREG")
				(number "8")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IRET")
				(number "3")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "E")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XTR116U"
		(extends "XTR115U")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "XTR116U"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/xtr115.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-20mA Current Loop Transmitter, VREF 4.096V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-20mA Current Loop Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
