(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BFCN-1445"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1445"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1445+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1420-1470MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
		(symbol "BFCN-1445_0_1")
		(symbol "BFCN-1445_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BFCN-152W-75"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-152W-75"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-7"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1445+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "950-1970MHz 75 Ohm Passive Band Pass Filter, FV1206-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?7*"
			(at 0 0 0)
		)
		(symbol "BFCN-152W-75_0_1")
		(symbol "BFCN-152W-75_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BFCN-1560"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1560"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1560+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1500-1620MHz 50 Ohm Passive Band Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
		(symbol "BFCN-1560_0_1")
		(symbol "BFCN-1560_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BFCN-1860"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1860"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1860+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1580-2200MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
		(symbol "BFCN-1860_0_1")
		(symbol "BFCN-1860_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BFCN-1900"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1900"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1900+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1893-1920MHz 50 Ohm Passive Band Pass Filter, FV1206-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?5*"
			(at 0 0 0)
		)
		(symbol "BFCN-1900_0_1")
		(symbol "BFCN-1900_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BFCN-5100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-5100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-6"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-5100+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3100-7100MHz 50 Ohm Passive Band Pass Filter, FV1206-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?6*"
			(at 0 0 0)
		)
		(symbol "BFCN-5100_0_1")
		(symbol "BFCN-5100_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPF-A355"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "BPF-A355"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HQ1157"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BPF-A355+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Bandpass Filter, 310 to 400 MHz, 50 Ohm, Mini-Circuits HQ1157"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bandpass Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HQ1157*"
			(at 0 0 0)
		)
		(symbol "BPF-A355_0_1")
		(symbol "BPF-A355_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HFCN-1322"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1322"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1322+.pdf"
			(at 0 0 0)
		)
		(property "Description" "13300MHz 50 Ohm Passive High Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
		(symbol "HFCN-1322_0_1")
		(symbol "HFCN-1322_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HFCN-440"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-440"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-440+.pdf"
			(at 0 0 0)
		)
		(property "Description" "440MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
		(symbol "HFCN-440_0_1")
		(symbol "HFCN-440_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HFCN-672"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-672"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-672+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6275MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
		(symbol "HFCN-672_0_1")
		(symbol "HFCN-672_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFCN-113"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-113"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-113+.pdf"
			(at 0 0 0)
		)
		(property "Description" "11000MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
		(symbol "LFCN-113_0_1")
		(symbol "LFCN-113_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFCN-80"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-80"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 0)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
		(symbol "LFCN-80_0_1")
		(symbol "LFCN-80_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPF-B0R3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LPF-B0R3"
			(at 0 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HZ1198_LandPatternPL-247"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LPF-B0R3+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Pass Filter, DC to 0.3 MHz, 50 Ohm, Mini-Circuits HZ1198"
			(at 0 0 0)
		)
		(property "ki_keywords" "low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HZ1198*"
			(at 0 0 0)
		)
		(symbol "LPF-B0R3_0_1")
		(symbol "LPF-B0R3_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RBP-280"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "RBP-280"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_GP731_LandPatternPL-176"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/RBP-280+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Bandpass Filter, 260 to 310 MHz, 50 Ohm, Mini-Circuits GP731"
			(at 0 0 0)
		)
		(property "ki_keywords" "bandpass filter rf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*GP731*"
			(at 0 0 0)
		)
		(symbol "RBP-280_0_1")
		(symbol "RBP-280_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RBPF-246"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "RBPF-246"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CK605_LandPatternPL-012"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/RBPF-246+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Bandpass Filter, 236 to 265 MHz, 50 Ohm, Mini-Circuits CK605"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bandpass Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CK605*"
			(at 0 0 0)
		)
		(symbol "RBPF-246_0_1")
		(symbol "RBPF-246_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RLP-30"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "RLP-30"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_GP1212_LandPatternPL-176"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/RLP-30+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Low Pass Filter, DC to 30 MHz, 50 Ohm, Mini-Circuits GP1212"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Pass Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*GP1212*"
			(at 0 0 0)
		)
		(symbol "RLP-30_0_1")
		(symbol "RLP-30_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SCHF-31"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SCHF-31"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_YY161_LandPatternPL-049"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SCHF-31+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "High Pass Filter, 31 to 1500 MHz, 50 Ohm, Mini-Circuits YY161"
			(at 0 0 0)
		)
		(property "ki_keywords" "highpass filter rf"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*YY161*"
			(at 0 0 0)
		)
		(symbol "SCHF-31_0_1")
		(symbol "SCHF-31_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SXBP-140"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SXBP-140"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HF1139_LandPatternPL-230"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SXBP-140+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Bandpass Filter, 130 to 150 MHz, 50 Ohm, Mini-Circuits HF1139"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits Band-Pass Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HF1139*"
			(at 0 0 0)
		)
		(symbol "SXBP-140_0_1")
		(symbol "SXBP-140_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TA0232A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at -5.08 10.16 0)
		)
		(property "Value" "TA0232A"
			(at -1.27 7.62 0)
		)
		(property "Footprint" "Filter:Filter_SAW-8_3.8x3.8mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.golledge.com/media/1831/ma05497.pdf"
			(at -5.08 8.89 0)
		)
		(property "Description" "Bandpass Filter, 1090MHz, SAW filter 8-pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW Filter 1090 bandpass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*SAW*3.8x3.8mm*"
			(at 0 0 0)
		)
		(symbol "TA0232A_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "IN_1")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "IN_2")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "OUT_1")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "OUT_2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TA0970B"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at -5.08 10.16 0)
		)
		(property "Value" "TA0970B"
			(at -1.27 7.62 0)
		)
		(property "Footprint" "Filter:Filter_SAW-6_3.8x3.8mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.golledge.com/media/3785/mp08167.pdf"
			(at -5.08 8.89 0)
		)
		(property "Description" "Bandpass Filter, 1090MHz, SAW filter 6-pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW Filter 1090 bandpass MP08167"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*SAW*3.8x3.8mm*"
			(at 0 0 0)
		)
		(symbol "TA0970B_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B3715"
		(extends "TA0970B")
		(property "Reference" "X"
			(at 5.08 7.62 0)
		)
		(property "Value" "B3715"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Filter:Filter_SAW_Epcos_DCC6C_3x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.mouser.de/datasheet/2/842/epcos16633_1-2300371.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bandpass Filter, 869MHz, SAW filter 6-pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW Filter 869 bandpass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*SAW*DCC6C*3x3mm*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1525"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1525"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1525+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1480-1570MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1575"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1575"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1575+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1530-1620MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1690"
		(extends "BFCN-1560")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1690"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1690+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1570-1810MHz 50 Ohm Passive Band Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1840"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1840"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1840+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1750-1930MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1855"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1855"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1855+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1790-1920MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-1945"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-1945"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-1945+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1850-2040MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2275"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2275"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2275+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2170-2380MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2360"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2360"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2360+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2250-2470MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2435"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2435"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2435+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2340-2530MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2450"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2450"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2450+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2400-2550MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2500"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2500+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2100-2900MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2555"
		(extends "BFCN-1560")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2555"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2555+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2500-2610MHz 50 Ohm Passive Band Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2700"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2700+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2600-2800MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2840"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2840"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2840+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2750-2930MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2850"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2850"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2850+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2750-2950MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2900"
		(extends "BFCN-1560")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2900"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2900+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2700-3100MHz 50 Ohm Passive Band Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2910"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2910"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2910+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2850-2970MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-2975"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-2975"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-2975+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2570-3440MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3010"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3010"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3010+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2920-3100MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3085"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3085"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3085+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2800-3400MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3085A"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3085A"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3085A+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2800-3400MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3115"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3115"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3115+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "2720-3570MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3600"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3600"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3600+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3300-3900MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-3700"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-3700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-3700+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3000-4600MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-4100"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-4100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-4100+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3700-4500MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-4440"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-4440"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-4440+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "4200-4700MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-4800"
		(extends "BFCN-1445")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-4800"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-4800+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "4400-5200MHz 50 Ohm Passive Band Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-5200"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-5200"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-5200+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "4250-6300MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-5540"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-5540"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-5540+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "4620-6640MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-5750"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-5750"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-5750+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5650-5850MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7200"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7200"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7200+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7100-7300MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7331"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7331"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7331+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "6850-7850MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7350"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7350"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7350+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7150-7550MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7500"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7500+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7450-7650MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7700"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7700+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7500-7900MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-7900"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-7900"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-7900+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7800-8100MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-8000"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-8000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-8000+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "7900-8100MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-8350"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-8350"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-8350+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8250-8450MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-8450"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-8450"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-8450+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8350-8550MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "BFCN-8650"
		(extends "BFCN-1860")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "BFCN-8650"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/BFCN-8650+.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8550-8750MHz 50 Ohm Passive Band Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits band pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1000"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1080"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1080"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1080+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1080MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1100"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1100+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1100MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1150"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1150"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1150+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1150MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1200"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1200"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1200+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1180MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1200D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1200D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1200D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1180MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1300"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1300"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1300+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1300MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1300D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1300D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1300D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1300MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1320"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1320"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1320+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1320MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1320D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1320D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1320D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1320MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1500"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1550MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1500D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1550MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1600"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1600"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1600+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1600MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1600D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1600D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1600D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1600MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1760"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1760"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1760+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1760MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1810"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1810"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1810+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1810MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1810D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1810D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1810D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1810MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1910"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1910"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1910+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1910MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-1910D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-1910D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-1910D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1910MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2000"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2000.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2100"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2100+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2100MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2100D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2100D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2100D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2100MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2275"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2275"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2275+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2275MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2700"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2700+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2500MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2700A"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2700A"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2700A+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2700MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-2700AD"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-2700AD"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-2700AD+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2700MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3100"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3100+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3100MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3100D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3100D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3100D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3100MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3500"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3500MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3500D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3500MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3800"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3800"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3800+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3800MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-3800D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-3800D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-3800D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3800MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-4400"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-4400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-4400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4400MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-4400D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-4400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-4400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4400MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-4600"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-4600"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-4600+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4600MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-5050"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-5050"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-5050+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5050MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-5500"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-5500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-5500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5500MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-5500D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-5500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-5500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5500MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-6010"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-6010"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-6010+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6010MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-650"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-650"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-650+.pdf"
			(at 0 0 0)
		)
		(property "Description" "650MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-650D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-650D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-650D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "650MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-7150"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-7150"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-7150+.pdf"
			(at 0 0 0)
		)
		(property "Description" "7150MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-740"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-740"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-740+.pdf"
			(at 0 0 0)
		)
		(property "Description" "740MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-740D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-740D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-740D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "740MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-7971"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-7971"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-7971+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8000MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-8400"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-8400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-8400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8400MHz 50 Ohm Passive High Pass Filter, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-8400D"
		(extends "HFCN-672")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-8400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-1"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-8400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8400MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?1*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-880"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-880"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-880+.pdf"
			(at 0 0 0)
		)
		(property "Description" "880MHz 50 Ohm Passive High Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-880D"
		(extends "HFCN-440")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-880D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-880D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "880MHz 50 Ohm Passive High Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "HFCN-9700"
		(extends "HFCN-1322")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "HFCN-9700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/HFCN-9700+.pdf"
			(at 0 0 0)
		)
		(property "Description" "9070MHz 50 Ohm Passive High Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits high pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1000"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1000D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1000D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1000D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1000MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-105"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-105"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-105+.pdf"
			(at 0 0 0)
		)
		(property "Description" "105MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-120"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-120"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-120+.pdf"
			(at 0 0 0)
		)
		(property "Description" "120MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1200"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1200"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1200+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1200D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1200D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1200D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1200MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-123"
		(extends "LFCN-113")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-123"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-123+.pdf"
			(at 0 0 0)
		)
		(property "Description" "12000MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1282"
		(extends "LFCN-113")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1282"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1282+.pdf"
			(at 0 0 0)
		)
		(property "Description" "12800MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1325"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1325"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1325+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1325MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1450"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1450"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1450+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1450MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1500"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1500D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1500MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1525"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1525"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1525+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1525MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1525D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1525D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1525D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1525MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1575"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1575"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1575+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1575MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1575D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1575D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1575D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1575MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-160"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-160"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-160+.pdf"
			(at 0 0 0)
		)
		(property "Description" "160MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1700"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1700+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1700MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1700D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1700D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1700D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1700MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-180"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-180"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-180+.pdf"
			(at 0 0 0)
		)
		(property "Description" "180MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1800"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1800"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1800+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1800MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-1800D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-1800D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-1800D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1800MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-190"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-190"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-190+.pdf"
			(at 0 0 0)
		)
		(property "Description" "190MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2000"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2000D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2000D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2000D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2000MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-225"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-225"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-225+.pdf"
			(at 0 0 0)
		)
		(property "Description" "225MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2250"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2250"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2250+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2200MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2250D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2250D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2250D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2250MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-225D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-225D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-225D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "225MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2290"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2290"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2290+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2290MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2500"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2500MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2500D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2500MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2600"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2600"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2600+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2600MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2600D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2600D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2600D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2600MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2750"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2750"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2750+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2750MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2750D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2750D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2750D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2750MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2850"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2850"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2850+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2800MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-2850D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-2850D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-2850D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2800MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3000"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3000MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3000D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3000D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3000D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3000MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-320"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-320"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-320+.pdf"
			(at 0 0 0)
		)
		(property "Description" "320MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-320D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-320D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-320D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "320MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3800"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3800"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3800+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3900MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-3800D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-3800D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-3800D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "3900MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-4400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-4400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-4400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-4400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-4400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-4400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-490"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-490"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-490+.pdf"
			(at 0 0 0)
		)
		(property "Description" "490MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-490D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-490D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-490D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "490MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5000"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5000MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5000D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5000D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5000D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5000MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-530"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-530"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-530+.pdf"
			(at 0 0 0)
		)
		(property "Description" "530MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-530D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-530D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-530D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "530MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5500"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5500"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5500+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5500MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5500D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5500D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5500D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5500MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-575"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-575"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-575+.pdf"
			(at 0 0 0)
		)
		(property "Description" "575MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-575D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-575D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-575D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "575MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5850"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5850"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5850+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5850MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-5850D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-5850D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-5850D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "5850MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6000"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6000"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6000+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6000MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6000D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6000D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6000D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6000MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-630"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-630"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-630+.pdf"
			(at 0 0 0)
		)
		(property "Description" "630MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-630D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-630D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-630D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "630MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6400"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6400MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6400D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6400D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6400D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6400MHz 50 Ohm Passive Low Pass Filter, DC capable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6700"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6700"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6700+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6700MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-6700D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-6700D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-6700D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "6700MHz 50 Ohm Passive Low Pass Filter, DC cabable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-7200"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-7200"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-7200+.pdf"
			(at 0 0 0)
		)
		(property "Description" "7200MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-7200D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-7200D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-7200D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "7200MHz 50 Ohm Passive Low Pass Filter, DC cabable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-722"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-722"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-722+.pdf"
			(at 0 0 0)
		)
		(property "Description" "7200MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-800"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-800"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-800+.pdf"
			(at 0 0 0)
		)
		(property "Description" "800MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-800D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-800D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-800D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "800MHz 50 Ohm Passive Low Pass Filter, DC cabable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-8400"
		(extends "LFCN-113")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-8400"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-8400+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8400MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-8440"
		(extends "LFCN-113")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-8440"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-8440+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8440MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-900"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-900"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-900+.pdf"
			(at 0 0 0)
		)
		(property "Description" "850MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-900D"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-900D"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-900D+.pdf"
			(at 0 0 0)
		)
		(property "Description" "850MHz 50 Ohm Passive Low Pass Filter, DC cabable, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-9170"
		(extends "LFCN-113")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-9170"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206-4"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-9170+.pdf"
			(at 0 0 0)
		)
		(property "Description" "9170MHz 50 Ohm Passive Low Pass Filter, FV1206-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206?4*"
			(at 0 0 0)
		)
	)
	(symbol "LFCN-95"
		(extends "LFCN-80")
		(property "Reference" "FL"
			(at 0 10.795 0)
		)
		(property "Value" "LFCN-95"
			(at 0 8.89 0)
		)
		(property "Footprint" "Filter:Filter_Mini-Circuits_FV1206"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-95+.pdf"
			(at 0 0 0)
		)
		(property "Description" "95MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits low pass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Mini?Circuits*FV1206*"
			(at 0 0 0)
		)
	)
	(symbol "STA0232A"
		(extends "TA0232A")
		(property "Reference" "X"
			(at -5.08 10.16 0)
		)
		(property "Value" "STA0232A"
			(at -1.27 7.62 0)
		)
		(property "Footprint" "Filter:Filter_SAW-8_3.8x3.8mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.golledge.com/media/1831/ma05497.pdf"
			(at -5.08 8.89 0)
		)
		(property "Description" "Bandpass Filter, 1090MHz, SAW filter 8-pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW Filter 1090 bandpass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*SAW*3.8x3.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STA1090EC"
		(extends "TA0970B")
		(property "Reference" "X"
			(at -5.08 10.16 0)
		)
		(property "Value" "STA1090EC"
			(at -1.27 7.62 0)
		)
		(property "Footprint" "Filter:Filter_SAW-6_3.8x3.8mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.golledge.com/media/3785/mp08167.pdf"
			(at -5.08 8.89 0)
		)
		(property "Description" "Bandpass Filter, 1090MHz, SAW filter 6-pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW Filter 1090 bandpass"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*SAW*3.8x3.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SXBP-100"
		(extends "SXBP-140")
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SXBP-100"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HF1139_LandPatternPL-230"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SXBP-100+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Bandpass Filter, 87 to 117 MHz, 50 Ohm, Mini-Circuits HF1139"
			(at 0 0 0)
		)
		(property "ki_keywords" "bandpass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HF1139*"
			(at 0 0 0)
		)
	)
	(symbol "SXBP-202"
		(extends "SXBP-140")
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SXBP-202"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HF1139_LandPatternPL-230"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SXBP-202+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Bandpass Filter, 198 to 206 MHz, 50 Ohm, Mini-Circuits HF1139"
			(at 0 0 0)
		)
		(property "ki_keywords" "bandpass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HF1139*"
			(at 0 0 0)
		)
	)
	(symbol "SXBP-27R5"
		(extends "SXBP-140")
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "SXBP-27R5"
			(at 6.35 7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_HF1139_LandPatternPL-230"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/SXBP-27R5+.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Bandpass Filter, 24 to 31 MHz, 50 Ohm, Mini-Circuits HF1139"
			(at 0 0 0)
		)
		(property "ki_keywords" "bandpass filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*HF1139*"
			(at 0 0 0)
		)
	)
)
