(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LM134H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM134H"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-46-3"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, TO-46"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?46*"
			(at 0 0 0)
		)
		(symbol "LM134H_0_1")
		(symbol "LM134H_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM334M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM334M"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM334M_0_1")
		(symbol "LM334M_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM334SM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM334SM"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, SO-8 Alternate"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9m*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM334SM_0_1")
		(symbol "LM334SM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM334Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM334Z"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
		(symbol "LM334Z_0_1")
		(symbol "LM334Z_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3092xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LT3092xDD"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3092fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA 2-Terminal Programmable Current Source, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current source"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3092xDD_0_1")
		(symbol "LT3092xDD_1_1"
			(pin no_connect line
				(at -1.27 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -1.27 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3092xST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LT3092xST"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3092fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA 2-Terminal Programmable Current Source, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "current source"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "LT3092xST_0_1")
		(symbol "LT3092xST_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3092xTS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LT3092xTS8"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3092fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA 2-Terminal Programmable Current Source, TSOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "current source"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT3092xTS8_0_1")
		(symbol "LT3092xTS8_1_1"
			(pin no_connect line
				(at -1.27 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -1.27 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PSSI2021SAY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.255 0)
		)
		(property "Value" "PSSI2021SAY"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PSSI2021SAY.pdf"
			(at 7.62 0 0)
		)
		(property "Description" "Constant current source, Io 15µA to 50mA, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "iref adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "PSSI2021SAY_0_1"
			(pin power_out line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "PSSI2021SAY_1_1"
			(pin no_connect line
				(at -2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "REF200AU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.175 4.445 0)
		)
		(property "Value" "REF200AU"
			(at -3.175 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -3.175 0.635 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/ref200.pdf"
			(at 7.62 0 0)
		)
		(property "Description" "2x100μA Current Sources/Sinks with Current Mirror, SO-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "Current Source/Sink 100μA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "REF200AU_0_1"
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "S")
				(number "6")
			)
		)
		(symbol "REF200AU_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "REF200AU_2_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "REF200AU_3_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM234Z-3"
		(extends "LM334Z")
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM234Z-3"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM234Z-6"
		(extends "LM334Z")
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM234Z-6"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
	)
	(symbol "LM334Z-LFT1"
		(extends "LM334Z")
		(property "Reference" "U"
			(at 0.635 6.35 0)
		)
		(property "Value" "LM334Z-LFT1"
			(at 0.635 4.445 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0.635 -4.445 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm134.pdf"
			(at 0 0 0)
		)
		(property "Description" "1μA to 10mA 3-Terminal Adjustable Current Source, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Current Source 10mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*Inline*"
			(at 0 0 0)
		)
	)
)
