(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "HV100K5-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HV100K5-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/hv100%20b060513.pdf"
			(at 8.89 1.27 0)
		)
		(property "Description" "Hot-Swap Current Limiter Controller, SOT223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hot-Swap Current Limiter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "HV100K5-G_0_1")
		(symbol "HV100K5-G_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VPP")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VNN")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "GATE")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV101K5-G"
		(extends "HV100K5-G")
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "HV101K5-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.supertex.com/pdf/datasheets/HV100.pdf"
			(at 8.89 1.27 0)
		)
		(property "Description" "Hot-Swap Current Limiter Controller, SOT223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Hot-Swap Current Limiter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
)
