(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADP3336ARMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "ADP3336ARMZ"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 20.32 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP3336.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Accuracy Ultralow IQ, 500mA anyCAP Adjustable Low Dropout Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADP3336ARMZ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7118ACPZN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "ADP7118ACPZN"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, Adjustable, LFCSP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADP7118ACPZN_0_1")
		(symbol "ADP7118ACPZN_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE/ADJ")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7142ARDZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142ARDZ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, Adjustable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADP7142ARDZ_0_1")
		(symbol "ADP7142ARDZ_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE/ADJ")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7142AUJZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142AUJZ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, Adjustable, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ADP7142AUJZ_0_1")
		(symbol "ADP7142AUJZ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE/ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7182AUJZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "ADP7182AUJZ"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7182.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Negative, Adjustable, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ADP7182AUJZ_0_1")
		(symbol "ADP7182AUJZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7182AUJZ-1.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "ADP7182AUJZ-1.8"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7182.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Negative, -1.8V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "ADP7182AUJZ-1.8_0_1")
		(symbol "ADP7182AUJZ-1.8_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMS1117CD"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, adjustable output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
		(symbol "AMS1117CD_0_1")
		(symbol "AMS1117CD_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMS1117CD-1.5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.5V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
		(symbol "AMS1117CD-1.5_0_1")
		(symbol "AMS1117CD-1.5_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMS1117CS"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, adjustable output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AMS1117CS_0_1")
		(symbol "AMS1117CS_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMS1117CS-1.5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.5V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AMS1117CS-1.5_0_1")
		(symbol "AMS1117CS-1.5_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP1117-15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-15"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "AP1117-15_0_1")
		(symbol "AP1117-15_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP1117-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, adjustable output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "AP1117-ADJ_0_1")
		(symbol "AP1117-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP131-15"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-15"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 1.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP131-15_0_1")
		(symbol "AP131-15_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2127N3-1.2"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N3-1.2"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.2V fixed positive output, SOT-23-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AP2127N3-1.2_0_1")
		(symbol "AP2127N3-1.2_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204K-1.5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-1.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 1.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "AP2204K-1.5_0_1")
		(symbol "AP2204K-1.5_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204K-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout adjustable linear regulator, wide input voltage range, SOT-23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "AP2204K-ADJ_0_1")
		(symbol "AP2204K-ADJ_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204MP-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204MP-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:Diodes_PSOP-8"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout adjustable linear regulator, wide input voltage range, PSOP-8 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*PSOP*"
			(at 0 0 0)
		)
		(symbol "AP2204MP-ADJ_0_1")
		(symbol "AP2204MP-ADJ_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204R-1.5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 1.5V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "AP2204R-1.5_0_1")
		(symbol "AP2204R-1.5_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204RA-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204RA-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.3V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "AP2204RA-3.3_0_1")
		(symbol "AP2204RA-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2204RB-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204RB-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.3V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "AP2204RB-3.3_0_1")
		(symbol "AP2204RB-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP22615AWU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -8.89 0)
		)
		(property "Value" "AP22615AWU"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/AP22815_615.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Current limited power switch, single channel, 3.0V to 5.5V, 3A, SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "ki_keywords" "Limit USB active-high load-switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP22615AWU_0_1")
		(symbol "AP22615AWU_1_0"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISET")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP22615BWU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -8.89 0)
		)
		(property "Value" "AP22615BWU"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.diodes.com/datasheet/download/AP22815_615.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Current limited power switch, single channel, 3.0V to 5.5V, 3A, SOT-23-6"
			(at 0 -21.59 0)
		)
		(property "ki_keywords" "Limit USB active-low load-switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP22615BWU_0_1")
		(symbol "AP22615BWU_1_0"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{EN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISET")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP7370-12FDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-12FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Low-Dropout Linear Regulator, 1.2V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AP7370-12FDC_0_1")
		(symbol "AP7370-12FDC_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP7381-28SA-7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7381-28SA-7"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7381.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.8V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "Diodes ldo nrnd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP7381-28SA-7_0_1")
		(symbol "AP7381-28SA-7_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865N-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-12-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "APE8865N-12-HF-3_0_1")
		(symbol "APE8865N-12-HF-3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865NL-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-12-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "APE8865NL-12-HF-3_0_1")
		(symbol "APE8865NL-12-HF-3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865NR-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-12-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "APE8865NR-12-HF-3_0_1")
		(symbol "APE8865NR-12-HF-3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865U4-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-12-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "APE8865U4-12-HF-3_0_1")
		(symbol "APE8865U4-12-HF-3_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865U5-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-12-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "APE8865U5-12-HF-3_0_1")
		(symbol "APE8865U5-12-HF-3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APE8865Y5-12-HF-3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-12-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "APE8865Y5-12-HF-3_0_1")
		(symbol "APE8865Y5-12-HF-3_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZ1084-1.2"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-1.2"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.2V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
		(symbol "AZ1084-1.2_0_1")
		(symbol "AZ1084-1.2_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZ1117-1.2"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-1.2"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 1.2V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
		(symbol "AZ1117-1.2_0_1")
		(symbol "AZ1117-1.2_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZ1117-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
		(symbol "AZ1117-ADJ_0_1")
		(symbol "AZ1117-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD00FC0WEFJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD00FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at -10.16 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, variable LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator variable positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BD00FC0WEFJ_0_1")
		(symbol "BD00FC0WEFJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -3.81 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -1.27 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD00FC0WFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD00FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 13.97 10.16 0)
		)
		(property "Description" "1A, variable LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator variable positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "BD00FC0WFP_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD15GA5WEFJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD15GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 1.5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BD15GA5WEFJ_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Vo_s")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD30FC0WEFJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD30FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 3.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BD30FC0WEFJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -3.81 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -1.27 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD30FC0WFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD30FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 3.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "BD30FC0WFP_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD33FC0FP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD33FC0FP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 3.3V LDO regulator with OVP & TSP, without enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "BD33FC0FP_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT75xx-1-SOT89"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 -3.81 0)
		)
		(property "Value" "HT75xx-1-SOT89"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.holtek.com/documents/10179/116711/HT75xx-1v250.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "100mA Low Dropout Voltage Regulator, Fixed Output, SOT89"
			(at 0 0 0)
		)
		(property "ki_keywords" "100mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "HT75xx-1-SOT89_0_1")
		(symbol "HT75xx-1-SOT89_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICL7663"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "ICL7663"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/ICL7663.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "50mA 5V/Programmable Voltage Regulator, DIP-8/SO-8/TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 50mA 5V fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?99*"
			(at 0 0 0)
		)
		(symbol "ICL7663_0_1")
		(symbol "ICL7663_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT1")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICL7664"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -8.255 0)
		)
		(property "Value" "ICL7664"
			(at 0 -8.255 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.27 0)
		)
		(property "Datasheet" "http://pe2bz.philpem.me.uk/pdf%20on%20typenumber/I-L/ICL7664.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "50mA Dual Mode -5V/Programmable Negative Voltage Regulator, DIP-8/SO-8/TO-99"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 50mA -5V fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO?99*"
			(at 0 0 0)
		)
		(symbol "ICL7664_0_1")
		(symbol "ICL7664_1_1"
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "SHDN")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT1")
				(number "7")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT2")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX25401TBV"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX25401TBV"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IFX25401-DS-v01_02-en.pdf?fileId=db3a304320d39d590120f62a690569f7"
			(at 0 0 0)
		)
		(property "Description" "Adjustable LDO Linear Voltage Regulator (TO-263-5)"
			(at 0 0 0)
		)
		(property "ki_keywords" "adjustable LDO positive voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "IFX25401TBV_0_1")
		(symbol "IFX25401TBV_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "I")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "VA")
				(number "4")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX25401TBV50"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX25401TBV50"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IFX25401-DS-v01_02-en.pdf?fileId=db3a304320d39d590120f62a690569f7"
			(at 0 0 0)
		)
		(property "Description" "Fixed 5V LDO Linear Voltage Regulator (TO-263-5)"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed ldo positive voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "IFX25401TBV50_0_1")
		(symbol "IFX25401TBV50_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "I")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX25401TEV"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX25401TEV"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IFX25401-DS-v01_02-en.pdf?fileId=db3a304320d39d590120f62a690569f7"
			(at 0 0 0)
		)
		(property "Description" "Adjustable LDO Linear Voltage Regulator (TO-252-4)"
			(at 0 0 0)
		)
		(property "ki_keywords" "adjustable LDO positive voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "IFX25401TEV_0_1")
		(symbol "IFX25401TEV_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "I")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "VA")
				(number "4")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX25401TEV50"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX25401TEV50"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IFX25401-DS-v01_02-en.pdf?fileId=db3a304320d39d590120f62a690569f7"
			(at 0 0 0)
		)
		(property "Description" "Fixed 5V LDO Linear Voltage Regulator (TO-252-4)"
			(at 0 0 0)
		)
		(property "ki_keywords" "fixed ldo positive voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "IFX25401TEV50_0_1")
		(symbol "IFX25401TEV50_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "I")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX27001TFV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, adjustable output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "IFX27001TFV_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "I")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IFX27001TFV15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV15"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, 1.5V fixed output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "IFX27001TFV15_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "I")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Q")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KA378R05"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "KA378R05"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/KA378R05-D.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Positive 3A 35V Linear Regulator with Disable Pin, LDO, Fixed Output 5V, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive LDO Disable Pin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "KA378R05_0_1")
		(symbol "KA378R05_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vdis")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L200"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "L200"
			(at 5.08 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.8mm_StaggerOdd_Lead7.13mm_TabDown"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.zen22142.zen.co.uk/Circuits/Power/l200.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Adjustable voltage and current regulator, 2A, 36V"
			(at 0 0 0)
		)
		(property "ki_keywords" "2A Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "L200_0_1")
		(symbol "L200_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "LIMIT")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "REF")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L7805"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7805"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
		(symbol "L7805_0_1")
		(symbol "L7805_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L7905"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L7905"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c9/16/86/41/c7/2b/45/f2/CD00000450.pdf/files/CD00000450.pdf/jcr:content/translations/en.CD00000450.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Linear Regulator, Fixed Output -5V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "L7905_0_1")
		(symbol "L7905_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L79L05_SOT89"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L05_SOT89"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "L79L05_SOT89_0_1")
		(symbol "L79L05_SOT89_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD1086D2MTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2MTR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Adjustable TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin2*"
			(at 0 0 0)
		)
		(symbol "LD1086D2MTR_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ/GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD1086D2TTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2TTR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Adjustable, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?2*"
			(at 0 0 0)
		)
		(symbol "LD1086D2TTR_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ/GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD1086DTTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086DTTR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Adjustable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252?2*"
			(at 0 0 0)
		)
		(symbol "LD1086DTTR_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ/GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD1086PUR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086PUR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.3x3.24mm"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Adjustable, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LD1086PUR_0_1")
		(symbol "LD1086PUR_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ/GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD1086V-DG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086V-DG"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Adjustable, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LD1086V-DG_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ/GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD39015M08R"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M08R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 0.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LD39015M08R_0_1")
		(symbol "LD39015M08R_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD39150DT18"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD39150DT18"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld39150.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1.5A Ultra Low Dropout regulator, positive, 1.8V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
		(symbol "LD39150DT18_0_1")
		(symbol "LD39150DT18_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD3985G122R_TSOT23"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G122R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.22V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LD3985G122R_TSOT23_0_1")
		(symbol "LD3985G122R_TSOT23_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD3985M122R_SOT23"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M122R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.22V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LD3985M122R_SOT23_0_1")
		(symbol "LD3985M122R_SOT23_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDK130-08_SOT23_SOT353"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-08_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 0.8V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
		(symbol "LDK130-08_SOT23_SOT353_0_1")
		(symbol "LDK130-08_SOT23_SOT353_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDK130-ADJ_DFN6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-ADJ_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, adjustable positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "LDK130-ADJ_DFN6_0_1")
		(symbol "LDK130-ADJ_DFN6_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDK130-ADJ_SOT23_SOT353"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-ADJ_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, adjustable positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
		(symbol "LDK130-ADJ_SOT23_SOT353_0_1")
		(symbol "LDK130-ADJ_SOT23_SOT353_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDK130PU08R_DFN6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU08R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 0.8V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "LDK130PU08R_DFN6_0_1")
		(symbol "LDK130PU08R_DFN6_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "BP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LK112M15TR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M15TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LK112M15TR_0_1")
		(symbol "LK112M15TR_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "Bypass")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1084-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1084-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 27V Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "LM1084-3.3_0_1")
		(symbol "LM1084-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1084-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1084-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 29V Adjustable Linear Regulator, TO-220 / TO-263 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "LM1084-ADJ_0_1")
		(symbol "LM1084-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1117LD-1.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117LD-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 1.8V fixed output, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON?8*"
			(at 0 0 0)
		)
		(symbol "LM1117LD-1.8_0_1")
		(symbol "LM1117LD-1.8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1117LD-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117LD-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON?8*"
			(at 0 0 0)
		)
		(symbol "LM1117LD-ADJ_0_1")
		(symbol "LM1117LD-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "4")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2931-ADJ_TO92"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2931-ADJ_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA Low drop-out regulator, Adjustable Output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM2931-ADJ_TO92_0_1")
		(symbol "LM2931-ADJ_TO92_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2936-3.0"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-3.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 3.0V fixed output, TO-252/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* SOT?223*"
			(at 0 0 0)
		)
		(symbol "LM2936-3.0_0_1")
		(symbol "LM2936-3.0_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2990SX-5.0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 4.064 0)
		)
		(property "Value" "LM2990SX-5.0"
			(at -3.048 4.064 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2990.pdf"
			(at -31.75 19.05 0)
		)
		(property "Description" "Three termianl low-dropout 1A negative voltage regulator, Input -6V to -26V, Out -5V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin2* TO?220*"
			(at 0 0 0)
		)
		(symbol "LM2990SX-5.0_0_1")
		(symbol "LM2990SX-5.0_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317L_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317L_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snvs775k/snvs775k.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "100mA 35V Adjustable Linear Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM317L_SO8_0_1")
		(symbol "LM317L_SO8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "VO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317L_SOT-89"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317L_SOT-89"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317l.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA 35V Adjustable Linear Regulator, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "LM317L_SOT-89_0_1")
		(symbol "LM317L_SOT-89_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317L_TO92"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317L_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snvs775k/snvs775k.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA 35V Adjustable Linear Regulator, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM317L_TO92_0_1")
		(symbol "LM317L_TO92_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_SOT-223"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_SOT-223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 35V Adjustable Linear Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "LM317_SOT-223_0_1")
		(symbol "LM317_SOT-223_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_TO-220"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_TO-220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 35V Adjustable Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM317_TO-220_0_1")
		(symbol "LM317_TO-220_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_TO-252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_TO-252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/snvs774n/snvs774n.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 35V Adjustable Linear Regulator, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "LM317_TO-252_0_1")
		(symbol "LM317_TO-252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_TO-263"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_TO-263"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 35V Adjustable Linear Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM317_TO-263_0_1")
		(symbol "LM317_TO-263_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_TO3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_TO3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 35V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
		(symbol "LM317_TO3_0_1")
		(symbol "LM317_TO3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM317_TO39"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM317_TO39"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA 35V Adjustable Linear Regulator, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
		(symbol "LM317_TO39_0_1")
		(symbol "LM317_TO39_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337L_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337L_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337l.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA 35V Adjustable Negative Linear Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Negative Voltage Regulator 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM337L_SO8_0_1")
		(symbol "LM337L_SO8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "6")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "VI")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337L_TO92"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337L_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337l.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA 35V Adjustable Linear Regulator, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM337L_TO92_0_1")
		(symbol "LM337L_TO92_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_SOT223"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_SOT223"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Adjustable Linear Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "LM337_SOT223_0_1")
		(symbol "LM337_SOT223_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_TO220"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Adjustable Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM337_TO220_0_1")
		(symbol "LM337_TO220_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_TO252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_TO252"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1636957.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Adjustable Linear Regulator, TO-252(DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "LM337_TO252_0_1")
		(symbol "LM337_TO252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_TO263"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_TO263"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/LM337-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Adjustable Linear Regulator, TO-263(D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "LM337_TO263_0_1")
		(symbol "LM337_TO263_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_TO3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_TO3"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
		(symbol "LM337_TO3_0_1")
		(symbol "LM337_TO3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM337_TO39"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM337_TO39"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Adjustable Linear Regulator, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
		(symbol "LM337_TO39_0_1")
		(symbol "LM337_TO39_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 7.62 270)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3480-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM3480-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3480.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA, Quasi Low Dropout Voltage Regulator, 3.3V positive fixed output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo linear fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM3480-3.3_0_1")
		(symbol "LM3480-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM350_TO220"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM350_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/LM350-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 33V Adjustable Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 3A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM350_TO220_0_1")
		(symbol "LM350_TO220_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM723_DIP14"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 10.795 0)
		)
		(property "Value" "LM723_DIP14"
			(at 0.635 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0.635 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm723.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "Linear Regulator (adjustable), DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "POWER REGUL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM723_DIP14_0_1")
		(symbol "LM723_DIP14_1_1"
			(pin power_out line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V+")
				(number "12")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VC")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "7")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CSEN")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VZ")
				(number "9")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM723_TO100"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.635 10.795 0)
		)
		(property "Value" "LM723_TO100"
			(at 0.635 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-100-10"
			(at 0.635 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm723.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "Linear Regulator (adjustable), TO-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "POWER REGUL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?100*"
			(at 0 0 0)
		)
		(symbol "LM723_TO100_0_1")
		(symbol "LM723_TO100_1_1"
			(pin power_out line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VC")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "10")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CSEN")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "6")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FC")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7805_TO220"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7805_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM7805_TO220_0_1")
		(symbol "LM7805_TO220_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM78M05_TO252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78M05_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78M00-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "LM78M05_TO252_0_1")
		(symbol "LM78M05_TO252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7905_TO220"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7905_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM7905_TO220_0_1")
		(symbol "LM7905_TO220_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM79L05_TO92"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79L05_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-Terminal Negative Regulator, -5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative regulatpr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM79L05_TO92_0_1")
		(symbol "LM79L05_TO92_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2951-3.0_DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.0_DIP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.0V, LDO, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LP2951-3.0_DIP_0_1")
		(symbol "LP2951-3.0_DIP_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTAP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2951-3.0_SOIC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.0_SOIC"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.0V, LDO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LP2951-3.0_SOIC_0_1")
		(symbol "LP2951-3.0_SOIC_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTAP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2951-3.0_VSSOP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.0_VSSOP"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.0V, LDO, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LP2951-3.0_VSSOP_0_1")
		(symbol "LP2951-3.0_VSSOP_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTAP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2951-3.0_WSON"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.0_WSON"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.2x2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.0V, LDO, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LP2951-3.0_WSON_0_1")
		(symbol "LP2951-3.0_WSON_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SHUTDOWN")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FEEDBACK")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTAP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2980-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LP2980-ADJ"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2980-adj.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "50mA 15V Low-noise Low-dropout Regulator, 1.23-15V adjustable output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 50mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LP2980-ADJ_0_1")
		(symbol "LP2980-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2985-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 1.8V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LP2985-1.8_0_1")
		(symbol "LP2985-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ON/~{OFF}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2987-5.0_SOIC8_VSSOP8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-5.0_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 5.0V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LP2987-5.0_SOIC8_VSSOP8_0_1")
		(symbol "LP2987-5.0_SOIC8_VSSOP8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHTD}")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DELAY")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2987-5.0_WSON8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-5.0_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 5.0V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LP2987-5.0_WSON8_0_1")
		(symbol "LP2987-5.0_WSON8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHTD}")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DELAY")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2988-5.0_SOIC8_VSSOP8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-5.0_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 5.0V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LP2988-5.0_SOIC8_VSSOP8_0_1")
		(symbol "LP2988-5.0_SOIC8_VSSOP8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHTD}")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DELAY")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP2988-5.0_WSON8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-5.0_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 5.0V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LP2988-5.0_WSON8_0_1")
		(symbol "LP2988-5.0_WSON8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHTD}")
				(number "8")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DELAY")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "7")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38512MR-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38512MR-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp38512-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Fast-Transient Response Low-Dropout Linear Voltage Regulator with Error Flag, Adjustable Output, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LP38512MR-ADJ_0_1")
		(symbol "LP38512MR-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "DAP")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38512TJ-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38512TJ-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDQ"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp38512.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Fast-Transient Response Low-Dropout Linear Voltage Regulator with Error Flag, 1.8V Output, NDQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDQ*"
			(at 0 0 0)
		)
		(symbol "LP38512TJ-1.8_0_1")
		(symbol "LP38512TJ-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38512TJ-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38512TJ-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_NDQ"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp38512-adj.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Fast-Transient Response Low-Dropout Linear Voltage Regulator with Error Flag, Adjustable Output, NDQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*NDQ*"
			(at 0 0 0)
		)
		(symbol "LP38512TJ-ADJ_0_1")
		(symbol "LP38512TJ-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38512TS-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38512TS-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp38512.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Fast-Transient Response Low-Dropout Linear Voltage Regulator with Error Flag, 1.8V Output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator DDPAK D2PAK"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*TabPin6*"
			(at 0 0 0)
		)
		(symbol "LP38512TS-1.8_0_1")
		(symbol "LP38512TS-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38691SD-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38691SD-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38691.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 1.8V output voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "LP38691SD-1.8_0_1")
		(symbol "LP38691SD-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SNS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38693DT-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693DT-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 1.8V output voltage, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "LP38693DT-1.8_0_1")
		(symbol "LP38693DT-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38693MP-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693MP-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 1.8V output voltage, Enable Pin, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
		(symbol "LP38693MP-1.8_0_1")
		(symbol "LP38693MP-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP38693SD-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693SD-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 1.8V output voltage, Enable Pin, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "LP38693SD-1.8_0_1")
		(symbol "LP38693SD-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SNS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3963-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3963-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 1.8V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LP3963-1.8_0_1")
		(symbol "LP3963-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3966-1.8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3966-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 1.8V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LP3966-1.8_0_1")
		(symbol "LP3966-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3966-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3966-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, adjustable output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LP3966-ADJ_0_1")
		(symbol "LP3966-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3982ILD-1.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982ILD-1.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack_ThermalVias"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LP3982ILD-1.8_0_1")
		(symbol "LP3982ILD-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3982ILD-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982ILD-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack_ThermalVias"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA, Micropower, Ultra-Low-Dropout, Low-Noise Adjustable CMOS Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "adjustable linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LP3982ILD-ADJ_0_1")
		(symbol "LP3982ILD-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3982IMM-1.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMM-1.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LP3982IMM-1.8_0_1")
		(symbol "LP3982IMM-1.8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP3982IMM-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMM-ADJ"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA, Micropower, Ultra-Low-Dropout, Low-Noise Adjustable CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "adjustable linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LP3982IMM-ADJ_0_1")
		(symbol "LP3982IMM-ADJ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP5907MFX-1.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-1.2"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 1.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LP5907MFX-1.2_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP5912-0.9DRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-0.9DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 0.9V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LP5912-0.9DRV_0_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(symbol "LP5912-0.9DRV_1_1"
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LR8K4-G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 3.81 0)
		)
		(property "Value" "LR8K4-G"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005399B.pdf"
			(at 0 0 0)
		)
		(property "Description" "30mA 450V High-Voltage Linear Regulator (Adjustable), TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "LR8K4-G_0_1")
		(symbol "LR8K4-G_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LR8N3-G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 3.81 0)
		)
		(property "Value" "LR8N3-G"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.supertex.com/pdf/datasheets/LR8.pdf"
			(at 0 0 0)
		)
		(property "Description" "30mA 450V High-Voltage Linear Regulator (Adjustable), TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LR8N3-G_0_1")
		(symbol "LR8N3-G_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LR8N8-G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 3.81 0)
		)
		(property "Value" "LR8N8-G"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.supertex.com/pdf/datasheets/LR8.pdf"
			(at 0 0 0)
		)
		(property "Description" "30mA 450V High-Voltage Linear Regulator (Adjustable), SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Voltage Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*"
			(at 0 0 0)
		)
		(symbol "LR8N8-G_0_1")
		(symbol "LR8N8-G_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1117-2.85"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1117-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1117fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.85V fixed output, SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263*"
			(at 0 0 0)
		)
		(symbol "LT1117-2.85_0_1")
		(symbol "LT1117-2.85_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1117-ADJ"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1117-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1117fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263*"
			(at 0 0 0)
		)
		(symbol "LT1117-ADJ_0_1")
		(symbol "LT1117-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1129-3.3_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-3.3_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, 3.3V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1129-3.3_SO8_0_1")
		(symbol "LT1129-3.3_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1129-3.3_TO220_TO263"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-3.3_TO220_TO263"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, 3.3V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LT1129-3.3_TO220_TO263_0_1")
		(symbol "LT1129-3.3_TO220_TO263_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1129-ADJ_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-ADJ_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, adjustable output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LT1129-ADJ_SO8_0_1")
		(symbol "LT1129-ADJ_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1129-ADJ_TO220_TO263"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-ADJ_TO220_TO263"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, adjustable output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LT1129-ADJ_TO220_TO263_0_1")
		(symbol "LT1129-ADJ_TO220_TO263_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1175-5_SO8_DIP8"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.715 -8.255 0)
		)
		(property "Value" "LT1175-5_SO8_DIP8"
			(at 0 -8.255 0)
		)
		(property "Footprint" ""
			(at 0.635 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 -5.08 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, fixed output voltage -5V, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1175-5_SO8_DIP8_0_1")
		(symbol "LT1175-5_SO8_DIP8_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ILIM4")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ILIM2")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1175-5_SOT223"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LT1175-5_SOT223"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, fixed output voltage -5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "LT1175-5_SOT223_0_1")
		(symbol "LT1175-5_SOT223_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1175-5_TO263_TO220"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.715 -3.175 0)
		)
		(property "Value" "LT1175-5_TO263_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, fixed output voltage -5V, TO-220-5/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
		(symbol "LT1175-5_TO263_TO220_0_1")
		(symbol "LT1175-5_TO263_TO220_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1584-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1584-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 7A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 7A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LT1584-3.3_0_1")
		(symbol "LT1584-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1585-3.3"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1585-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 4.6A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 4.6A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "LT1585-3.3_0_1")
		(symbol "LT1585-3.3_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1585-ADJ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1585-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 4.6A 35V Low Dropout Fast Response Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 4.6A Positive Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "LT1585-ADJ_0_1")
		(symbol "LT1585-ADJ_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1761-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 5V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1761-5_0_1")
		(symbol "LT1761-5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1761-BYP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-BYP"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER 100mA LDO adjustable regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1761-BYP_0_1")
		(symbol "LT1761-BYP_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1761-SD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-SD"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER 100mA LDO adjustable regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1761-SD_0_1")
		(symbol "LT1761-SD_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1962"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "300mA, Adjustable, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT1962_0_1")
		(symbol "LT1962_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1962-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-5"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "5.0V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT1962-5_0_1")
		(symbol "LT1962-5_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1963AxQ-1.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxQ-1.5"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.5V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "LT1963AxQ-1.5_0_1")
		(symbol "LT1963AxQ-1.5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1963AxST-1.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxST-1.5"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.5V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
		(symbol "LT1963AxST-1.5_0_1")
		(symbol "LT1963AxST-1.5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1963EQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963EQ"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963fc.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.5A, Adjustable, Low Noise, Linear Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "LT1963EQ_0_1")
		(symbol "LT1963EQ_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1964-5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -5.715 0)
		)
		(property "Value" "LT1964-5"
			(at 0 -5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1964fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER 200mA Low Noise LDO negative regulator, fixed output -5V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1964-5_0_1")
		(symbol "LT1964-5_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1964-BYP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -5.715 0)
		)
		(property "Value" "LT1964-BYP"
			(at 0 -5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1964fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER 200mA Low Noise LDO negative regulator, adjustable output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1964-BYP_0_1")
		(symbol "LT1964-BYP_1_1"
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1964-SD"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -5.715 0)
		)
		(property "Value" "LT1964-SD"
			(at 0 -5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1964fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER 200mA Low Noise LDO negative regulator, adjustable output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT1964-SD_0_1")
		(symbol "LT1964-SD_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3010"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/30105fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA 3-80V Micropower Low Dropout Regulator, adjustable output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3010_0_1")
		(symbol "LT3010_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3010-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3010-5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/30105fe.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA 3-80V Micropower Low Dropout Regulator, fixed output 5V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3010-5_0_1")
		(symbol "LT3010-5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3011xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "LT3011xDD"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 3.81 12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3011f.pdf"
			(at 3.81 13.97 0)
		)
		(property "Description" "50mA, 3V to 80V Low Dropout Micropower Linear Regulator with PWRGD, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "variable regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3011xDD_0_1")
		(symbol "LT3011xDD_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "10")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "8")
			)
			(pin open_collector line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "PWRGD")
				(number "5")
			)
			(pin unspecified line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3011xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "LT3011xMSE"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 3.81 12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3011f.pdf"
			(at 3.81 13.97 0)
		)
		(property "Description" "50mA, 3V to 80V Low Dropout Micropower Linear Regulator with PWRGD, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "variable regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3011xMSE_0_1")
		(symbol "LT3011xMSE_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "11")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "9")
			)
			(pin open_collector line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "PWRGD")
				(number "6")
			)
			(pin unspecified line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3015Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015Q"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A, Adjustable, Low Noise, Negative Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "LT3015Q_0_1")
		(symbol "LT3015Q_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3015xQ-2.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-2.5"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-2.5V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "LT3015xQ-2.5_0_1")
		(symbol "LT3015xQ-2.5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SENSE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3032"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3032"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_DE14MA"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3032ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, Dual Low Dropout Linear Regulator, Positive/Negative Low Noise, Adjustable Output, DFN-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*DE14MA*"
			(at 0 0 0)
		)
		(symbol "LT3032_0_1")
		(symbol "LT3032_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INP")
				(number "14")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDNP}")
				(number "12")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTP")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJP")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYPP")
				(number "3")
			)
		)
		(symbol "LT3032_2_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INN")
				(number "6")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "INN")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDNN}")
				(number "10")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTN")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJN")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYPN")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3032-5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3032-5"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_DE14MA"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3032ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, Dual Low Dropout Linear Regulator, Positive/Negative Low Noise, 5V Output, DFN-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*DE14MA*"
			(at 0 0 0)
		)
		(symbol "LT3032-5_0_1")
		(symbol "LT3032-5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INP")
				(number "14")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDNP}")
				(number "12")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTP")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYPP")
				(number "3")
			)
		)
		(symbol "LT3032-5_2_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INN")
				(number "6")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "INN")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDNN}")
				(number "10")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTN")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYPN")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3033xUDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT3033xUDC"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:UDC-QFN-20-4EP_3x4mm_P0.5mm_EP0.41x0.25mm"
			(at 0 10.795 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3033.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "3A, Very Low Dropout Linear Regulator with Programmable Current Limit, 0.95V to 10Vin, 0.2V to 9.7Vout, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear positive voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*4EP*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3033xUDC_0_0"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "15")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "16")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "21")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "22")
			)
		)
		(symbol "LT3033xUDC_0_1")
		(symbol "LT3033xUDC_1_0"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "14")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "17")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "23")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "24")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
		)
		(symbol "LT3033xUDC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "12")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "PWRGD")
				(number "11")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "REF/BYP")
				(number "9")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "10")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IMON")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3042xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3042xMSE"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3042fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA, Adjustable, Ultralow Noise, Ultrahigh PSRR RF Linear Regulator, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3042xMSE_0_1")
		(symbol "LT3042xMSE_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UV")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTS")
				(number "9")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGFB")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3045xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3045xDD"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3045fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, Adjustable, Ultralow Noise, Ultrahigh PSRR Linear Regulator, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3045xDD_0_1")
		(symbol "LT3045xDD_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UV")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "5")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTS")
				(number "9")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGFB")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3045xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3045xMSE"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3045fa.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA, Adjustable, Ultralow Noise, Ultrahigh PSRR Linear Regulator, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3045xMSE_0_1")
		(symbol "LT3045xMSE_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN/UV")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ILIM")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "12")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTS")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PGFB")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3080xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.445 6.35 0)
		)
		(property "Value" "LT3080xDD"
			(at 10.16 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3080fc.pdf"
			(at 0.254 20.828 0)
		)
		(property "Description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, DFN-8"
			(at 0.254 18.034 0)
		)
		(property "ki_keywords" "linear analog linear-technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP?3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3080xDD_0_1")
		(symbol "LT3080xDD_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{CONTROL}")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3080xMS8E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.604 0)
		)
		(property "Value" "LT3080xMS8E"
			(at 10.414 6.604 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3080fc.pdf"
			(at -0.254 18.542 0)
		)
		(property "Description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, MSOP-8"
			(at 1.016 15.748 0)
		)
		(property "ki_keywords" "linear analog linear-technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP?3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3080xMS8E_0_1")
		(symbol "LT3080xMS8E_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{CONTROL}")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3080xQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.604 0)
		)
		(property "Value" "LT3080xQ"
			(at 10.414 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at -5.08 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3080fc.pdf"
			(at -43.688 19.558 0)
		)
		(property "Description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, TO-220"
			(at 0 10.16 0)
		)
		(property "ki_keywords" "linear analog linear-technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin3*"
			(at 0 0 0)
		)
		(symbol "LT3080xQ_0_1")
		(symbol "LT3080xQ_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{CONTROL}")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3080xST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3080xST"
			(at 7.874 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3080fc.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, SOT-223"
			(at 1.27 9.398 0)
		)
		(property "ki_keywords" "linear analog linear-technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "LT3080xST_0_1")
		(symbol "LT3080xST_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3080xT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 6.604 0)
		)
		(property "Value" "LT3080xT"
			(at 10.414 6.604 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3080fc.pdf"
			(at 0.762 13.97 0)
		)
		(property "Description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, TO-220"
			(at 0.762 10.414 0)
		)
		(property "ki_keywords" "linear analog linear-technology"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*"
			(at 0 0 0)
		)
		(symbol "LT3080xT_0_1")
		(symbol "LT3080xT_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "V_{CONTROL}")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3091xT7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LT3091xT7"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-7_P2.54x3.7mm_StaggerOdd_Lead3.8mm_Vertical"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3091fa.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "–36V, 1.5A Negative Linear Adjustable Regulator with Programmable Current Limit, TO-220-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*P2.54x3.7mm*"
			(at 0 0 0)
		)
		(symbol "LT3091xT7_0_1")
		(symbol "LT3091xT7_1_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IMONN")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SET")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "LT3091xT7_1_1"
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "GND")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3093xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT3093xMSE"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 10.795 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt3093.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "-200mA, Adjustable, Ultralow Noise, Ultrahigh PSRR RF Negative Linear Regulator, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear negative voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT3093xMSE_0_0"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "12")
			)
		)
		(symbol "LT3093xMSE_0_1")
		(symbol "LT3093xMSE_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/UV")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 0 0)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIOC")
				(number "7")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SET")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTS")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "PGFB")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ILIM")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC3026-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "LTC3026-1"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/30261f.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.14V-5.5V, 1.5A Low Input Voltage VLDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator LDO positive adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*EP1.65x2.38mm* MSOP*1EP*3x3mm*P0.5mm*EP1.68x1.88mm*"
			(at 0 0 0)
		)
		(symbol "LTC3026-1_0_1")
		(symbol "LTC3026-1_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "BIAS")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GNDS")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "10")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1615xUK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MAX1615xUK"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1615-MAX1616.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "High Voltage, Low Power Linear Regulator for Notebook PCs - 3.3V or 5V Fixed"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "MAX1615xUK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "5/~{3}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1616xUK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MAX1616xUK"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1615-MAX1616.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "High Voltage, Low Power Linear Regulator for Notebook PCs - Adjustable"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "MAX1616xUK_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1658ESA"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MAX1658ESA"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX1658-MAX1659.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "350mA Linear LDO Regulator, Fixed Output 3.3V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 350mA 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX1658ESA_0_1")
		(symbol "MAX1658ESA_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHTD}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SET")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX16910"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MAX16910"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 0 13.335 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX16910.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Automotive Linear LDO Regulator, Fixed Output 5V/3.3V or Adjustable, SO-8/DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX16910_0_1")
		(symbol "MAX16910_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "TIMEOUT")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND/PAD")
				(number "9")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SET0V")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX38908xTD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX38908xTD"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX38907-MAX38908.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A, High-Performance LDO Linear Regulator, 0.9V-5.5Vin, 0.6V-5Vout, 2.7V-20Vbias, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator Maxim Analog Devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TDFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX38908xTD_0_1")
		(symbol "MAX38908xTD_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "BIAS")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "12")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "14")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "POK")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX38911ATA+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX38911ATA+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX38911-MAX38912.pdf"
			(at 0 0 0)
		)
		(property "Description" "11μVRMS Low-Noise, 500mA LDO Linear Regulator with Low-Power Mode, 2V-5.5Vin, 1.8Vout, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator Maxim Analog Devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX38911ATA+_0_1")
		(symbol "MAX38911ATA+_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "MODE")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTS")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "POK")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX38912ATA+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX38912ATA+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX38911-MAX38912.pdf"
			(at 0 0 0)
		)
		(property "Description" "11μVRMS Low-Noise, 500mA LDO Linear Regulator with Low-Power Mode, 1.7V-5.5Vin, 0.8V-5Vout, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator Maxim Analog Devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TDFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX38912ATA+_0_1")
		(symbol "MAX38912ATA+_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "MODE")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "BYP")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "POK")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX5092AATE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 15.875 0)
		)
		(property "Value" "MAX5092AATE"
			(at 0 15.875 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 18.415 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5092-MAX5093.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "4V to 72V Input LDOs with Boost Preregulator, 250mA Output, 3.3V Preset Vout, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage 72V Input LDO Boost Preregulator 250mA 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MAX5092AATE_0_1")
		(symbol "MAX5092AATE_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "LX")
				(number "10")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "LX")
				(number "11")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{HOLD}")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "16")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CT")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "SGND/PAD")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "SGND")
				(number "3")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "BSOUT")
				(number "9")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BSFB")
				(number "13")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VL")
				(number "14")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PGND_BST")
				(number "12")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT_SENSE")
				(number "7")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PGND_LDO")
				(number "5")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX603"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MAX603"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX603-MAX604.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "500mA Linear LDO Regulator, Fixed Output 5V, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 500mA 5V fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX603_0_1")
		(symbol "MAX603_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{OFF}")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SET")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX663"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "MAX663"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://pdfserv.maximintegrated.com/en/ds/MAX663-MAX666.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "50mA Dual Mode 5V/Programmable Micropower Voltage Regulator, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 50mA 5V fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX663_0_1")
		(symbol "MAX663_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT1")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "2")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VTC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX664"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 -8.255 0)
		)
		(property "Value" "MAX664"
			(at 0 -8.255 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.27 0)
		)
		(property "Datasheet" "http://pdfserv.maximintegrated.com/en/ds/MAX663-MAX666.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "50mA Dual Mode -5V/Programmable Micropower Negative Voltage Regulator, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 50mA -5V fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX664_0_1")
		(symbol "MAX664_1_1"
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "SHDN")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT1")
				(number "7")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT2")
				(number "1")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX666"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "MAX666"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "http://pdfserv.maximintegrated.com/en/ds/MAX663-MAX666.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "50mA Dual Mode 5V/Programmable Micropower Voltage Regulator, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 50mA 5V fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX666_0_1")
		(symbol "MAX666_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "LBI")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "VSET")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LBO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX883"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "MAX883"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX882-MAX884.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Fixed Output 5V or Adjustable with Shutdown Mode, 0C to +70C, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX883_0_1")
		(symbol "MAX883_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{OFF}(~{STBY})")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{LBI}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SET")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{LBO}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC78L05_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L05_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC78L05_SO8_0_1")
		(symbol "MC78L05_SO8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC78L05_SOT89"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L05_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "MC78L05_SOT89_0_1")
		(symbol "MC78L05_SOT89_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC78L05_TO92"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L05_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "MC78L05_TO92_0_1")
		(symbol "MC78L05_TO92_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC78LC18NTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78LC18NTR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc78lc00-d.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 50mA 12V Linear Regulator, Fixed Output 1.8V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 50mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MC78LC18NTR_0_1")
		(symbol "MC78LC18NTR_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC79L05_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79L05_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC79L05_SO8_0_1")
		(symbol "MC79L05_SO8_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC79M05_TO252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M05_TO252"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -5V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "MC79M05_TO252_0_1")
		(symbol "MC79M05_TO252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1700x-300xxTT"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-300xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.0V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1700x-300xxTT_0_1")
		(symbol "MCP1700x-300xxTT_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1703Ax-330xxDB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-330xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.3V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
		(symbol "MCP1703Ax-330xxDB_0_1")
		(symbol "MCP1703Ax-330xxDB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1703Ax-330xxMB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-330xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.3V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "MCP1703Ax-330xxMB_0_1")
		(symbol "MCP1703Ax-330xxMB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1703Ax-330xxTT"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-330xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.3V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1703Ax-330xxTT_0_1")
		(symbol "MCP1703Ax-330xxTT_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1727-0802xMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "MCP1727-0802xMF"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 0.8V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1727-0802xMF_0_0"
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Cdelay")
				(number "6")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "Sense")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWRGD")
				(number "5")
			)
		)
		(symbol "MCP1727-0802xMF_0_1")
		(symbol "MCP1727-0802xMF_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1727-0802xSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "MCP1727-0802xSN"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 0.8V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP1727-0802xSN_0_0"
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Cdelay")
				(number "6")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "Sense")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWRGD")
				(number "5")
			)
		)
		(symbol "MCP1727-0802xSN_0_1")
		(symbol "MCP1727-0802xSN_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1727-ADJxMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "MCP1727-ADJxMF"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Adjustable Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Adjustable LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1727-ADJxMF_0_0"
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Cdelay")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "ADJ")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWRGD")
				(number "5")
			)
		)
		(symbol "MCP1727-ADJxMF_0_1")
		(symbol "MCP1727-ADJxMF_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1727-ADJxSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "MCP1727-ADJxSN"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Adjustable Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Adjustable LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP1727-ADJxSN_0_0"
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Cdelay")
				(number "6")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "ADJ")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWRGD")
				(number "5")
			)
		)
		(symbol "MCP1727-ADJxSN_0_1")
		(symbol "MCP1727-ADJxSN_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "Vin")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1754S-5002xCB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-5002xCB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 5V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1754S-5002xCB_0_1")
		(symbol "MCP1754S-5002xCB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1754S-5002xMB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-5002xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 5V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "MCP1754S-5002xMB_0_1")
		(symbol "MCP1754S-5002xMB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1804x-1802xDB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-1802xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 1.8V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "MCP1804x-1802xDB_0_1")
		(symbol "MCP1804x-1802xDB_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1804x-1802xMT"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-1802xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 1.8V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "MCP1804x-1802xMT_0_1")
		(symbol "MCP1804x-1802xMT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1804x-1802xOT"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-1802xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 1.8V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1804x-1802xOT_0_1")
		(symbol "MCP1804x-1802xOT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1825S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1825S"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at -2.54 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/22056b.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "500mA, Low-Voltage, Low Quiescent Current LDO Regulator, SOT-223, TO-220, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2* TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "MCP1825S_0_1")
		(symbol "MCP1825S_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1826S"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1826S"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at -2.54 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22057B.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "1000mA, Low-Voltage, Low Quiescent Current LDO Regulator, SOT-223, TO-220, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2* TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "MCP1826S_0_1")
		(symbol "MCP1826S_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ME6211C33M5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C33M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "500mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 3.3V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "ME6211C33M5_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "CE")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29152WT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29152WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
		(symbol "MIC29152WT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29152WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29152WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "1.5A low dropout linear regulator, adjustable output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
		(symbol "MIC29152WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29153WT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29153WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
		(symbol "MIC29153WT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29153WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29153WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A low dropout linear regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "MIC29153WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FLG")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29302WU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29302WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "MIC29302WU_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC29752WT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29752WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-5_Vertical"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A low dropout linear regulator, adjustable output, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "7.5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*247*"
			(at 0 0 0)
		)
		(symbol "MIC29752WT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5205YM5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, adjustable output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MIC5205YM5_0_1")
		(symbol "MIC5205YM5_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5219-2.5YMM"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.5YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.5V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC5219-2.5YMM_0_1")
		(symbol "MIC5219-2.5YMM_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5219YMM"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, adjustable output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC5219YMM_0_1")
		(symbol "MIC5219YMM_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5350"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "MIC5350"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:Micrel_MLF-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5350.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "dual 300mA/500mA LDO, MLF-8"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "dual LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MLF*2x2mm*P0.5mm*EP0.6x1.2mm*"
			(at 0 0 0)
		)
		(symbol "MIC5350_0_1"
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "MIC5350_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "4")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT1")
				(number "8")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "BYP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5353-2.5YMT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-2.5YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MIC5353-2.5YMT_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "BYP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5353YMT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353YMT"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MIC5353YMT_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "BYP")
				(number "6")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5355-S4YMME"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5355-S4YMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.2V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC5355-S4YMME_0_1")
		(symbol "MIC5355-S4YMME_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "4")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT1")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5356-MMYML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-MMYML"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-8-1EP_3x3mm_P0.65mm_EP1.55x2.3mm_ThermalVias"
			(at 38.1 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 2.8V/2.8V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA DFN-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC5356-MMYML_0_1")
		(symbol "MIC5356-MMYML_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN1")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "4")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOUT1")
				(number "8")
			)
			(pin power_out line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VOUT2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5365-3.3YC5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5365-3.3YC5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5365.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
		(symbol "MIC5365-3.3YC5_0_1")
		(symbol "MIC5365-3.3YC5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5365-3.3YD5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "MIC5365-3.3YD5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5365.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MIC5365-3.3YD5_0_1")
		(symbol "MIC5365-3.3YD5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC5504-3.3YM5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5504-3.3YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "MIC5504-3.3YM5_0_1")
		(symbol "MIC5504-3.3YM5_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1117-12_TO252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-12_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 12V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 12V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "NCP1117-12_TO252_0_1")
		(symbol "NCP1117-12_TO252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP1117-ADJ_TO252"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-ADJ_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Adjustable Output 1.25 - 18.8V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO ADJUSTABLE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "NCP1117-ADJ_TO252_0_1")
		(symbol "NCP1117-ADJ_TO252_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ADJ")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP115AMX120TCG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "NCP115AMX120TCG"
			(at 10.16 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP115-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "300mA Low-Dropout Linear Regulators, 1.2V output voltage, LDO with low noise and enable pin, XDFN-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*XDFN4*1EP*1.0x1.0mm*"
			(at 0 0 0)
		)
		(symbol "NCP115AMX120TCG_0_1")
		(symbol "NCP115AMX120TCG_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP133AMX100TCG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "NCP133AMX100TCG"
			(at 10.16 5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 15.24 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NCP133-D.PDF"
			(at 1.27 -15.24 0)
		)
		(property "Description" "500  mA  VLDO  equipped  with  NMOS  pass transistor  and  a  separate  bias  supply  voltage"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN?6?1EP*1.2x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "NCP133AMX100TCG_0_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "BIAS")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "ADJ/NC")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP163AFCS120T2G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS120T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.2V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "NCP163AFCS120T2G_0_1")
		(symbol "NCP163AFCS120T2G_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "A1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "B1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP163ASN150T1G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN150T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.5V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "NCP163ASN150T1G_0_1")
		(symbol "NCP163ASN150T1G_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP662SQ15"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "NCP662SQ15"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-82AB"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP662-D.PDF"
			(at -7.62 20.32 0)
		)
		(property "Description" "100-mA, 12V Max. Input, Ultralow-IQ LDO, 1.5V, SC-82AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?82AB*"
			(at 0 0 0)
		)
		(symbol "NCP662SQ15_0_1")
		(symbol "NCP662SQ15_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCV8114ASN120T1G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN120T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.2V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "NCV8114ASN120T1G_0_1")
		(symbol "NCV8114ASN120T1G_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NVC8674DS50"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "NVC8674DS50"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCV8674-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "350mA, 5.0V Very Low Iq Low Dropout Linear Regulator, TO-263-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo regulator 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
		(symbol "NVC8674DS50_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPX2920M3-3.3_SOT223"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920M3-3.3_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "SPX2920M3-3.3_SOT223_0_1")
		(symbol "SPX2920M3-3.3_SOT223_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPX2920S-3.3_SO8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 3.81 0)
		)
		(property "Value" "SPX2920S-3.3_SO8"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "400mA Fixed/Adjustable 1.2-20V Low Drop-out Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 400mA 3.3V Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SPX2920S-3.3_SO8_0_1")
		(symbol "SPX2920S-3.3_SO8_1_1"
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{SD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TAP")
				(number "6")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SPX2920T-3.3_TO263"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920T-3.3_TO263"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 3.3V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "SPX2920T-3.3_TO263_0_1")
		(symbol "SPX2920T-3.3_TO263_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1014-xCT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1014-xCT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/21335e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "50 mA CMOS LDOs with Shutdown and Reference Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TC1014-xCT_0_1")
		(symbol "TC1014-xCT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "Bypass")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1017-xCT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1017-xCT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -6.35 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21813F.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "150mA, Tiny CMOS LDO With Shutdown, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TC1017-xCT_0_1")
		(symbol "TC1017-xCT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1017-xLT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1017-xLT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -6.35 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21813F.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "150mA, Tiny CMOS LDO With Shutdown, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
		(symbol "TC1017-xLT_0_1")
		(symbol "TC1017-xLT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1017R-xLT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1017R-xLT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at -6.35 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21813F.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "150mA, Tiny CMOS LDO With Shutdown, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
		(symbol "TC1017R-xLT_0_1")
		(symbol "TC1017R-xLT_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1054"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TC1054"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 6.985 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21350E.pdf"
			(at -7.62 5.08 0)
		)
		(property "Description" "50mA Low Dropout Regulator with ERROR output in 5-Pin SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TC1054_0_1")
		(symbol "TC1054_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{ERROR}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC1262-33"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TC1262-33"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA Low Dropout CMOS Voltage Regulator, Fixed Output 3.3V, TO-220/SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3.3V 500mA Positive CMOS LDO Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?220* TO?263*"
			(at 0 0 0)
		)
		(symbol "TC1262-33_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VI")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCR2EE11"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE11"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.1V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
		(symbol "TCR2EE11_0_1")
		(symbol "TCR2EE11_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV70012_SOT23-5"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70012_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV70012_SOT23-5_0_1")
		(symbol "TLV70012_SOT23-5_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV70012_SOT353"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70012_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5/SC-70-5/SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
		(symbol "TLV70012_SOT353_0_1")
		(symbol "TLV70012_SOT353_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV70012_WSON6"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70012_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.2V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
		(symbol "TLV70012_WSON6_0_1")
		(symbol "TLV70012_WSON6_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV71x_WSON-6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TLV71x_WSON-6"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv711.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Dual, 200mA, Low-Iq Low-Dropout Regulator for Portable Devices, SON-6"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "dual LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON*1.5x1.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLV71x_WSON-6_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN1")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN2")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV75509PDRV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75509PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 0.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLV75509PDRV_0_1")
		(symbol "TLV75509PDRV_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV75801PDBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TLV75801PDBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv758p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low-Dropout Linear Regulator, Adjustable Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TLV75801PDBV_0_1")
		(symbol "TLV75801PDBV_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV75801PDRV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TLV75801PDRV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv758p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low-Dropout Linear Regulator, Adjustable Output, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLV75801PDRV_0_1")
		(symbol "TLV75801PDRV_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV76701DRVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76701DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Adjustable Output 0.8-13.6V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A, 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "TLV76701DRVx_0_1")
		(symbol "TLV76701DRVx_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV76701QWDRBxQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76701QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Adjustable Output 0.8-14.6V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLV76701QWDRBxQ1_0_1")
		(symbol "TLV76701QWDRBxQ1_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV76733QWDRBxQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76733QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 3.3V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLV76733QWDRBxQ1_0_1")
		(symbol "TLV76733QWDRBxQ1_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "SNS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLV76750DRVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76750DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 5.0V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A, 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
		(symbol "TLV76750DRVx_0_1")
		(symbol "TLV76750DRVx_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "SNS")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS51200DRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TPS51200DRC"
			(at 7.62 10.16 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps51200.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "Sink and Source DDR Termination Regulator, VSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "DDR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSON?10?1EP?3x3mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS51200DRC_0_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "VIN")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "VOSNS")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "EN")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VLDOIN")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "VO")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "PGOOD")
				(number "9")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "REFIN")
				(number "1")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "REFOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS70202_HTSSOP20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 15.875 0)
		)
		(property "Value" "TPS70202_HTSSOP20"
			(at -3.81 15.875 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps702.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA/250mA Dual Adjustable Low Drop-out Regulator with Voltage Supervisor, PowerPAD TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO Adjustable Regulator 500mA 250mA Voltage Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS70202_HTSSOP20_0_1")
		(symbol "TPS70202_HTSSOP20_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(hide yes)
				(name "VIN1")
				(number "2")
			)
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{EN1}")
				(number "5")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN2")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "VIN2")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{EN2}")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{MR}")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "VOUT1")
				(number "18")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VOUT1")
				(number "19")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "FB1")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PG1")
				(number "16")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "VOUT2")
				(number "12")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB2")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PG2")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS70245_HTSSOP20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.335 0)
		)
		(property "Value" "TPS70245_HTSSOP20"
			(at -2.54 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps702.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "3.3V 500mA/1.2V 250mA Dual Low Drop-out Regulator with Voltage Supervisor, PowerPAD TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual 3.3V 1.2V LDO Regulator 500mA 250mA Voltage Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS70245_HTSSOP20_0_1")
		(symbol "TPS70245_HTSSOP20_1_1"
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN1")
				(number "2")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{EN1}")
				(number "5")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN2")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "VIN2")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{EN2}")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{MR}")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "VOUT1")
				(number "18")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUT1")
				(number "19")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENS1")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PG1")
				(number "16")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "VOUT2")
				(number "12")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSENS2")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PG2")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS70302"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70302"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps703.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Sequenced Outputs, ADJ 1A/ADJ 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS70302_0_1")
		(symbol "TPS70302_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN1")
				(number "2")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{MR1}")
				(number "6")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN2")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "VIN2")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{MR2}")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SEQ")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "24")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND/HS")
				(number "25")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUT1")
				(number "22")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "VOUT1")
				(number "23")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENSE1/FB1")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PG1")
				(number "19")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "14")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "VOUT2")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSENSE2/FB2")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS70402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70402"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps704.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Independent Enable, ADJ 1A/ADJ 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS70402_0_1")
		(symbol "TPS70402_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN1")
				(number "2")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{EN1}")
				(number "6")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIN2")
				(number "10")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "VIN2")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{EN2}")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{MR}")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "24")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND/HS")
				(number "25")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VOUT1")
				(number "22")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "VOUT1")
				(number "23")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VSENSE1/FB1")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PG1")
				(number "19")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT2")
				(number "14")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "VOUT2")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSENSE2/FB2")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PG2")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7101"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS7101"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps71.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "500mA Adjustable 1.2-9.75V Low Drop-out Voltage Regulator, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 500mA Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TPS7101_0_1")
		(symbol "TPS7101_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7150"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "TPS7150"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps71.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Low Drop-out Voltage Regulator, Fixed Output 5V, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TPS7150_0_1")
		(symbol "TPS7150_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS71518__SC70"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71518__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 1.8V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TPS71518__SC70_0_1")
		(symbol "TPS71518__SC70_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS72201"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS72201"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps722.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low input voltage 50mA LDO variable output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS72201_0_1")
		(symbol "TPS72201_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS72218"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS72218"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps722.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low input voltage 50mA LDO, 1.8V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS72218_0_1")
		(symbol "TPS72218_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS72301DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS72301DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps723.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "200-mA, Low-Noise, High-PSRR, Negative Output Low-Dropout Linear Regulator, Adjustable Output (-1.2 V to -10 V), SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS72301DBV_0_1")
		(symbol "TPS72301DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS72325DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS72325DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps723.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "200-mA, Low-Noise, High-PSRR, Negative Output Low-Dropout Linear Regulator, Fixed Output -2.5 V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS72325DBV_0_1")
		(symbol "TPS72325DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "NR")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS73601DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73601DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop Adjustable Out Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Adjustable LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS73601DBV_0_1")
		(symbol "TPS73601DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS73625DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73625DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 2.5V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS73625DBV_0_1")
		(symbol "TPS73625DBV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "NR")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS74401_VQFN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS74401_VQFN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" ""
			(at 20.32 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=tps74401&fileType=pdf"
			(at 0 12.7 0)
		)
		(property "Description" "0.8 to 3.6V adjustable, 3.0-A, Ultra-LDO with Programmable Soft-Start"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*VQFN*RGR* Texas*VQFN*RGW*"
			(at 0 0 0)
		)
		(symbol "TPS74401_VQFN_0_1")
		(symbol "TPS74401_VQFN_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "6")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "BIAS")
				(number "10")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin no_connect line
				(at -2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin no_connect line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "18")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PG")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS74801AWDRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS74801AWDRC"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps748a.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Texas Instruments 1.5A, Low-Dropout Linear Regulator With Programmable Soft-Start, 0.8-6.0Vin, 2.7-6.0Vbias, 0.8-3.6Vout"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator LDO positive adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS74801AWDRC_0_1")
		(symbol "TPS74801AWDRC_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "BIAS")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "10")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS75005RGW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "TPS75005RGW"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps75005.pdf"
			(at 0 0 0)
		)
		(property "Description" "Integrated MCU Power Solution, Dual Low Drop-Out Regulator 500mA with Supervisor, VQFN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO Regulator Dual Integrated Power SVS Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS75005RGW_0_1")
		(symbol "TPS75005RGW_1_1"
			(pin power_in line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IN")
				(number "18")
			)
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IN")
				(number "19")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VMON")
				(number "16")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "EN")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SEQ")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VSET")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "TEST")
				(number "11")
			)
			(pin power_in line
				(at -10.16 -22.86 90)
				(length 2.54)
				(name "PAD")
				(number "21")
			)
			(pin power_in line
				(at -7.62 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "SS1")
				(number "12")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "CT1")
				(number "13")
			)
			(pin input line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "SS2")
				(number "4")
			)
			(pin passive line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "CT2")
				(number "3")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "VDET")
				(number "5")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT1_S")
				(number "14")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT2")
				(number "1")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT2_S")
				(number "2")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PG")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS76301"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76301"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO variable output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS76301_0_1")
		(symbol "TPS76301_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS76316"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76316"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO, 1.6V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS76316_0_1")
		(symbol "TPS76316_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS76901"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76901"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Adjustable Out Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Adjustable LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS76901_0_1")
		(symbol "TPS76901_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS76912"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76912"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS76912_0_1")
		(symbol "TPS76912_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77701_HTSSOP20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77701_HTSSOP20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 3.81 -5.08 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Adjustable Output 1.5-5.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS77701_HTSSOP20_0_1")
		(symbol "TPS77701_HTSSOP20_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND/PAD")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "14")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77701_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77701_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Adjustable Output 1.5-5.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS77701_SO8_0_1")
		(symbol "TPS77701_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77715_HTSSOP20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77715_HTSSOP20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 3.81 -5.08 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS77715_HTSSOP20_0_1")
		(symbol "TPS77715_HTSSOP20_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND/PAD")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77715_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77715_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS77715_SO8_0_1")
		(symbol "TPS77715_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77801_HTSSOP20"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS77801_HTSSOP20"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Adjustable Output 1.2-5.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS77801_HTSSOP20_0_1")
		(symbol "TPS77801_HTSSOP20_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "19")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "20")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND/PAD")
				(number "21")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "PG")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77801_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77801_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Adjustable Output 1.2-5.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Adjustable Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS77801_SO8_0_1")
		(symbol "TPS77801_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77815_HTSSOP20"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS77815_HTSSOP20"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS77815_HTSSOP20_0_1")
		(symbol "TPS77815_HTSSOP20_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND/HS")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "19")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "20")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND/HS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND/PAD")
				(number "21")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "PG")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS77815_SO8"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77815_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TPS77815_SO8_0_1")
		(symbol "TPS77815_SO8_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "VOUT")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS78233DDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78233DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS78233DDC_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(symbol "TPS78233DDC_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS79301-EP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79301-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Adjustable Output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS79301-EP_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS79318-EP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79318-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS79318-EP_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "BP")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A20xxxDQN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A20xxxDQN"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a20.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "300 mA Low Dropout Voltage Regulator, Fixed Output, 1.6..6.0Vin, Low-Noise (7μV RMS), 6.5μA IQ LDO, X2SON-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Texas-Instruments"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*X2SON*1x1mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS7A20xxxDQN_0_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
		)
		(symbol "TPS7A20xxxDQN_1_1"
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "Pad")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A3301RGW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS7A3301RGW"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGW0020A_VQFN-20-1EP_5x5mm_P0.65mm_EP3.15x3.15mm_ThermalVias"
			(at 1.27 11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a33.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1A, Low-Noise Lod-Dropout Negative Voltage Regulator, -3..-36V Input, Adjustable -1.18...-33V Output, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo voltage negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGW0020A*"
			(at 0 0 0)
		)
		(symbol "TPS7A3301RGW_0_1")
		(symbol "TPS7A3301RGW_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "15")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "16")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "13")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NR/SS")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A39"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "TPS7A39"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10_ThermalVias"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a39.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "Dual, 150-mA, ±3.3V to ±33V Input, +1.2V to +30V and -30V to 0V Output, Wide VIN Positive and Negative LDO Voltage Regulator, 3x3mm WSON-10 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO Regulator Adj Positive Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PVSON*"
			(at 0 0 0)
		)
		(symbol "TPS7A39_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INP")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NR/SS")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "INN")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTP")
				(number "10")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "FBP")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "BUF")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "FBN")
				(number "7")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUTN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A4101DGN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 -6.35 0)
		)
		(property "Value" "TPS7A4101DGN"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:Texas_DGN0008B_VSSOP-8-1EP_3x3mm_P0.65mm_EP2x3mm_Mask1.88x1.98mm_ThermalVias"
			(at 7.62 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a4101.pdf"
			(at 7.62 -13.97 0)
		)
		(property "Description" "High voltage low-dropout linear regulator, 7V to 50 VIn, 1.175V to 48V output, 50mA, MSOP-8-EP"
			(at 7.62 -19.05 0)
		)
		(property "ki_keywords" "LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DGN0008B*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS7A4101DGN_0_1")
		(symbol "TPS7A4101DGN_1_0"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
		)
		(symbol "TPS7A4101DGN_1_1"
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A4701xRGW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 19.05 0)
		)
		(property "Value" "TPS7A4701xRGW"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGW0020A_VQFN-20-1EP_5x5mm_P0.65mm_EP3.15x3.15mm_ThermalVias"
			(at 4.445 21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a47.pdf"
			(at 0 24.13 0)
		)
		(property "Description" "1A, Low-Noise Low-Dropout Voltage Regulator, 3-35V Input, Adjustable 1.4-34V Output, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo voltage noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGW0020A*"
			(at 0 0 0)
		)
		(symbol "TPS7A4701xRGW_0_1")
		(symbol "TPS7A4701xRGW_1_1"
			(pin power_in line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN")
				(number "15")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "16")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "EN")
				(number "13")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "0.1V")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "0.2V")
				(number "11")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "0.4V")
				(number "10")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "0.8V")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "1.6V")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "3.2V")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "6.4V")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "6.4V")
				(number "4")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_out line
				(at 10.16 15.24 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SENSE/FB")
				(number "3")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "NR")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A7001DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS7A7001DDA"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:TI_SO-PowerPAD-8"
			(at -1.27 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps7a7001.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, Low-Dropout Voltage Regulator, 1.425-6.5V Input, Adjustable Min 0.5V Output, PowerPad SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo regulator voltage linear"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TI*SO*PowerPAD*"
			(at 0 0 0)
		)
		(symbol "TPS7A7001DDA_0_1")
		(symbol "TPS7A7001DDA_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "FB")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A7200RGW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TPS7A7200RGW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGW0020A_VQFN-20-1EP_5x5mm_P0.65mm_EP3.15x3.15mm_ThermalVias"
			(at 1.27 19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps7a7200.pdf"
			(at -3.81 12.7 0)
		)
		(property "Description" "2A, Low-Dropout Voltage Regulator, 1.5-6.5V Input, Adjustable 0.9-5V Output, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGW0020A*"
			(at 0 0 0)
		)
		(symbol "TPS7A7200RGW_0_1")
		(symbol "TPS7A7200RGW_1_1"
			(pin power_in line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IN")
				(number "15")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "16")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "17")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SS")
				(number "13")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "50mV")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "100mV")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "200mV")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "400mV")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "800mV")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "1.6V")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "19")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "20")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SNS")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS7A91"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TPS7A91"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PDSO-N10_EP1.2x2mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps7a91.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "1A, High-Accuracy, Low-Noise LDO Voltage Regulator, Texas S-PDSO-N10"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PDSO*"
			(at 0 0 0)
		)
		(symbol "TPS7A91_0_1")
		(symbol "TPS7A91_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "10")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN")
				(number "9")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS_CTRL")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NR/SS")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UA78M05QDCYRQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.81 0)
		)
		(property "Value" "UA78M05QDCYRQ1"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/UA78M-Q1"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 25V Linear Regulator, Fixed Output 5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Q100 0.5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "UA78M05QDCYRQ1_0_1")
		(symbol "UA78M05QDCYRQ1_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6220B331MR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "XC6220B331MR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6220/XC6220.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "1A, Low Drop-out Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 1A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "XC6220B331MR_0_1")
		(symbol "XC6220B331MR_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "CE")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "VOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "uA7805"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7805"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
		(symbol "uA7805_0_1")
		(symbol "uA7805_1_1"
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADP7142ARDZ-1.8"
		(extends "ADP7142ARDZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142ARDZ-1.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 1.8V Fixed Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142ARDZ-2.5"
		(extends "ADP7142ARDZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142ARDZ-2.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 2.5V Fixed Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142ARDZ-3.3"
		(extends "ADP7142ARDZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142ARDZ-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 3.3V Fixed Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142ARDZ-5.0"
		(extends "ADP7142ARDZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142ARDZ-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 5.0V Fixed Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142AUJZ-1.8"
		(extends "ADP7142AUJZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142AUJZ-1.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 1.8V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142AUJZ-2.5"
		(extends "ADP7142AUJZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142AUJZ-2.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 2.5V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142AUJZ-3.3"
		(extends "ADP7142AUJZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142AUJZ-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 3.3V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7142AUJZ-5.0"
		(extends "ADP7142AUJZ")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "ADP7142AUJZ-5.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, 5.0V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7182AUJZ-2.5"
		(extends "ADP7182AUJZ-1.8")
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "ADP7182AUJZ-2.5"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7182.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Negative, -2.5V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7182AUJZ-3.3"
		(extends "ADP7182AUJZ-1.8")
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "ADP7182AUJZ-3.3"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7182.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Negative, -3.3V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADP7182AUJZ-5.0"
		(extends "ADP7182AUJZ-1.8")
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "ADP7182AUJZ-5.0"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7182.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Negative, -5.0V Fixed Output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, adjustable output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-1.5"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-1.8"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-2.5"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-2.85"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.85V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-3.3"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117-5.0"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 5.0V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CD-1.8"
		(extends "AMS1117CD-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CD-2.5"
		(extends "AMS1117CD-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.5V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CD-2.85"
		(extends "AMS1117CD-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.85V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CD-3.3"
		(extends "AMS1117CD-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CD-5.0"
		(extends "AMS1117CD-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CD-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 5.0V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CS-1.8"
		(extends "AMS1117CS-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CS-2.5"
		(extends "AMS1117CS-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.5V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CS-2.85"
		(extends "AMS1117CS-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.85V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CS-3.3"
		(extends "AMS1117CS-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AMS1117CS-5.0"
		(extends "AMS1117CS-1.5")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AMS1117CS-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 5.0V fixed output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP1117-18"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-18"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AP1117-25"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-25"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AP1117-33"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-33"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AP1117-50"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP1117-50"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.diodes.com/datasheets/AP1117.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 5.0V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-15Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-15Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 1.5V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-18Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-18Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 1.8V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-20Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-20Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 2.0V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-25Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-25Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 2.5V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-28Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-28Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 2.8V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-30Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-30Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 3.0V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-33Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-33Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 3.3V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP130-35Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP130-35Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP130.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "0.3A Low Dropout regulator, positive, 3.5V fixed output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*3*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-18"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-18"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 1.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-20"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-25"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-25"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-28"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-28"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-29"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-29"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.9V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-30"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-30"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 3.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-33"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-33"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP131-35"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "AP131-35"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/AP131.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 3.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2112K-1.2"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2112K-1.2"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 2.5V-6V input voltage range, 1.2V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2112K-1.8"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2112K-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 2.5V-6V input voltage range, 1.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2112K-2.5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2112K-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 3V-6V input voltage range, 2.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2112K-2.6"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2112K-2.6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 3.1V-6V input voltage range, 2.6V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2112K-3.3"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2112K-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-1.0"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-1.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-1.2"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-1.2"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.2V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-1.5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-1.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-1.8"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-2.5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 2.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-2.8"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-2.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 2.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-3.0"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-3.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-3.3"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-4.2"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-4.2"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 4.2V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-4.75"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-4.75"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 4.75V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127K-ADJ"
		(extends "AP2204K-ADJ")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2127K-ADJ"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA low dropout adjustable linear regulator, shutdown pin, 2.5V-6V input voltage, SOT-23-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-1.0"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-1.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.0V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-1.2"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-1.2"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.2V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-1.5"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.5V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-1.8"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.8V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-2.5"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 2.5V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-2.8"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-2.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 2.8V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-3.0"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-3.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.0V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N-3.3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.3V fixed positive output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127N3-1.5"
		(extends "AP2127N3-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127N3-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 1.5V fixed positive output, SOT-23-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP2127R-3.3"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP2127R-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2127.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.3V fixed positive output, SOT-89 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-1.8"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-1.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 1.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-2.5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 2.5V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-2.8"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-2.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 2.8V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-3.0"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-3.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-3.3"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204K-5.0"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -5.08 5.715 0)
		)
		(property "Value" "AP2204K-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2204.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 5.0V fixed positive output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-1.8"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 1.8V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-2.5"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 2.5V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-2.8"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-2.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 2.8V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-3.0"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-3.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.0V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-3.3"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 3.3V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204R-5.0"
		(extends "AP2204R-1.5")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204R-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 5.0V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204RA-5.0"
		(extends "AP2204RA-3.3")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204RA-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 5.0V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP2204RB-5.0"
		(extends "AP2204RB-3.3")
		(property "Reference" "U"
			(at -5.08 3.175 0)
		)
		(property "Value" "AP2204RB-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AP2204.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, wide input voltage range, 5.0V fixed positive output, SOT-89-3 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-10E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-10E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.0V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-12E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-12E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.2V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-15E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-15E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-18E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-18E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-25E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-25E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-28E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-28E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 2.8V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7361C-33E"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7361C-33E"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7361C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-15FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-15FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Low-Dropout Linear Regulator, 1.5V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-18FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-18FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Low-Dropout Linear Regulator, 1.8V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-28FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-28FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "350mA Low-Dropout Linear Regulator, 2.8V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-30FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-30FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "350mA Low-Dropout Linear Regulator, 3.0V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-33FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-33FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "350mA Low-Dropout Linear Regulator, 3.3V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-36FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-36FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "350mA Low-Dropout Linear Regulator, 3.6V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7370-50FDC"
		(extends "AP7370-12FDC")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7370-50FDC"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1.01x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7370.pdf"
			(at 0 0 0)
		)
		(property "Description" "350mA Low-Dropout Linear Regulator, 5.0V fixed output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AP7381-33SA-7"
		(extends "AP7381-28SA-7")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7381-33SA-7"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7381.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "Diodes ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7381-50SA-7"
		(extends "AP7381-28SA-7")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7381-50SA-7"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7381.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 5.0V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "Diodes ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7381-70SA-7"
		(extends "AP7381-28SA-7")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7381-70SA-7"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7381.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 7.0V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "Diodes ldo nrnd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-28SA"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-28SA"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 2.8V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-28V"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-28V"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline_Wide"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 2.8V, Wide Input Voltage Range 40V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-28Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-28Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 2.8V, Wide Input Voltage Range 40V, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89?3*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-33SA"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-33SA"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 3.3V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-33V"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-33V"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline_Wide"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 3.3V, Wide Input Voltage Range 40V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-33Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-33Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 3.3V, Wide Input Voltage Range 40V, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89?3*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-50SA"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-50SA"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 5V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-50V"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-50V"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline_Wide"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 5V, Wide Input Voltage Range 40V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-50Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-50Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 5V, Wide Input Voltage Range 40V, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89?3*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-70SA"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-70SA"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 7V, Wide Input Voltage Range 40V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-70V"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-70V"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline_Wide"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 7V, Wide Input Voltage Range 40V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "AP7384-70Y"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AP7384-70Y"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP7384.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Low Dropout Voltage Regulator, Fixed Output 7V, Wide Input Voltage Range 40V, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "50mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89?3*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-15-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-15-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-16-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-16-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-17-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-17-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-18-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-18-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-19-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-19-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-20-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-20-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-21-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-21-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-22-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-22-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-23-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-23-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-24-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-24-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-25-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-25-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-26-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-26-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-27-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-27-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-28-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-28-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-29-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-29-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-30-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-30-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-31-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-31-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-32-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-32-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865N-33-HF-3"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865N-33-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-15-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-15-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-16-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-16-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-17-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-17-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-18-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-18-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-19-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-19-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-20-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-20-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-21-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-21-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-22-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-22-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-23-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-23-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-24-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-24-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-25-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-25-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-26-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-26-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-27-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-27-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-28-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-28-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-29-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-29-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-30-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-30-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-31-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-31-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-32-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-32-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NL-33-HF-3"
		(extends "APE8865NL-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NL-33-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-15-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-15-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-16-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-16-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-17-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-17-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-18-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-18-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-19-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-19-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-20-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-20-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-21-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-21-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-22-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-22-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-23-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-23-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-24-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-24-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-25-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-25-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-26-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-26-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-27-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-27-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-28-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-28-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-29-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-29-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-30-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-30-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-31-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-31-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-32-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-32-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865NR-33-HF-3"
		(extends "APE8865NR-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "APE8865NR-33-HF-3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-15-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-15-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-16-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-16-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-17-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-17-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-18-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-18-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-19-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-19-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-20-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-20-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-21-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-21-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-22-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-22-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-23-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-23-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-24-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-24-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-25-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-25-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-26-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-26-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-27-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-27-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-28-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-28-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-29-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-29-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-30-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-30-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-31-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-31-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-32-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-32-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U4-33-HF-3"
		(extends "APE8865U4-12-HF-3")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "APE8865U4-33-HF-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-343_SC-70-4"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SC-70-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-15-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-15-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-16-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-16-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-17-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-17-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-18-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-18-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-19-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-19-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-20-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-20-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-21-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-21-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-22-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-22-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-23-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-23-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-24-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-24-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-25-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-25-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-26-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-26-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-27-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-27-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-28-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-28-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-29-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-29-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-30-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-30-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-31-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-31-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-32-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-32-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865U5-33-HF-3"
		(extends "APE8865U5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865U5-33-HF-3"
			(at -3.175 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-15-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-15-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-16-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-16-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.6V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-17-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-17-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-18-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-18-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-19-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-19-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-20-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-20-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-21-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-21-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-22-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-22-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-23-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-23-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-24-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-24-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.4V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-25-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-25-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-26-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-26-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-27-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-27-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-28-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-28-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-29-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-29-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-30-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-30-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-31-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-31-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-32-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-32-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "APE8865Y5-33-HF-3"
		(extends "APE8865Y5-12-HF-3")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "APE8865Y5-33-HF-3"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.tme.eu/fr/Document/ced3461ed31ea70a3c416fb648e0cde7/APE8865-3.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-1.5"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-1.8"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-2.5"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-2.85"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-3.3"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1084-5.0"
		(extends "AZ1084-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1084-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 12V Fixed LDO Linear Regulator, 1.5V, TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-1.5"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-1.5"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 1.5V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-1.8"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 1.8V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-2.5"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 2.5V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-2.85"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 2.85V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-3.3"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117-5.0"
		(extends "AZ1117-1.2")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 5.0V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117D-ADJ"
		(extends "LM317_TO-252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117D-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117H-ADJ"
		(extends "LM317_SOT-223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117H-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117R-ADJ"
		(extends "LM317L_SOT-89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117R-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117S-ADJ"
		(extends "LM317_TO-263")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117S-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "AZ1117T-ADJ"
		(extends "LM317_TO-220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "AZ1117T-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/AZ1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A 20V Adjustable LDO Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BD15GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD15GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 1.5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD18GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD18GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 1.8V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD18GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD18GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 1.8V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD25GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD25GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 2.5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD25GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD25GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 2.5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD30GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD30GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 3V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD30GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD30GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 3V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD33FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD33FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 3.3V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD33FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD33FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 3.3V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD33GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD33GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 3.3V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD33GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD33GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 3.3V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD50FC0FP"
		(extends "BD33FC0FP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD50FC0FP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 5.0V LDO regulator with OVP & TSP, without enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD50FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD50FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 5.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD50FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD50FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 5.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD50GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD50GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD50GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD50GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 5V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD60FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD60FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 6.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD60FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD60FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 6.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD60GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD60GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 6V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD60GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD60GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 6V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD70FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD70FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 7.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD70FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD70FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 7.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD70GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD70GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 7V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD70GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD70GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 7V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD80FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD80FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 8.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD80FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD80FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 8.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD80GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD80GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 8V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD80GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD80GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 8V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD90FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD90FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 9.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD90FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BD90FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 9.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BD90GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD90GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 9V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BD90GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD90GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 9V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ0FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ0FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 10.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ0FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ0FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 10.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ0GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BDJ0GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 10V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ0GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BDJ0GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 10V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ2FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ2FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 12.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ2FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ2FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 12.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ2GA3WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BDJ2GA3WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga3wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "300mA, 12V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ2GA5WEFJ"
		(extends "BD15GA5WEFJ")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BDJ2GA5WEFJ"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxga5wefj-e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "500mA, 12V LDO regulator with OVP & TSP, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ5FC0WEFJ"
		(extends "BD30FC0WEFJ")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ5FC0WEFJ"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at -1.27 10.16 0)
		)
		(property "Description" "1A, 15.0V LDO regulator with OVP & TSP, with enable, HTSOP-J8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BDJ5FC0WFP"
		(extends "BD30FC0WFP")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "BDJ5FC0WFP"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-4"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/linear_regulator/bdxxfc0wefj-e.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "1A, 15.0V LDO regulator with OVP & TSP, with enable, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator fixed positive over voltage protection thermal shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IFX27001TFV18"
		(extends "IFX27001TFV15")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV18"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, 1.8V fixed output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IFX27001TFV26"
		(extends "IFX27001TFV15")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV26"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, 2.6V fixed output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IFX27001TFV33"
		(extends "IFX27001TFV15")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV33"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, 3.3V fixed output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IFX27001TFV50"
		(extends "IFX27001TFV15")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "IFX27001TFV50"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/dc75757ae45a88e5f69bdce3f2a651a5fe0ca07d/ifx27001_ds_10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "1A Low Dropout Regulator, positive, 5.0V fixed output, TO-252-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO positive voltage industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "KA378R12C"
		(extends "KA378R05")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "KA378R12C"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/KA378R12CTU-D.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Positive 3A 35V Linear Regulator with Disable Pin, LDO, Fixed Output 12V, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive LDO Disable Pin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "KA378R33"
		(extends "KA378R05")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "KA378R33"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-4_Vertical"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/KA378R33-D.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Positive 3A 35V Linear Regulator with Disable Pin, LDO, Fixed Output 3.3V, TO-220F-4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive LDO Disable Pin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "KA78M05_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "KA78M05_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78M00-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "KF25BDT"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "KF25BDT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/kfxx.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 20V Linear Regulator, Fixed Output 2.5V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "KF33BDT"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "KF33BDT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/kfxx.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 20V Linear Regulator, Fixed Output 3.3V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "KF50BDT"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "KF50BDT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/kfxx.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 20V Linear Regulator, Fixed Output 5V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "KF80BDT"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "KF80BDT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/kfxx.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 20V Linear Regulator, Fixed Output 8V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "L7806"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7806"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 6V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7808"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7808"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 8V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7809"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7809"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 9V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7812"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7812"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 12V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7815"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7815"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 15V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7818"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7818"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 18V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7824"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7824"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 40V Linear Regulator, Fixed Output 24V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L7885"
		(extends "L7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L7885"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 8.5V, TO-220/TO-263/TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "L78L05_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L05_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L05_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L05_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L05_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L05_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L06_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L06_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 6V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L06_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L06_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 6V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L06_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L06_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 6V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L08_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L08_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L08_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L08_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L08_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L08_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L09_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L09_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 9V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L09_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L09_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 9V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L09_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L09_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 9V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L10_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L10_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 10V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L10_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L10_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 10V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L10_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L10_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 10V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L12_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L12_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L12_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L12_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L12_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L12_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L15_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L15_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 15V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L15_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L15_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 15V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L15_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L15_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 15V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L18_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L18_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 18V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L18_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L18_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 18V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L18_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L18_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 18V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L24_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L24_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 24V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L24_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L24_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 24V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L24_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L24_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 24V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L78L33_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L33_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 3.3V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L78L33_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L33_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 3.3V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L78L33_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "L78L33_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 3.3V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L7908"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L7908"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c9/16/86/41/c7/2b/45/f2/CD00000450.pdf/files/CD00000450.pdf/jcr:content/translations/en.CD00000450.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Linear Regulator, Fixed Output -8V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "L7912"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L7912"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c9/16/86/41/c7/2b/45/f2/CD00000450.pdf/files/CD00000450.pdf/jcr:content/translations/en.CD00000450.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Linear Regulator, Fixed Output -12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "L7915"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L7915"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c9/16/86/41/c7/2b/45/f2/CD00000450.pdf/files/CD00000450.pdf/jcr:content/translations/en.CD00000450.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Linear Regulator, Fixed Output -15V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "L79L05_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L05_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L79L05_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L05_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L79L08_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L08_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L79L08_SOT89"
		(extends "L79L05_SOT89")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L08_SOT89"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L79L08_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L08_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L79L12_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L12_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L79L12_SOT89"
		(extends "L79L05_SOT89")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L12_SOT89"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L79L12_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L12_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "L79L15_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L15_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "L79L15_SOT89"
		(extends "L79L05_SOT89")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L15_SOT89"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "L79L15_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "L79L15_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1827870.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 100mA -30V Linear Regulator, Fixed Output -5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LD0186D2T50TR"
		(extends "LD1086D2TTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD0186D2T50TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 5V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086D2M33TR"
		(extends "LD1086D2MTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2M33TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 3.3V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086D2T12TR"
		(extends "LD1086D2TTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2T12TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 12V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086D2T18TR"
		(extends "LD1086D2TTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2T18TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 1.8V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086D2T33TR"
		(extends "LD1086D2TTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086D2T33TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 3.3V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086DT18TR"
		(extends "LD1086DTTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086DT18TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 1.8V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086DT25TR"
		(extends "LD1086DTTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086DT25TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 2.5V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086DT33TR"
		(extends "LD1086DTTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086DT33TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 3.3V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086DT50TR"
		(extends "LD1086DTTR")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086DT50TR"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 5V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252?2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086V18-DG"
		(extends "LD1086V-DG")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086V18-DG"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 1.8V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LD1086V33-DG"
		(extends "LD1086V-DG")
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "LD1086V33-DG"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld1086.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Positive, 1.5A 30V, Linear Regulator, Fixed Output 3.3V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear Regulator 1.5A Fixed Output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LD1117S12TR_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD1117S12TR_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 1.2V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1117S18TR_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD1117S18TR_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 1.8V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1117S25TR_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD1117S25TR_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 2.5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1117S33TR_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD1117S33TR_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD1117S50TR_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD1117S50TR_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 5.0V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M10R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M10R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M125R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M125R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.25V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M12R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M12R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M15R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M15R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M18R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M18R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M25R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M25R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39015M33R"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD39015M33R"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/ld39015.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low quiescent current low noise voltage regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD39150DT25"
		(extends "LD39150DT18")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD39150DT25"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld39150.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1.5A Ultra Low Dropout regulator, positive, 2.5V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD39150DT33"
		(extends "LD39150DT18")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LD39150DT33"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld39150.pdf"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1.5A Ultra Low Dropout regulator, positive, 3.3V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G18R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G18R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.8V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G25R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G25R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.5V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G26R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G26R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.6V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G27R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G27R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.7V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G28R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G28R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.8V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G30R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G30R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.0V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G33R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G33R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985G47R_TSOT23"
		(extends "LD3985G122R_TSOT23")
		(property "Reference" "U"
			(at -4.064 5.588 0)
		)
		(property "Value" "LD3985G47R_TSOT23"
			(at 0 5.588 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 4.7V, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M18R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M18R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M25R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M25R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M26R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M26R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.6V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M27R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M27R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M28R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M28R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M29R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M29R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M30R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M30R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M33R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M33R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LD3985M47R_SOT23"
		(extends "LD3985M122R_SOT23")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LD3985M47R_SOT23"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00003395.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 4.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-10_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-10_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 1.0V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-12_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-12_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 1.2V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-15_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-15_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 1.5V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-18_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-18_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 1.8V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-25_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-25_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 2.5V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-29_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-29_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 2.9V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-30_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-30_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 3.0V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-32_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-32_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 3.2V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130-33_SOT23_SOT353"
		(extends "LDK130-08_SOT23_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130-33_SOT23_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, 3.3V fixed positive output, SOT-23-5/SOT-353-5/SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOT?353* *SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU10R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU10R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 1.0V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU12R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU12R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 1.2V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU15R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU15R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 1.5V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU18R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU18R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 1.8V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU25R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU25R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 2.5V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU29R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU29R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 2.9V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU30R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU30R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 3.0V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU32R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU32R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 3.2V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDK130PU33R_DFN6"
		(extends "LDK130PU08R_DFN6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "LDK130PU33R_DFN6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6_1.3x1.2mm_P0.4mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/29/10/f7/87/2f/66/47/f4/DM00076097.pdf/files/DM00076097.pdf/jcr:content/translations/en.DM00076097.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA low dropout linear regulator, low quiescent current very, low noise, shutdown pin, fixed 3.3V positive output, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive low noise low quienscent current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.3x1.2mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "LF120_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF120_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 12.0V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF120_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF120_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 12.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF15_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF15_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 1.5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF15_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF15_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 1.5V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF18_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF18_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 1.8V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF18_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF18_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 1.8V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF25_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF25_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 2.5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF25_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF25_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 2.5V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF33_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF33_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 3.3V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF33_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF33_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 3.3V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF47_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF47_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 4.7V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF47_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF47_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 4.7V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF50_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF50_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 5.0V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF50_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF50_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 5.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF60_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF60_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 6.0V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF60_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF60_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 6.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF80_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF80_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 8.0V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF80_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF80_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 8.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF85_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF85_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 8.5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF85_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF85_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 8.5V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LF90_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF90_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 9.0V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LF90_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LF90_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 500mA, Fixed Vo 9.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M18TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M18TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M25TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M25TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M33TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M33TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M50TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M50TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 5.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M55TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M55TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 5.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M60TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M60TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 6.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LK112M80TR"
		(extends "LK112M15TR")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LK112M80TR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.st.com/resource/ja/datasheet/lk112.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low noise and low drop voltage regulator with shutdown function, 150mA, Vout = 8.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM1084-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1084-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1084.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A 27V Linear Regulator, Fixed Output 5.0V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1085-12"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1085-12"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1085.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 18V Linear Regulator, Fixed Output 12.0V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1085-3.3"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1085-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1085.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 27V Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1085-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1085-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1085.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 25V Linear Regulator, Fixed Output 5.0V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1085-ADJ"
		(extends "LM1084-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1085-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1085.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 29V Adjustable Linear Regulator, TO-220 / TO-263 (D2-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117DT-1.8"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117DT-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117DT-2.5"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117DT-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.5V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117DT-3.3"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117DT-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117DT-5.0"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117DT-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117DT-ADJ"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117DT-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117LD-2.5"
		(extends "LM1117LD-1.8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117LD-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.5V fixed output, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON?8*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117LD-3.3"
		(extends "LM1117LD-1.8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117LD-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON?8*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117LD-5.0"
		(extends "LM1117LD-1.8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117LD-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON?8*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117MP-1.8"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117MP-1.8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 1.8V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117MP-2.5"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117MP-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.5V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117MP-3.3"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117MP-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117MP-5.0"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117MP-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117MP-ADJ"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117MP-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117S-3.3"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117S-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117S-5.0"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117S-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117S-ADJ"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117S-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117T-2.5"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117T-2.5"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.5V fixed output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117T-3.3"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117T-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117T-5.0"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117T-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM1117T-ADJ"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM1117T-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM117_TO3"
		(extends "LM317_TO3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM117_TO3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "1,5A 35V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1,5A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "LM117_TO39"
		(extends "LM317_TO39")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM117_TO39"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA 35V Adjustable Linear Regulator, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "LM137_TO3"
		(extends "LM337_TO3")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM137_TO3"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "LM150_TO3"
		(extends "LM317_TO3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM150_TO3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm350a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 33V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 3A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "LM2931-3.3_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2931-3.3_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100 mA 60V Linear Low Dropout Regulator, Fixed Output 3.3V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Dropout Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2931-5.0_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2931-5.0_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM2931-5.0_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2931-5.0_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100 mA 60V Linear Low Dropout Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Dropout Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2931AZ-5.0_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2931AZ-5.0_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "100mA Low drop-out regulator, Fixed Output 5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM2936-3.0_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-3.0_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 3.0V fixed output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM2936-3.3"
		(extends "LM2936-3.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 3.3V fixed output, TO-252/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM2936-3.3_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-3.3_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 3.3V fixed output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM2936-5.0"
		(extends "LM2936-3.0")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 5.0V fixed output, TO-252/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252* SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM2936-5.0_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2936-5.0_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2936.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "50mA Ultra-Low Quiescent Current LDO Voltage Regulator, 5.0V fixed output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM2937xMP"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2937xMP"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2937.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "500-mA Low Dropout Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Low Dropuout Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LM2937xS"
		(extends "SPX2920T-3.3_TO263")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2937xS"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2937.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "500-mA Low Dropout Regulator, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Low Dropuout Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LM2937xT"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM2937xT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2937.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "500-mA Low Dropout Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Low Dropuout Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2990SX-12"
		(extends "LM2990SX-5.0")
		(property "Reference" "U"
			(at -7.874 4.064 0)
		)
		(property "Value" "LM2990SX-12"
			(at -3.048 4.064 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2990.pdf"
			(at -31.75 19.05 0)
		)
		(property "Description" "Three termianl low-dropout 1A negative voltage regulator, Input -6V to -26V, Out -12V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin2* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM2990SX-15"
		(extends "LM2990SX-5.0")
		(property "Reference" "U"
			(at -7.874 4.064 0)
		)
		(property "Value" "LM2990SX-15"
			(at -3.048 4.064 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2990.pdf"
			(at -31.75 19.05 0)
		)
		(property "Description" "Three termianl low-dropout 1A negative voltage regulator, Input -6V to -26V, Out -15V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin2* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM341T-05_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM341T-05_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm341.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM341T-12_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM341T-12_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm341.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 12V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM341T-15_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM341T-15_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm341.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 15V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM3480-12"
		(extends "LM3480-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM3480-12"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3480.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA, Quasi Low Dropout Voltage Regulator, 12V positive fixed output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo linear fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM3480-15"
		(extends "LM3480-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM3480-15"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3480.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA, Quasi Low Dropout Voltage Regulator, 15V positive fixed output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo linear fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM3480-5.0"
		(extends "LM3480-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM3480-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm3480.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA, Quasi Low Dropout Voltage Regulator, 5.0V positive fixed output, SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo linear fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM350_TO3"
		(extends "LM317_TO3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM350_TO3"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm350a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A 33V Adjustable Linear Regulator, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 3A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "LM7806_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7806_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 6V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7808_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7808_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 8V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7809_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7809_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 9V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7810_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7810_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 10V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7812_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7812_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 12V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7815_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7815_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 15V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7818_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7818_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 18V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7824_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM7824_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 24V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM78L05_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78L05_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L06A-D.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM78L05_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78L05_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L06A-D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM78L12_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78L12_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L06A-D.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM78L12_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78L12_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L06A-D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM78M05_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LM78M05_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78M00-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7906_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7906_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 6V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7908_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7908_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 8V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7909_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7909_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 9V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7910_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7910_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 10V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7912_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7912_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "hhttps://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 12V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7915_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7915_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 15V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7918_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7918_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 18V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM7924_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM7924_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output 24V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM79L12_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79L12_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-Terminal Negative Regulator, -12V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative regulatpr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM79L15_TO92"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79L15_TO92"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-Terminal Negative Regulator, -15V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative regulatpr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LM79M05_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79M05_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM79M12_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79M12_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output 12V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LM79M15_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LM79M15_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output 15V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-3.0_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-3.0_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 3.0V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-3.0_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-3.0_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 3.0V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-3.3_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-3.3_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 3.3V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-3.3_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-3.3_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 3.3V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-5.0_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-5.0_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 5.0V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "LP2950-5.0_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LP2950-5.0_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 5.0V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-3.3_DIP"
		(extends "LP2951-3.0_DIP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.3_DIP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.3V, LDO, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-3.3_SOIC"
		(extends "LP2951-3.0_SOIC")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.3_SOIC"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.3V, LDO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-3.3_VSSOP"
		(extends "LP2951-3.0_VSSOP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.3_VSSOP"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.3V, LDO, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-3.3_WSON"
		(extends "LP2951-3.0_WSON")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-3.3_WSON"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.2x2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 3.3V, LDO, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-5.0_DIP"
		(extends "LP2951-3.0_DIP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-5.0_DIP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 5.0V, LDO, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-5.0_SOIC"
		(extends "LP2951-3.0_SOIC")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-5.0_SOIC"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 5.0V, LDO, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-5.0_VSSOP"
		(extends "LP2951-3.0_VSSOP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-5.0_VSSOP"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 5.0V, LDO, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2951-5.0_WSON"
		(extends "LP2951-3.0_WSON")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LP2951-5.0_WSON"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x3mm_P0.5mm_EP1.2x2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2951.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micropower Voltage Regulators with Shutdown, 100mA, Fixed Output 5.0V, LDO, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micropower Voltage Regulators with Shutdown"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-10.0"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-10.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 10.0V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-2.5"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 2.5V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-2.8"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-2.8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 2.8V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-2.9"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-2.9"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 2.9V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-3.0"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-3.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 3.0V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-3.1"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-3.1"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 3.1V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-3.3"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 3.3V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2985-5.0"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2985-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2985.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA 16V Low-noise Low-dropout Regulator With Shutdown, 5.0V output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator linear  SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP2987-3.0_SOIC8_VSSOP8"
		(extends "LP2987-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-3.0_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 3.0V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2987-3.0_WSON8"
		(extends "LP2987-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-3.0_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 3.0V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2987-3.3_SOIC8_VSSOP8"
		(extends "LP2987-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-3.3_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 3.3V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2987-3.3_WSON8"
		(extends "LP2987-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2987-3.3_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, MicroPower, Fixed Output 3.3V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-2.8_SOIC8_VSSOP8"
		(extends "LP2988-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-2.8_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 2.8V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-2.8_WSON8"
		(extends "LP2988-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-2.8_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 2.8V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.0_SOIC8_VSSOP8"
		(extends "LP2988-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.0_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.0V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.0_WSON8"
		(extends "LP2988-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.0_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.0V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.3_SOIC8_VSSOP8"
		(extends "LP2988-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.3_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.3V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.3_WSON8"
		(extends "LP2988-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.3_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.3V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.8_SOIC8_VSSOP8"
		(extends "LP2988-5.0_SOIC8_VSSOP8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.8_SOIC8_VSSOP8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" ""
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.8V, SO8/MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP2988-3.8_WSON8"
		(extends "LP2988-5.0_WSON8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP2988-3.8_WSON8"
			(at -1.905 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.2x3mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2987.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Low Noise, MicroPower, Fixed Output 3.8V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 200mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38691SD-2.5"
		(extends "LP38691SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38691SD-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38691.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 2.5V output voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38691SD-3.3"
		(extends "LP38691SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38691SD-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38691.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 3.3V output voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38691SD-5.0"
		(extends "LP38691SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38691SD-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38691.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 5.0V output voltage, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693DT-2.5"
		(extends "LP38693DT-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693DT-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 2.5V output voltage, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693DT-3.3"
		(extends "LP38693DT-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693DT-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 3.3V output voltage, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693DT-5.0"
		(extends "LP38693DT-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693DT-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 5.0V output voltage, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693MP-2.5"
		(extends "LP38693MP-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693MP-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 2.5V output voltage, Enable Pin, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693MP-3.3"
		(extends "LP38693MP-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693MP-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 3.3V output voltage, Enable Pin, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693MP-5.0"
		(extends "LP38693MP-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693MP-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 5.0V output voltage, Enable Pin, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693SD-2.5"
		(extends "LP38693SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693SD-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 2.5V output voltage, Enable Pin, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693SD-3.3"
		(extends "LP38693SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693SD-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 3.3V output voltage, Enable Pin, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP38693SD-5.0"
		(extends "LP38693SD-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP38693SD-5.0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_3x3mm_P0.95mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp38693.pdf"
			(at 0 0 0)
		)
		(property "Description" "500-mA Low-Dropout CMOS Linear Regulators Stable With Ceramic Output Capacitors, 5.0V output voltage, Enable Pin, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x3mm*P0.95mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3963-2.5"
		(extends "LP3963-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3963-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 2.5V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "LP3963-3.3"
		(extends "LP3963-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3963-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 3.3V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "LP3966-2.5"
		(extends "LP3966-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3966-2.5"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 2.5V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "LP3966-3.3"
		(extends "LP3966-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LP3966-3.3"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3966.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A Fast Ultra Low Dropout Linear Regulator, 3.3V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982ILD-2.5"
		(extends "LP3982ILD-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982ILD-2.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack_ThermalVias"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982ILD-3.0"
		(extends "LP3982ILD-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982ILD-3.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack_ThermalVias"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982ILD-3.3"
		(extends "LP3982ILD-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982ILD-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack_ThermalVias"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*3x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982IMM-2.5"
		(extends "LP3982IMM-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMM-2.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982IMM-3.0"
		(extends "LP3982IMM-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMM-3.0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982IMM-3.3"
		(extends "LP3982IMM-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMM-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3982IMMX-2.82"
		(extends "LP3982IMM-1.8")
		(property "Reference" "U"
			(at 7.62 -6.35 0)
		)
		(property "Value" "LP3982IMMX-2.82"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 5.08 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp3982.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.82V, 300mA, Micropower, Ultra-Low-Dropout, Low-Noise CMOS Regulator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP3987H-33B5"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP3987H-33B5"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2004271836_LOWPOWER-LP3987H-33B5F_C517256.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "LowPowerSemi, 600-mA Ultra-Low-Noise Low-IQ LDO, 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output Low-dropout LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP3992-18B5"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP3992-18B5"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304140030_LOWPOWER-LP3992-18B5F_C324569.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "LowPowerSemi, 300-mA Ultra-Low-Noise Low-IQ LDO, 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output Low-dropout  LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-1.5"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-1.5"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 1.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-1.8"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-1.8"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-2.5"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-2.5"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-2.8"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-2.8"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 2.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-2.85"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-2.85"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 2.85V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-2.9"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-2.9"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 2.9V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-3.0"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-3.0"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-3.1"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-3.1"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 3.1V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-3.2"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-3.2"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 3.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-3.3"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-3.3"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5907MFX-4.5"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5907MFX-4.5"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "250-mA Ultra-Low-Noise Low-IQ LDO, 4.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-1.0DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-1.0DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 1.0V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-1.1DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-1.1DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 1.1V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-1.2DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-1.2DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 1.2V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-1.5DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-1.5DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 1.5V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-1.8DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-1.8DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 1.8V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-2.5DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-2.5DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 2.5V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-2.8DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-2.8DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 2.8V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-3.0DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-3.0DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 3.0V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-3.3DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-3.3DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 3.3V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LP5912-5.0DRV"
		(extends "LP5912-0.9DRV")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LP5912-5.0DRV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5912.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "500-mA Ultra-Low-Noise Low-IQ LDO, 5.0V, WSON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1033C"
		(extends "LM337_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LT1033C"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1033fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 3A 35V Adjustable Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 3A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1083-12"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1083-12"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A 25V LDO Linear Regulator, Fixed Output 12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 7.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1083-3.3"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1083-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A 20V LDO Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 7.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1083-3.6"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1083-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A 20V LDO Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 7.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1083-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1083-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A 20V LDO Linear Regulator, Fixed Output 5.V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 7.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1083-ADJ"
		(extends "LM1084-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1083-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/108345fh.pdf"
			(at 0 0 0)
		)
		(property "Description" "7.5A 25V LDO Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Adjustable 7.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1084-12"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1084-12"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0A 25V LDO Linear Regulator, Fixed Output 12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1084-3.3"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1084-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0A 20V LDO Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1084-3.6"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1084-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0A 20V LDO Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1084-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1084-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0A 20V LDO Linear Regulator, Fixed Output 5.V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 5.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1084-ADJ"
		(extends "LM1084-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1084-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/108345fh.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0A 25V LDO Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Adjustable 5.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1085-12"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1085-12"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0A 25V LDO Linear Regulator, Fixed Output 12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 3.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1085-3.3"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1085-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0A 20V LDO Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 3.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1085-3.6"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1085-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0A 20V LDO Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 3.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1085-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1085-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1083ffe.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0A 20V LDO Linear Regulator, Fixed Output 5.V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 3.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1085-ADJ"
		(extends "LM1084-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1085-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/108345fh.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0A 25V LDO Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Adjustable 3.0A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-12"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-12"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 25V LDO Linear Regulator, Fixed Output 12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-2.85"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-2.85"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 18V LDO Linear Regulator, Fixed Output 2.85V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-3.3"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 20V LDO Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-3.6"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 20V LDO Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-5.0"
		(extends "LM1084-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 20V LDO Linear Regulator, Fixed Output 5.V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Fixed 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1086-ADJ"
		(extends "LM1084-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1086-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1086ffs.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A 25V LDO Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator Adjustable 1.5A Positive LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1117-3.3"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1117-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1117fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1117-5.0"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1117-5.0"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1117fd.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1129-3.3_SOT223"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1129-3.3_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "700mA Micropower Low drop-out regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LT1129-5.0_SO8"
		(extends "LT1129-3.3_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-5.0_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, 5.0V output voltage, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1129-5.0_SOT223"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1129-5.0_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "700mA Micropower Low drop-out regulator, Fixed Output 5.0V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LT1129-5.0_TO220_TO263"
		(extends "LT1129-3.3_TO220_TO263")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "LT1129-5.0_TO220_TO263"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/112935ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "700mA Micropower Low Dropout Linear Regulator, 5.0V output voltage, TO-220-5/TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Regulator positive fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*Vertical*StaggerOdd* TO?263*TabPin3*"
			(at 0 0 0)
		)
	)
	(symbol "LT1175-ADJ_SO8_DIP8"
		(extends "LT1175-5_SO8_DIP8")
		(property "Reference" "U"
			(at -5.715 -8.255 0)
		)
		(property "Value" "LT1175-ADJ_SO8_DIP8"
			(at 0 -8.255 0)
		)
		(property "Footprint" ""
			(at 0.635 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 -5.08 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, adjustable output voltage, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1175-ADJ_SOT223"
		(extends "LT1175-5_SOT223")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "LT1175-ADJ_SOT223"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, adjustable output voltage, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "LT1175-ADJ_TO263_TO220"
		(extends "LT1175-5_TO263_TO220")
		(property "Reference" "U"
			(at -5.715 -3.175 0)
		)
		(property "Value" "LT1175-ADJ_TO263_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1175ff.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "500mA Negative Low Dropout Micropower Regulator, adjustable output voltage, TO-220-5/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator LDO negative adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1584-3.38"
		(extends "LT1584-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1584-3.38"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 7A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.38V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 7A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1584-3.45"
		(extends "LT1584-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1584-3.45"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 7A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.45V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 7A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1584-3.6"
		(extends "LT1584-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1584-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 7A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 7A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1584-ADJ"
		(extends "LM350_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1584-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 7A 35V Low Dropout Fast Response Linear Regulator, Adjustable Output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 7A Positive Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "LT1585-3.38"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1585-3.38"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 4.6A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.38V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 4.6A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1585-3.45"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1585-3.45"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 4.6A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.45V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 4.6A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1585-3.6"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1585-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 4.6A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 4.6A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1587-3.3"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1587-3.3"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 3A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.3V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1587-3.45"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1587-3.45"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 3A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.45V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1587-3.6"
		(extends "LT1585-3.3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1587-3.6"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 3A 35V Low Dropout Fast Response Linear Regulator, Fixed Output 3.6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive Fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1587-ADJ"
		(extends "LT1585-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "LT1587-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/158457a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 3A 35V Low Dropout Fast Response Linear Regulator, Adjustable Output, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3A Positive Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-1.2"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-1.2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 1.2V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POWER LDO POSITIVE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-1.5"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-1.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 1.5V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "POWER LDO REGULATOR POSITIVE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-1.8"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-1.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 1.8V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-2"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 2V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-2.5"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-2.5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 2.5V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-2.8"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-2.8"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 2.8V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-3"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 3V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1761-3.3"
		(extends "LT1761-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT1761-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1761sff.pdf"
			(at 0 0 0)
		)
		(property "Description" "MICROPOWER Low Noise 3.3V 100mA LDO regulator, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR POSITIVE POWER LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT1762"
		(extends "LT1962")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1762"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "150mA, Adjustable, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1762-2.5"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1762-2.5"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "2.5V, 150mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1762-3"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1762-3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3V, 150mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1762-3.3"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1762-3.3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.3V, 150mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1762-5"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1762-5"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "5V, 150mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1962-1.5"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-1.5"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.5V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 1.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1962-1.8"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-1.8"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.8V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1962-2.5"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-2.5"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "2.5V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1962-3"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.0V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1962-3.3"
		(extends "LT1962-5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LT1962-3.3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.3V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AEQ"
		(extends "LT1963EQ")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AEQ"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.5A, Adjustable, Low Noise, Linear Voltage Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxQ-1.8"
		(extends "LT1963AxQ-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxQ-1.8"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.8V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxQ-2.5"
		(extends "LT1963AxQ-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxQ-2.5"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "2.5V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxQ-3.3"
		(extends "LT1963AxQ-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxQ-3.3"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.3V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxST-1.8"
		(extends "LT1963AxST-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxST-1.8"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "1.8V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxST-2.5"
		(extends "LT1963AxST-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxST-2.5"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "2.5V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LT1963AxST-3.3"
		(extends "LT1963AxST-1.5")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT1963AxST-3.3"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.3V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "LT3014xDD"
		(extends "LT3010")
		(property "Reference" "U"
			(at -6.985 6.35 0)
		)
		(property "Value" "LT3014xDD"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3014fd.pdf"
			(at 2.54 10.16 0)
		)
		(property "Description" "20mA output, 3V..80Vin, High voltage low-dropout regulator, DFN-8"
			(at 0 12.7 0)
		)
		(property "ki_keywords" "analog analog-devices linear linear-technology linear LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3014xS5"
		(extends "LT1761-SD")
		(property "Reference" "U"
			(at -6.985 6.35 0)
		)
		(property "Value" "LT3014xS5"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3014fd.pdf"
			(at 2.54 10.16 0)
		)
		(property "Description" "20mA output, 3V..80Vin, High voltage low-dropout regulator, SOT-23-5"
			(at 0 12.7 0)
		)
		(property "ki_keywords" "analog analog-devices linear linear-technology linear LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT3015xQ-12"
		(extends "LT3015xQ-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-12"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-12V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT3015xQ-15"
		(extends "LT3015xQ-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-15"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-15V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT3015xQ-3"
		(extends "LT3015xQ-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-3"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-3V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT3015xQ-3.3"
		(extends "LT3015xQ-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-3.3"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-3.3V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT3015xQ-5"
		(extends "LT3015xQ-2.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3015xQ-5"
			(at -3.81 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3015fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "-5V, 1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit, TO-263-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "negative voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "LT3032-12"
		(extends "LT3032-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3032-12"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_DE14MA"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3032ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, Dual Low Dropout Linear Regulator, Positive/Negative Low Noise, 12V Output, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*DE14MA*"
			(at 0 0 0)
		)
	)
	(symbol "LT3032-15"
		(extends "LT3032-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3032-15"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_DE14MA"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3032ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, Dual Low Dropout Linear Regulator, Positive/Negative Low Noise, 15V Output, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*DE14MA*"
			(at 0 0 0)
		)
	)
	(symbol "LT3032-3.3"
		(extends "LT3032-5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LT3032-3.3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:Linear_DE14MA"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3032ff.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, Dual Low Dropout Linear Regulator, Positive/Negative Low Noise, 3.3V Output, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO low noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Linear*DE14MA*"
			(at 0 0 0)
		)
	)
	(symbol "LT3094xDD"
		(extends "LT3093xMSE")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT3094xDD"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3094.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "–20V, 500mA, Ultralow Noise, Ultrahigh PSRR Negative Linear Regulator, -1.8..-20Vin, 0..-19.5Vout, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear negative voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3094xMSE"
		(extends "LT3093xMSE")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LT3094xMSE"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
			(at 0 10.795 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3094.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "-500mA, Adjustable, Ultralow Noise, Ultrahigh PSRR RF Negative Linear Regulator, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear negative voltage regulator low-noise"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1659ESA"
		(extends "MAX1658ESA")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MAX1659ESA"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX1658-MAX1659.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "350mA Linear LDO Regulator, Fixed Output 5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 350mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX38909xTD"
		(extends "MAX38908xTD")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX38909xTD"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX38909.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, High-Performance LDO Linear Regulator, 0.9V-5.5Vin, 0.6V-5Vout, 2.7V-20Vbias, TDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator Maxim Analog Devices"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TDFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5092BATE"
		(extends "MAX5092AATE")
		(property "Reference" "U"
			(at -8.89 15.875 0)
		)
		(property "Value" "MAX5092BATE"
			(at 0 15.875 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 18.415 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5092-MAX5093.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "4V to 72V Input LDOs with Boost Preregulator, 250mA Output, 5V Preset Vout, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage 72V Input LDO Boost Preregulator 250mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5093AATE"
		(extends "MAX5092AATE")
		(property "Reference" "U"
			(at -8.89 15.875 0)
		)
		(property "Value" "MAX5093AATE"
			(at 0 15.875 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 18.415 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5092-MAX5093.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "4V to 72V Input LDOs with Boost Preregulator, 250mA Output, 3.3V Preset Vout, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage 72V Input LDO Boost Preregulator 250mA 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX5093BATE"
		(extends "MAX5092AATE")
		(property "Reference" "U"
			(at -8.89 15.875 0)
		)
		(property "Value" "MAX5093BATE"
			(at 0 15.875 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 18.415 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX5092-MAX5093.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "4V to 72V Input LDOs with Boost Preregulator, 250mA Output, 5V Preset Vout, TQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage 72V Input LDO Boost Preregulator 250mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX604"
		(extends "MAX603")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MAX604"
			(at 0 5.715 0)
		)
		(property "Footprint" ""
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX603-MAX604.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "500mA Linear LDO Regulator, Fixed Output 3.3V, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator 500mA 3.3V fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX882"
		(extends "MAX883")
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "MAX882"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX882-MAX884.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Fixed Output 3.3V or Adjustable with Standby Mode, 0C to +70C, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX884"
		(extends "MAX883")
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "MAX884"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX882-MAX884.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "200mA Linear LDO Regulator, Fixed Output 3.3V or Adjustable with Shutdown Mode, 0C to +70C, DIP-8/SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Linear LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L06_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L06_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 6V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L06_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L06_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 6V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L08_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L08_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L08_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L08_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L08_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L08_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 8V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L12_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L12_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L12_SOT89"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L12_SOT89"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L12_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L12_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 12V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L15_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L15_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 15V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L15_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L15_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78L00A-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 15V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L18_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L18_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/vishay/mc78l00.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 18V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L18_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L18_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/vishay/mc78l00.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 18V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L24_SO8"
		(extends "MC78L05_SO8")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L24_SO8"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 5.08 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/vishay/mc78l00.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 24V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC78L24_TO92"
		(extends "MC78L05_TO92")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78L24_TO92"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/vishay/mc78l00.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 24V, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MC78LC25NTR"
		(extends "MC78LC18NTR")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78LC25NTR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc78lc00-d.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 80mA 12V Linear Regulator, Fixed Output 2.5V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 80mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MC78LC30NTR"
		(extends "MC78LC18NTR")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78LC30NTR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc78lc00-d.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 80mA 12V Linear Regulator, Fixed Output 3V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 80mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MC78LC33NTR"
		(extends "MC78LC18NTR")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78LC33NTR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc78lc00-d.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 80mA 12V Linear Regulator, Fixed Output 3.3V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 80mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MC78LC50NTR"
		(extends "MC78LC18NTR")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78LC50NTR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc78lc00-d.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 12V Linear Regulator, Fixed Output 5V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MC78M05_TO252"
		(extends "LM78M05_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MC78M05_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC78M00-D.PDF"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-252 (D-PAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "MC7905"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7905"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -5V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7905.2"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7905.2"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -5.2V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7906"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7906"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -6V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7908"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7908"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -8V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7912"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7912"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7915"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7915"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -15V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7918"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7918"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 35V Linear Regulator, Fixed Output -18V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC7924"
		(extends "L7905")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC7924"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7900-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 1A 40V Linear Regulator, Fixed Output -24V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "MC79L12_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79L12_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -35V Linear Regulator, Fixed Output -12V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC79L15_SO8"
		(extends "MC79L05_SO8")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79L15_SO8"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm79l.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Negative 100mA -35V Linear Regulator, Fixed Output -15V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M05_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M05_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M08_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M08_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -8V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M08_TO252"
		(extends "MC79M05_TO252")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M08_TO252"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -8V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M12_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M12_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -12V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M12_TO252"
		(extends "MC79M05_TO252")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M12_TO252"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -12V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M15_TO220"
		(extends "LM7905_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M15_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -15V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MC79M15_TO252"
		(extends "MC79M05_TO252")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MC79M15_TO252"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC79M00-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Negative 500mA 35V Linear Regulator, Fixed Output -15V, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 500mA Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-120xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-120xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.2V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-120xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-120xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.2V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-120xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-120xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.2V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-180xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-180xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.8V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-180xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-180xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.8V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-180xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-180xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 1.8V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-250xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-250xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.5V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-250xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-250xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.5V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-250xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-250xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.5V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-280xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-280xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.8V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-280xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-280xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.8V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-280xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-280xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 2.8V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-300xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-300xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.0V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-300xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-300xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.0V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-330xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-330xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.3V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-330xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-330xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.3V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-330xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-330xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 3.3V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-500xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-500xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 5.0V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-500xxTO"
		(extends "LM79L05_TO92")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "MCP1700x-500xxTO"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 5.0V output, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1700x-500xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1700x-500xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA Low Quiscent Current LDO, 5.0V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-120xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-120xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.2V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-120xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-120xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.2V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-120xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-120xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.2V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-150xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-150xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.5V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-150xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-150xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.5V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-150xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-150xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.5V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-180xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-180xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.8V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-180xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-180xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.8V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-180xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-180xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 1.8V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-250xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-250xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.5V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-250xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-250xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.5V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-250xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-250xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.5V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-280xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-280xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.8V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-280xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-280xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.8V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-280xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-280xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 2.8V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-300xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-300xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.0V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-300xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-300xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.0V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-300xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-300xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 3.0V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-400xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-400xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.0V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-400xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-400xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.0V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-400xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-400xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.0V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-500xxDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-500xxDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 5.0V, 250mA, Vin<=16V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-500xxMB"
		(extends "MCP1703Ax-330xxMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-500xxMB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 5.0V, 250mA, Vin<=16V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1703Ax-500xxTT"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1703Ax-500xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 5.0V, 250mA, Vin<=16V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-1202xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-1202xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 1.2V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-1202xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-1202xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 1.2V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-1802xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-1802xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 1.8V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-1802xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-1802xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 1.8V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-2502xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-2502xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 2.5V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-2502xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-2502xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 2.5V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-3002xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-3002xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 3.0V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-3002xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-3002xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 3.0V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-3302xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-3302xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 3.3V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-3302xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-3302xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 3.3V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-5002xMF"
		(extends "MCP1727-0802xMF")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-5002xMF"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 5.0V Output, 330mV Dropout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1727-5002xSN"
		(extends "MCP1727-0802xSN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP1727-5002xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemtest/APID/ProductDocuments/DataSheets/MCP1727-1.5A-Low-Voltage-Low-Quiescent-Current-LDO-Regulator-20001999D.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "1.5A, Low Voltage, Low Quiescent Current LDO Regulator, 2.3 - 6V Input, Fixed 5.0V Output, 330mV Dropout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Low Quiescent Current Fixed LDO Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1754S-1802xCB"
		(extends "MCP1754S-5002xCB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-1802xCB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 1.8V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1754S-1802xMB"
		(extends "MCP1754S-5002xMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-1802xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 1.8V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1754S-3302xCB"
		(extends "MCP1754S-5002xCB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-3302xCB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 3.3V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1754S-3302xMB"
		(extends "MCP1754S-5002xMB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1754S-3302xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002276C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Fixed 150mA Low Dropout Voltage Regulator, Positive, 3.3V output, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Regulator LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-3302xCB"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-3302xCB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA Low Quiscent Current LDO, 4.5-55V input, 3.3V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-3302xDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-3302xDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.5-55V input, 3.3V, 100mA, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-4102xCB"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-4102xCB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA Low Quiscent Current LDO, 4.5-55V input, 4.1V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-4102xDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-4102xDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.5-55V input, 4.1V, 100mA, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-5002xCB"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-5002xCB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA Low Quiscent Current LDO, 4.5-55V input, 5.0V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1792x-5002xDB"
		(extends "MCP1703Ax-330xxDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1792x-5002xDB"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP1792-Family-Data-Sheet-DS20006229D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Quiescent Current LDO Regulator, 4.5-55V input, 5.0V, 100mA, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1799x-330xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1799x-330xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP1799-Data-Sheet-20006248A.pdf"
			(at 0 0 0)
		)
		(property "Description" "80 mA High-Voltage Automotive LDO, 3.3V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1799x-500xxTT"
		(extends "MCP1700x-300xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1799x-500xxTT"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP1799-Data-Sheet-20006248A.pdf"
			(at 0 0 0)
		)
		(property "Description" "80 mA High-Voltage Automotive LDO, 5V output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator linear ldo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1802x-xx02xOT"
		(extends "TC1017-xCT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP1802x-xx02xOT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -6.35 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22053C.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "150mA, Tiny CMOS LDO With Shutdown, Fixed Voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-1802xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-1802xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 1.8V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-2502xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-2502xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 2.5V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-2502xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-2502xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 2.5V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-2502xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-2502xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 2.5V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-2502xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-2502xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 2.5V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3002xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-3002xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.0V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3002xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-3002xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.0V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3002xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-3002xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.0V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3002xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-3002xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.0V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3302xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-3302xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.3V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3302xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-3302xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.3V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3302xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-3302xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.3V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-3302xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-3302xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 3.3V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-5002xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-5002xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 5.0V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-5002xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-5002xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 5.0V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-5002xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-5002xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 5.0V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-5002xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-5002xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 5.0V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-A002xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-A002xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 10.0V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-A002xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-A002xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 10.0V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-A002xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-A002xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 10.0V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-A002xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-A002xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 10.0V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-C002xDB"
		(extends "MCP1804x-1802xDB")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-C002xDB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 12.0V Fixed Output, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-C002xMB"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "MCP1804x-C002xMB"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 12.0V Fixed Output, SOT-89-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-C002xMT"
		(extends "MCP1804x-1802xMT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-C002xMT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 12.0V Fixed Output, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MCP1804x-C002xOT"
		(extends "MCP1804x-1802xOT")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "MCP1804x-C002xOT"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA, 28V LDO Regulator With Shutdown, 12.0V Fixed Output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C10M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C10M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 1.0V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C12M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C12M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 1.2V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C15M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C15M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 1.5V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C18M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C18M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 1.8V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C21M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C21M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "300mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 2.1V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C25M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C25M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "400mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 2.5V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C27M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C27M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "400mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 2.7V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C28M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C28M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "450mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 2.8V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C29M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C29M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "450mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 2.9V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C30M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C30M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "500mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 3.0V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "ME6211C50M5"
		(extends "ME6211C33M5")
		(property "Reference" "U"
			(at -4.572 6.35 0)
		)
		(property "Value" "ME6211C50M5"
			(at 10.16 8.636 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -0.508 -13.462 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0.254 -17.018 0)
		)
		(property "Description" "500mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 5.0V fixed positive output, SOT-23-5"
			(at 1.778 -15.24 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29302AWD"
		(extends "MIC29302WU")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29302AWD"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/20005897B.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, shutdown pin, 3V to 16V input voltage, 1.24V to 15V adjustable output, TO-252"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*252*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29302AWU"
		(extends "MIC29302WU")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29302AWU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/20005897B.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, shutdown pin, 3V to 16V input voltage, 1.24V to 15V adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29302WT"
		(extends "MIC29152WT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29302WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29303WT"
		(extends "MIC29153WT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29303WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29303WU"
		(extends "MIC29153WU")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29303WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A low dropout linear regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "3A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29502WT"
		(extends "MIC29152WT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29502WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29502WU"
		(extends "MIC29302WU")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29502WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A low dropout linear regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29503WT"
		(extends "MIC29153WT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29503WT"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerEven_Lead3.8mm_Vertical"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A low dropout linear regulator, adjustable output, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*220*"
			(at 0 0 0)
		)
	)
	(symbol "MIC29503WU"
		(extends "MIC29153WU")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC29503WU"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-5_TabPin3"
			(at 2.54 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20005685a.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A low dropout linear regulator, adjustable output, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "5A LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-2.5YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-2.5YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 2.5V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-2.7YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-2.7YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 2.7V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-2.85YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-2.85YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 2.85V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-2.8YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-2.8YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 2.8V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-2.9YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-2.9YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 2.9V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.0YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.0YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.1YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.1YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.1V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.2YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.2YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.2V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.3YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.3YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.3V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.6YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.6YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.6V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-3.8YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-3.8YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 3.8V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-4.0YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-4.0YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 4.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5205-5.0YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5205-5.0YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005785A.pdf"
			(at 0 0 0)
		)
		(property "Description" "150mA low dropout linear regulator, fixed 5.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "150mA low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.5YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.5YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.5V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.6YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.6YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.6V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.7YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.7YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.7V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.85YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.85YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.85V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.85YMM"
		(extends "MIC5219-2.5YMM")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.85YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.85V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.8YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.8YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.8V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-2.9YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-2.9YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 2.9V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.0YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.0YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.0YMM"
		(extends "MIC5219-2.5YMM")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.0YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.1YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.1YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.1V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.3YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.3YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.3V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.3YMM"
		(extends "MIC5219-2.5YMM")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.3YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.3V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.6YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.6YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.6V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-3.6YMM"
		(extends "MIC5219-2.5YMM")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-3.6YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 3.6V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-5.0YM5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-5.0YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 5.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219-5.0YMM"
		(extends "MIC5219-2.5YMM")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219-5.0YMM"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, fixed 5.0V output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5219YM5"
		(extends "MIC5205YM5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "MIC5219YM5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC5219-500mA-Peak-Output-LDO-Regulator-DS20006021A.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA low dropout linear regulator, adjustable output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "500mA ultra-low-noise LDO linear voltage regulator adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-1.0xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-1.0xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 1.0V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-1.2xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-1.2xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 1.2V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-1.5xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-1.5xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 1.5V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-1.8xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-1.8xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 1.8V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-2.5xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-2.5xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 2.5V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-2.8xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-2.8xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 2.8V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-3.0xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-3.0xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.0V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5317-3.3xM5"
		(extends "AP2204K-1.5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5317-3.3xM5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/MIC5317-High-Performance-Single-150mA-LDO-DS20006195B.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 6V, SOT23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5353-1.8YMT"
		(extends "MIC5353-2.5YMT")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-1.8YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5353-2.6YMT"
		(extends "MIC5353-2.5YMT")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-2.6YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5353-2.8YMT"
		(extends "MIC5353-2.5YMT")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-2.8YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5353-3.0YMT"
		(extends "MIC5353-2.5YMT")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-3.0YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5353-3.3YMT"
		(extends "MIC5353-2.5YMT")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MIC5353-3.3YMT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm"
			(at 3.81 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf"
			(at 6.35 2.54 0)
		)
		(property "Description" "High-performance, single-output,  ultra-low  LDO regulator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF?6?1EP*1.6x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5355-G4YMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5355-G4YMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 1.8V/1.2V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5355-JGYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5355-JGYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 2.5V/1.8V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5355-SCYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5355-SCYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.0V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5355-SGYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5355-SGYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.8V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-G4YMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-G4YMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 1.8V/1.2V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-JGYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-JGYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 2.5V/1.8V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-MGYML"
		(extends "MIC5356-MMYML")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-MGYML"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-8-1EP_3x3mm_P0.65mm_EP1.55x2.3mm_ThermalVias"
			(at 38.1 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 2.8V/1.8V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA DFN-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-S4YMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-S4YMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.2V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-SCYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-SCYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.0V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5356-SGYMME"
		(extends "MIC5355-S4YMME")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "MIC5356-SGYMME"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias"
			(at 35.56 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Dual 500mA μCap Low Dropout Micropower Linear Regulator, 3.3V/1.8V, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LDO 500mA MSOP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5366-3.3YC5"
		(extends "MIC5365-3.3YC5")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MIC5366-3.3YC5"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic5365.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.3V, Output discharge circuit, Vin up to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*SC*70*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5501-3.0YM5"
		(extends "MIC5504-3.3YM5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5501-3.0YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 3.0V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5504-1.2YM5"
		(extends "MIC5504-3.3YM5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5504-1.2YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 1.2V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5504-1.8YM5"
		(extends "MIC5504-3.3YM5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5504-1.8YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 1.8V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5504-2.5YM5"
		(extends "MIC5504-3.3YM5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5504-2.5YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 2.5V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "MIC5504-2.8YM5"
		(extends "MIC5504-3.3YM5")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC5504-2.8YM5"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 2.8V, Vin up to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Micrel LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-1.5_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-1.5_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 1.5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-1.5_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-1.5_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 1.5V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-1.8_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-1.8_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 1.8V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-1.8_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-1.8_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 1.8V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 18.V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-1.9_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-1.9_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 1.9V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.9V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-12_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-12_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 12V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 12V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.0_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.0_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.0_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.0_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.0V 2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.5_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.5_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2.5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.5_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.5_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2.5V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.85_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.85_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2.85V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.85V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-2.85_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-2.85_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 2.85V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.85V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-3.3_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-3.3_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-3.3_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-3.3_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 3.3V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-5.0_SOT223"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-5.0_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-5.0_TO252"
		(extends "NCP1117-12_TO252")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-5.0_TO252"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 5.0V, TO-252 (DPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5.0V 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "NCP1117-ADJ_SOT223"
		(extends "AP1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NCP1117-ADJ_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 2.54 -6.35 0)
		)
		(property "Description" "1A Low drop-out regulator, Adjustable Output 1.25 - 18.8V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 12V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*TabPin2*"
			(at 0 0 0)
		)
	)
	(symbol "NCP115AMX250TCG"
		(extends "NCP115AMX120TCG")
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "NCP115AMX250TCG"
			(at 10.16 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP115-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "300mA Low-Dropout Linear Regulators, 2.5V output voltage, LDO with low noise and enable pin, XDFN-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*XDFN4*1EP*1.0x1.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS180T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS180T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.8V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS250T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS250T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.5V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS260T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS260T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.6V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS270T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS270T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.7V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS280T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS280T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.8V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS285T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS285T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.85V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS290T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS290T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.9V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS2925T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS2925T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.925V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCS514T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCS514T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 5.14V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT120T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT120T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.2V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT180T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT180T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.8V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT250T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT250T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.5V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT260T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT260T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.6V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT270T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT270T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.7V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT280T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT280T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.8V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT285T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT285T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.85V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT290T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT290T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.9V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT2925T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT2925T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.925V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT300T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT300T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 3.0V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT330T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT330T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 3.3V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163AFCT514T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163AFCT514T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 5.14V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN180T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN180T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.8V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN250T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN250T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.5V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN270T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN270T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.7V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN280T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN280T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.8V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN300T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN300T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 3.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN330T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN330T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 3.3V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN350T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN350T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 3.5V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163ASN500T1G"
		(extends "NCP163ASN150T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCP163ASN500T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 5.0V output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163BFCS180T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163BFCS180T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 1.8V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163BFCS2925T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163BFCS2925T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.925V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163BFCT180T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163BFCT180T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.925V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP163CFCS285T2G"
		(extends "NCP163AFCS120T2G")
		(property "Reference" "U"
			(at 3.81 -6.35 0)
		)
		(property "Value" "NCP163CFCS285T2G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-4_0.64x0.64mm_Layout2x2_P0.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "250mA low-noise LDO, 2.2V-5.5V input, 2.85V output, WLCSP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*0.64x0.64mm*Layout2x2*P0.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCP662SQ18"
		(extends "NCP662SQ15")
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "NCP662SQ18"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-82AB"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP662-D.PDF"
			(at -7.62 20.32 0)
		)
		(property "Description" "100-mA, 12V Max. Input, Ultralow-IQ LDO, 1.8V, SC-82AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?82AB*"
			(at 0 0 0)
		)
	)
	(symbol "NCP662SQ33"
		(extends "NCP662SQ15")
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "NCP662SQ33"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-82AB"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP662-D.PDF"
			(at -7.62 20.32 0)
		)
		(property "Description" "100-mA, 12V Max. Input, Ultralow-IQ LDO, 3.3V, SC-82AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?82AB*"
			(at 0 0 0)
		)
	)
	(symbol "NCP662SQ50"
		(extends "NCP662SQ15")
		(property "Reference" "U"
			(at 0 8.255 0)
		)
		(property "Value" "NCP662SQ50"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-82AB"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP662-D.PDF"
			(at -7.62 20.32 0)
		)
		(property "Description" "100-mA, 12V Max. Input, Ultralow-IQ LDO, 5.0V, SC-82AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?82AB*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN120"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN120"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 1.2V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN150"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN150"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 1.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN180"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN180"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 1.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN250"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN250"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN300"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN300"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN330"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN330"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCP718xSN500"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "NCP718xSN500"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP718-D.PDF"
			(at 0 12.7 0)
		)
		(property "Description" "300-mA, Wide Input Voltage, Low-IQ LDO, 5.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Wide Input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN150T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN150T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.5V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN165T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN165T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.65V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN180T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN180T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.8V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN250T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN250T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 2.5V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN280T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN280T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 2.8V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN300T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN300T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 3.0V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114ASN330T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114ASN330T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 3.3V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN120T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN120T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 1.2V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN150T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN150T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 1.5V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN180T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN180T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 1.8V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN280T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN280T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 2.8V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN300T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN300T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 3.0V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NCV8114BSN330T1G"
		(extends "NCV8114ASN120T1G")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "NCV8114BSN330T1G"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "300mA, Low Noise, Linear Regulator without output active discharge function, 1.7-5.5V input voltage range, 3.3V fixed positive output, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NDP6802SF-33"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NDP6802SF-33"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2401051806_NDP-NDP6802SF-33_C20415512.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 85Vin Linear Regulator, Fixed Output 3.3V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "NDP6802SF-50"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NDP6802SF-50"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2401051806_NDP-NDP6802SF-33_C20415512.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 85Vin Linear Regulator, Fixed Output 5V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "NDP6802SF-A2"
		(extends "MC78L05_SOT89")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "NDP6802SF-A2"
			(at -0.635 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2401051806_NDP-NDP6802SF-33_C20415512.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 100mA 85Vin Linear Regulator, Fixed Output 12V, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 100mA Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "NVC8674DS120"
		(extends "NVC8674DS50")
		(property "Reference" "U"
			(at -5.08 3.81 0)
		)
		(property "Value" "NVC8674DS120"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCV8674-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "350mA, 12.0V Very Low Iq Low Dropout Linear Regulator, TO-263-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "ldo regulator 12V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*263*"
			(at 0 0 0)
		)
	)
	(symbol "OM1323_TO220"
		(extends "LM337_TO220")
		(property "Reference" "U"
			(at -3.81 -3.175 0)
		)
		(property "Value" "OM1323_TO220"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/hirel/om1323.pdf"
			(at 0 0 0)
		)
		(property "Description" "Negative 1.5A 35V Adjustable Linear Regulator, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adjustable Voltage Regulator 1.5A Negative"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "SPX2920M3-5.0_SOT223"
		(extends "SPX2920M3-3.3_SOT223")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920M3-5.0_SOT223"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 5V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "SPX2920S-5.0_SO8"
		(extends "SPX2920S-3.3_SO8")
		(property "Reference" "U"
			(at -6.35 3.81 0)
		)
		(property "Value" "SPX2920S-5.0_SO8"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 6.35 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "400mA Fixed/Adjustable 1.2-20V Low Drop-out Voltage Regulator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 400mA 5V Adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SPX2920T-5.0_TO263"
		(extends "SPX2920T-3.3_TO263")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920T-5.0_TO263"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-3_TabPin2"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 5V, TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "SPX2920U-3.3_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920U-3.3_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 3.3V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "SPX2920U-5.0_TO220"
		(extends "LM7805_TO220")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "SPX2920U-5.0_TO220"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.zlgmcu.com/Sipex/LDO/PDF/spx2920.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "400mA Low drop-out regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L"
		(extends "MIC5205YM5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Adjustable, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO ADJ"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-1-2"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-1-2"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.2V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-1-5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-1-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-1-8"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-1-8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 1.8V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-2-5"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-2-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 2.5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-3-0"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-3-0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-3-3"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-3-3"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 3.3V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SPX3819M5-L-5-0"
		(extends "AP131-15")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "SPX3819M5-L-5-0"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 5.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "REGULATOR LDO 5.0V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1015-xCT"
		(extends "TC1014-xCT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1015-xCT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/21335e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "100 mA CMOS LDOs with Shutdown and Reference Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1055"
		(extends "TC1054")
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TC1055"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 6.985 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21350E.pdf"
			(at -7.62 5.08 0)
		)
		(property "Description" "100mA Low Dropout Regulator with ERROR output in 5-Pin SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1185-xCT"
		(extends "TC1014-xCT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1185-xCT"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/21335e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "150 mA CMOS LDOs with Shutdown and Reference Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1186"
		(extends "TC1054")
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TC1186"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 6.985 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21350E.pdf"
			(at -7.62 5.08 0)
		)
		(property "Description" "150mA Low Dropout Regulator with ERROR output in 5-Pin SOT-23 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1262-25"
		(extends "TC1262-33")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TC1262-25"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA Low Dropout CMOS Voltage Regulator, Fixed Output 2.5V, TO-220/SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 2.5V 500mA Positive CMOS LDO Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "TC1262-28"
		(extends "TC1262-33")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TC1262-28"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA Low Dropout CMOS Voltage Regulator, Fixed Output 2.8V, TO-220/SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 2.8V 500mA Positive CMOS LDO Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "TC1262-30"
		(extends "TC1262-33")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TC1262-30"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA Low Dropout CMOS Voltage Regulator, Fixed Output 3.0V, TO-220/SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 3.0V 500mA Positive CMOS LDO Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "TC1262-50"
		(extends "TC1262-33")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TC1262-50"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "500mA Low Dropout CMOS Voltage Regulator, Fixed Output 5.0V, TO-220/SOT-223/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 5.0V 500mA Positive CMOS LDO Microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?220* TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-1.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-1.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 1.8V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-2.5VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-2.5VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.5V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-2.6VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-2.6VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.6V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.6V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-2.7VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-2.7VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.7V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-2.85VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-2.85VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.85V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.85V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-2.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-2.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.8V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.8V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-3.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-3.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.0V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-3.3VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-3.3VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.3V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2014-5.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2014-5.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 5.0V 50mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-1.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-1.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 1.8V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-2.5VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-2.5VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.5V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-2.6VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-2.6VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.6V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.6V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-2.7VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-2.7VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.7V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-2.85VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-2.85VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.85V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.85V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-2.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-2.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.8V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.8V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-3.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-3.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.0V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-3.3VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-3.3VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.3V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2015-5.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2015-5.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0V 100mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 5.0V 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-1.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-1.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.8V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 1.8V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-2.5VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-2.5VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.5V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.5V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-2.6VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-2.6VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.6V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.6V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-2.7VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-2.7VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.7V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.7V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-2.85VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-2.85VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.85V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.85V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-2.8VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-2.8VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2.8V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 2.8V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-3.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-3.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.0V 50mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.0V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-3.3VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-3.3VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 3.3V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC2185-5.0VxCTTR"
		(extends "LP2985-1.8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TC2185-5.0VxCTTR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21662F.pdf"
			(at 0 0 0)
		)
		(property "Description" "5.0V 150mA CMOS LDO with Shutdown and Vref Bypass, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low dropout 5.0V 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE10"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE10"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.0V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE105"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE105"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.05V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE115"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE115"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.15V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE12"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE12"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.2V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE125"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE125"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.25V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE13"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE13"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.3V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE135"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE135"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.35V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE14"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE14"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.4V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE145"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE145"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.45V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE15"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE15"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.5V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE17"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE17"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.7V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE18"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE18"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.8V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE185"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE185"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.85V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE19"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE19"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 1.9V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE20"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE20"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 2.0V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE24"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE24"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 2.4V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE25"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE25"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 2.5V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE27"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE27"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 2.7V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TCR2EE275"
		(extends "TCR2EE11")
		(property "Reference" "U6"
			(at 0 9.3218 0)
		)
		(property "Value" "TCR2EE275"
			(at 0 7.0104 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13794&prodName=TCR2EF45"
			(at -6.35 6.35 0)
		)
		(property "Description" "200mA Low-dropout Voltage Regulator, Vout 2.75V, Vin up to 5.5V, SOT-553"
			(at 0 0 0)
		)
		(property "ki_keywords" "TOSHIBA LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?553*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-15"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-15"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 1.5V fixed output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-18"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-18"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-25"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-25"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 2.5V fixed output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-33"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-33"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-50"
		(extends "LT1117-2.85")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-50"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 5.0V fixed output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo fixed positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV1117-ADJ"
		(extends "LT1117-ADJ")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TLV1117-ADJ"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv1117.pdf"
			(at 0 0 0)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, adjustable output, TO-220/TO-252/TO-263/SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear regulator ldo adjustable positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223* TO?263* TO?252* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70013_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70013_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70015_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70015_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70015_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70015_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5/SC-70-5/SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70015_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70015_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70018_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70018_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70018_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70018_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70018_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70018_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70019_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70019_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70025_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70025_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70025_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70025_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70025_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70025_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70028_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70028_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70028_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70028_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70029_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70029_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 2.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70030_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70030_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70030_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70030_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3V, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70030_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70030_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70031_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70031_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.1V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70032_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70032_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70033_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70033_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70033_SOT353"
		(extends "TLV70012_SOT353")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70033_SOT353"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70033_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70033_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70036_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70036_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.6V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70036_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70036_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv700.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA Low Dropout Voltage Regulator, Fixed Output 3.6V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "200mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70212_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70212_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70215_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70215_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70218_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70218_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70225_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70225_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70225_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70225_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70228_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70228_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70228_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70228_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70229_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70229_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 2.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70230_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70230_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70231_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70231_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70233_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70233_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70233_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70233_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70235_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70235_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70236_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70236_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.6V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70237_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70237_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70237_WSON6"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70237_WSON6"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 3.7V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70242PDSE"
		(extends "TLV70012_WSON6")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70242PDSE"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 4.2V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*"
			(at 0 0 0)
		)
	)
	(symbol "TLV70245_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV70245_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 4.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV702475_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV702475_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv702.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 4.75V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7113318DDSE"
		(extends "TLV71x_WSON-6")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TLV7113318DDSE"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv711.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Dual, 200mA, Low-Iq Low-Dropout Regulator for Portable Devices, SON-6"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "dual LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON*1.5x1.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV7113333DDSE"
		(extends "TLV71x_WSON-6")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TLV7113333DDSE"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv711.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "Dual, 200mA, Low-Iq Low-Dropout Regulator for Portable Devices, SON-6"
			(at 0 -20.32 0)
		)
		(property "ki_keywords" "dual LDO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WSON*1.5x1.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71209_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71209_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv712.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 0.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71210_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71210_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv712.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71211_SOT23-5"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71211_SOT23-5"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv712.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "300mA Low Dropout Voltage Regulator, Fixed Output 1.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71310PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71310PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71311PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71311PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71312PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71312PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71315PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71315PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV713185PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV713185PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71318PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71318PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71325PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71325PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV713285PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV713285PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.85V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71328PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71328PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71330PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71330PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV71333PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV71333PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv713p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "150mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73310PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73310PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73311PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73311PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 1.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73312PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73312PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73315PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73315PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73318PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73318PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73325PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73325PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV733285PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV733285PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 2.85V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73328PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73328PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73330PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73330PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV73333PDBV"
		(extends "LD39015M08R")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV73333PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv733p.pdf"
			(at 0 0 0)
		)
		(property "Description" "300mA Capacitor-Free Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "300mA LDO Regulator Fixed Positive Capacitor-Free"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75509PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75509PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 0.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75510PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75510PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75510PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75510PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.0V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75512PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75512PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75512PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75512PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.2V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75515PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75515PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75515PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75515PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75518PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75518PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75518PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75518PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75519PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75519PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75519PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75519PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 1.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75525PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75525PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75525PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75525PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75528PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75528PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75528PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75528PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75529PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75529PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75529PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75529PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 2.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75530PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75530PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75530PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75530PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 3.0V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75533PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75533PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75533PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75533PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv755p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "500mA Low Dropout Voltage Regulator, Fixed Output 3.3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75709PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75709PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 0.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75709PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75709PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 0.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75710PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75710PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75710PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75710PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.0V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75712PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75712PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75712PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75712PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.2V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75715PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75715PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75715PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75715PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75718PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75718PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75718PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75718PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75719PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75719PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75719PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75719PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 1.9V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75725PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75725PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75725PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75725PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 2.5V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75728PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75728PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75728PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75728PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 2.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75729PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75729PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 2.9V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75730PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75730PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75730PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75730PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 3.0V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75733PDBV"
		(extends "TLV70012_SOT23-5")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75733PDBV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75733PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75733PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 3.3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV75740PDRV"
		(extends "TLV75509PDRV")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TLV75740PDRV"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv757p.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "1A Low IQ Small Size Low Dropout Voltage Regulator, Fixed Output 4.0V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76133DCY"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TLV76133DCY"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv761.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "3.3V, 1A, Low Noise, High-PSRR LDO Regulator, 2.5V...16V input, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage fixed low-dropout"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76150DCY"
		(extends "AP1117-15")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TLV76150DCY"
			(at -1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv761.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "5.0V, 1A, Low Noise, High-PSRR LDO Regulator, 2.5V...16V input, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltage fixed low-dropout"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76708DRVx"
		(extends "TLV76750DRVx")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76708DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A Precision Linear Voltage Regulator, with enable pin, Fixed Output 0.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76718DRVx"
		(extends "TLV76750DRVx")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76718DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A Precision Linear Voltage Regulator, with enable pin, Fixed Output 1.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76728DRVx"
		(extends "TLV76750DRVx")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76728DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A Precision Linear Voltage Regulator, with enable pin, Fixed Output 2.8V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76733DRVx"
		(extends "TLV76750DRVx")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76733DRVx"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767"
			(at -1.27 0 0)
		)
		(property "Description" "1A Precision Linear Voltage Regulator, with enable pin, Fixed Output 3.3V, WSON6"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.65*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76750QWDRBxQ1"
		(extends "TLV76733QWDRBxQ1")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76750QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 5.0V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76760QWDRBxQ1"
		(extends "TLV76733QWDRBxQ1")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76760QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 6.0V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76780QWDRBxQ1"
		(extends "TLV76733QWDRBxQ1")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76780QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 8.0V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLV76790QWDRBxQ1"
		(extends "TLV76733QWDRBxQ1")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "TLV76790QWDRBxQ1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/gpn/TLV767-q1"
			(at -1.27 0 0)
		)
		(property "Description" "1A, 16V Precision Linear Voltage Regulator, with enable pin, Fixed Output 9.0V, VSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1A 16V Precision Linear Voltage Regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70248_HTSSOP20"
		(extends "TPS70245_HTSSOP20")
		(property "Reference" "U"
			(at -8.89 13.335 0)
		)
		(property "Value" "TPS70248_HTSSOP20"
			(at -2.54 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps702.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "3.3V 500mA/1.5V 250mA Dual Low Drop-out Regulator with Voltage Supervisor, PowerPAD TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual 3.3V 1.5V LDO Regulator 500mA 250mA Voltage Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70251_HTSSOP20"
		(extends "TPS70245_HTSSOP20")
		(property "Reference" "U"
			(at -8.89 13.335 0)
		)
		(property "Value" "TPS70251_HTSSOP20"
			(at -2.54 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps702.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "3.3V 500mA/1.8V 250mA Dual Low Drop-out Regulator with Voltage Supervisor, PowerPAD TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual 3.3V 1.8V LDO Regulator 500mA 250mA Voltage Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70258_HTSSOP20"
		(extends "TPS70245_HTSSOP20")
		(property "Reference" "U"
			(at -8.89 13.335 0)
		)
		(property "Value" "TPS70258_HTSSOP20"
			(at -2.54 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps702.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "3.3V 500mA/2.5V 250mA Dual Low Drop-out Regulator with Voltage Supervisor, PowerPAD TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual 3.3V 2.5V LDO Regulator 500mA 250mA Voltage Supervisor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70345"
		(extends "TPS70302")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70345"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps703.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Sequenced Outputs, 3.3V 1A/1.2V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70348"
		(extends "TPS70302")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70348"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps703.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Sequenced Outputs, 3.3V 1A/1.5V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70351"
		(extends "TPS70302")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70351"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps703.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Sequenced Outputs, 3.3V 1A/1.8V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70358"
		(extends "TPS70302")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70358"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps703.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Sequenced Outputs, 3.3V 1A/2.5V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70445"
		(extends "TPS70402")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70445"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps704.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Independent Enable, 3.3V 1A/1.2V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70448"
		(extends "TPS70402")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70448"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps704.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Independent Enable, 3.3V 1A/1.5V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70451"
		(extends "TPS70402")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70451"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps704.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Independent Enable, 3.3V 1A/1.8V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS70458"
		(extends "TPS70402")
		(property "Reference" "U"
			(at -10.16 13.335 0)
		)
		(property "Value" "TPS70458"
			(at 0 13.335 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias"
			(at -0.635 15.875 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps704.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual-Output, Low Dropout Voltage Regulators With Integrated SVS For Split Voltage Systems, Independent Enable, 3.3V 1A/2.5V 2A, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual ldo regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7133"
		(extends "TPS7150")
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "TPS7133"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps71.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Low Drop-out Voltage Regulator, Fixed Output 3.3V, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7148"
		(extends "TPS7150")
		(property "Reference" "U"
			(at -6.35 8.255 0)
		)
		(property "Value" "TPS7148"
			(at 0 8.255 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps71.pdf"
			(at 0 0 0)
		)
		(property "Description" "500mA Low Drop-out Voltage Regulator, Fixed Output 4.85V, SO-8/DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 500mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71519__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71519__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 1.9V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71523__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71523__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 2.3V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71525__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71525__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 2.5V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71530__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71530__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 3V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71533__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71533__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 3.3V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS715345__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS715345__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 3.45V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS71550__SC70"
		(extends "TPS71518__SC70")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS71550__SC70"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 5.715 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps715.pdf"
			(at -7.62 20.32 0)
		)
		(property "Description" "Low-drop Voltage Regulator, Io up to 50mA, Fixed Vo 5V, Ignd 3.2uA , SC70."
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO regulator voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "TPS72215"
		(extends "TPS72218")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS72215"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps722.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low input voltage 50mA LDO, 1.5V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS72216"
		(extends "TPS72218")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS72216"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps722.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low input voltage 50mA LDO, 1.6V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS72301DDC"
		(extends "TPS72301DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS72301DDC"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps723.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "200-mA, Low-Noise, High-PSRR, Negative Output Low-Dropout Linear Regulator, Adjustable Output (-1.2 V to -10 V), TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73018DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73018DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps730.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Noise, High PSRR, 200mA Low Drop 1.8V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed LDO 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS730285DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS730285DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps730.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Low Noise, High PSRR, 200mA Low Drop 2.85V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fixed LDO 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73101DBV"
		(extends "TPS73601DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73101DBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop Adjustable Out Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Adjustable LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS731125DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS731125DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 1.25V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73115DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73115DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 1.5V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73118DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73118DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 1.8V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73125DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73125DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 2.5V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73130DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73130DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 3.0V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73131DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73131DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 3.1V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73132DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73132DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 3.2V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73133DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73133DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 3.3V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73150DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73150DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps731.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 150mA Low Drop 5.0V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 150mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS736125DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS736125DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 1.25V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73615DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73615DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 1.5V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73616DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73616DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 1.6V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73618DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73618DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 1.8V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73619DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73619DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 1.9V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73630DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73630DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 3.0V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73632DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73632DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 3.2V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73633DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73633DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 3.3V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS73643DBV"
		(extends "TPS73625DBV")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TPS73643DBV"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps736.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cap free NMOS 400mA Low Drop 4.3V Regulator, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cap free Fixed LDO 400mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS74801DRC"
		(extends "TPS74801AWDRC")
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "TPS74801DRC"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at 0 10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps74801.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Texas Instruments 1.5A, Low-Dropout Linear Regulator With Programmable Soft-Start, 0.8-5.5Vin, 2.7-6.0Vbias, 0.8-3.6Vout"
			(at 0 0 0)
		)
		(property "ki_keywords" "regulator LDO positive adjustable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76318"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76318"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 1.8V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76325"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76325"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 2.5V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76327"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76327"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 2.7V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76329"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76329"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 2.8V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76330"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76330"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 3.0V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76333"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76333"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 3.3V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76338"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76338"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 3.8V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76350"
		(extends "TPS76316")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS76350"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps763.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power 150mA LDO 5.0V fixed output voltage, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "linear low dropout Regulator fixed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76915"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76915"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76918"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76918"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76925"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76925"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76927"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76927"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 2.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76928"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76928"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76930"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76930"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76933"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76933"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS76950"
		(extends "TPS76912")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS76950"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps769.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Ultra Low Power 100mA Low Drop Out Regulator 5.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ultra Low Power Fixed LDO 100mA 5V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77718_HTSSOP20"
		(extends "TPS77715_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77718_HTSSOP20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 3.81 -5.08 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.8V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77718_SO8"
		(extends "TPS77715_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77718_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.8V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77725_HTSSOP20"
		(extends "TPS77715_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77725_HTSSOP20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 3.81 -5.08 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 2.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77725_SO8"
		(extends "TPS77715_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77725_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 2.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77733_HTSSOP20"
		(extends "TPS77715_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77733_HTSSOP20"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 3.81 -5.08 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 3.3V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77733_SO8"
		(extends "TPS77715_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77733_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 3.3V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77818_HTSSOP20"
		(extends "TPS77815_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS77818_HTSSOP20"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.8V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77818_SO8"
		(extends "TPS77815_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77818_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 1.8V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77825_HTSSOP20"
		(extends "TPS77815_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS77825_HTSSOP20"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 2.5V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77825_SO8"
		(extends "TPS77815_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77825_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 2.5V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77833_HTSSOP20"
		(extends "TPS77815_HTSSOP20")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TPS77833_HTSSOP20"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 0 10.795 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 3.3V, HTSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS77833_SO8"
		(extends "TPS77815_SO8")
		(property "Reference" "U"
			(at -6.35 5.715 0)
		)
		(property "Value" "TPS77833_SO8"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps777.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "750mA Fast-Transient Low Dropout Voltage Regulator, Fixed Output 3.3V, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "750mA LDO Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78218DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78218DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78223DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78223DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 2.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78225DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78225DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78227DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78227DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 2.7V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78228DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78228DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 2.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78230DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78230DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS78236DDC"
		(extends "TPS78233DDC")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS78236DDC"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps782"
			(at 0 12.7 0)
		)
		(property "Description" "150-mA, 500nA Ultra-Low-IQ LDO, 3.6V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS79325-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79325-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 2.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS79328-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79328-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 2.8V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS793285-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS793285-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 2.85V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS79330-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79330-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 3.0V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS79333-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS79333-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 3.3V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS793475-EP"
		(extends "TPS79318-EP")
		(property "Reference" "U"
			(at -3.81 5.715 0)
		)
		(property "Value" "TPS793475-EP"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps79333-ep.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "200mA UltraLow-Noise, High-Precision, Fast RF, Low Drop-out Voltage Regulator, Fixed Output 4.75V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 200mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0508PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0508PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 0.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0508PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0508PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 0.8V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0510PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0510PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0512PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0512PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0512PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0512PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.2V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0515PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0515PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0518PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0518PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.8V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0518PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0518PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 1.8V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0520PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0520PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.0V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0522PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0522PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.2V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0522PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0522PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.2V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0525PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0525PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0527PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0527PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.7V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A05285PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A05285PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.85V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0528PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0528PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 2.8V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0530PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0530PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 3.0V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0530PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0530PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 3.0V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0531PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0531PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 3.1V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0533PDBV"
		(extends "LP5907MFX-1.2")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "TPS7A0533PDBV"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A0533PDBZ"
		(extends "MCP1703Ax-330xxTT")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "TPS7A0533PDBZ"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7a05.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "200-mA Ultra-Low-Iq LDO, 3.3V, SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Output LDO Low-Iq"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS7A90"
		(extends "TPS7A91")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TPS7A90"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PDSO-N10_EP1.2x2mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps7a90.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "0.5A, High-Accuracy, Low-Noise LDO Voltage Regulator, Texas S-PDSO-N10"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO voltage regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PDSO*"
			(at 0 0 0)
		)
	)
	(symbol "UA78M08QDCYRQ1"
		(extends "UA78M05QDCYRQ1")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "UA78M08QDCYRQ1"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/UA78M-Q1"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 25V Linear Regulator, Fixed Output 8V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Q100 0.5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "UA78M10QDCYRQ1"
		(extends "UA78M05QDCYRQ1")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "UA78M10QDCYRQ1"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/UA78M-Q1"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 28V Linear Regulator, Fixed Output 10V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Q100 0.5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "UA78M33QDCYRQ1"
		(extends "UA78M05QDCYRQ1")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "UA78M33QDCYRQ1"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/UA78M-Q1"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 500mA 25V Linear Regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Automotive Q100 0.5A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "XC6206PxxxMR"
		(extends "APE8865N-12-HF-3")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "XC6206PxxxMR"
			(at 0 3.175 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at 0 5.715 0)
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf"
			(at 0 0 0)
		)
		(property "Description" "Positive 60-250mA Low Dropout Regulator, Fixed Output, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Torex LDO Voltage Regulator Fixed Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?3*"
			(at 0 0 0)
		)
	)
	(symbol "XC6210B332MR"
		(extends "XC6220B331MR")
		(property "Reference" "U"
			(at 0 8.89 0)
		)
		(property "Value" "XC6210B332MR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6210/XC6210.pdf"
			(at 19.05 -25.4 0)
		)
		(property "Description" "700mA, Low Drop-out Voltage Regulator, Fixed Output 3.3V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LDO Voltage Regulator 700mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "uA7808"
		(extends "uA7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7808"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 8V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "uA7810"
		(extends "uA7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7810"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 10V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "uA7812"
		(extends "uA7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7812"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 12V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "uA7815"
		(extends "uA7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7815"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 15V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "uA7824"
		(extends "uA7805")
		(property "Reference" "U"
			(at -3.81 3.175 0)
		)
		(property "Value" "uA7824"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0.635 -3.81 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua78.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 24V, TO-220/TO-263"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage Regulator 1A Positive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263* TO?220*"
			(at 0 0 0)
		)
	)
)
