(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "34.81-8240"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "34.81-8240"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Finder_34.81"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://gfinder.findernet.com/public/attachments/34/EN/S34USAEN.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-slim - Solid State Relay, 2A, 240V AC output, Zero crossing switching"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photo-Triac Opto Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Finder*34.81*"
			(at 0 0 0)
		)
		(symbol "34.81-8240_0_1")
		(symbol "34.81-8240_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "34.81-9024"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "34.81-9024"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Finder_34.81"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Slim Solid-State Relay, 2A, 24V DC output switching"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Finder*34.81*"
			(at 0 0 0)
		)
		(symbol "34.81-9024_0_1")
		(symbol "34.81-9024_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "A2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AQH0213"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "AQH0213"
			(at -2.54 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 300mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AQH0213_0_0"
			(text "ZCD"
				(at -2.54 -3.81 0)
			)
		)
		(symbol "AQH0213_0_1")
		(symbol "AQH0213_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AQH0213A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH0213A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 300mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "AQH0213A_0_1")
		(symbol "AQH0213A_1_1"
			(text "ZCD"
				(at -2.54 -3.81 0)
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AQH0223"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH0223"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -17.78 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 300mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "AQH0223_0_1")
		(symbol "AQH0223_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AQH0223A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH0223A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 300mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "AQH0223A_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASSR-1218"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ASSR-1218"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x4.3mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0173EN"
			(at 0 0 0)
		)
		(property "Description" "Form A, Solid State Relay (Photo MOSFET) 60V, 0.2A, 10Ohm, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x4.3mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "ASSR-1218_0_1")
		(symbol "ASSR-1218_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CPC1002N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CPC1002N"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_3.8x4.1mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/CPC1002N.pdf/$file/CPC1002N.pdf"
			(at 0 0 0)
		)
		(property "Description" "Form A, Solid State Relay (Photo MOSFET) 60V, 0.7A, 0.55Ohm, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.8x4.1mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "CPC1002N_0_1")
		(symbol "CPC1002N_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CPC1017N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CPC1017N"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_3.8x4.1mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/CPC1017N.pdf/$file/CPC1017N.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Form A, Solid State Relay (Photo MOSFET) 60V, 0.1A, 16Ohm, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.8x4.1mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "CPC1017N_0_1")
		(symbol "CPC1017N_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FOD420"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FOD420"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FOD4218-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 0.75mA, Itm 300mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "FOD420_0_1")
		(symbol "FOD420_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FODM3011"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3011"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 250V, Ift 10mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "FODM3011_0_1")
		(symbol "FODM3011_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LCC110"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "LCC110"
			(at -0.254 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/LCC110.pdf/$file/LCC110.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-Form-C OptoMOS® Relay, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LCC110_0_0"
			(text "NC"
				(at 2.54 8.89 0)
			)
			(text "NO"
				(at 2.54 -8.89 0)
			)
		)
		(symbol "LCC110_0_1")
		(symbol "LCC110_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "nc")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "nc")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MOC3010M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3010M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 250V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "MOC3010M_0_1")
		(symbol "MOC3010M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MOC3031M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3031M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 250V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "MOC3031M_0_0"
			(text "ZCD"
				(at 0.508 -2.54 0)
			)
		)
		(symbol "MOC3031M_0_1")
		(symbol "MOC3031M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S102S01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S102S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 8mA, IT 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
		(symbol "S102S01_0_1")
		(symbol "S102S01_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S102S02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S102S02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s02_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 8mA, IT 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
		(symbol "S102S02_0_0"
			(text "ZCD"
				(at 0.508 -2.54 0)
			)
		)
		(symbol "S102S02_0_1")
		(symbol "S102S02_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP141G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP141G"
			(at -5.08 -5.207 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/TLP141G(U,F)-Toshiba-datasheet-134958.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Thyristor Based, Vdrm 400V, It 150mA, Viso 2500V, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptoThyristor DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP141G_0_1")
		(symbol "TLP141G_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP160G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP160G"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16916&prodName=TLP160G"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 5mA, SOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP160G_0_1")
		(symbol "TLP160G_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP161G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP161G"
			(at -4.699 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16921&prodName=TLP161G"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 5mA, SOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP161G_0_0"
			(text "ZCD"
				(at 0.508 -2.54 0)
			)
		)
		(symbol "TLP161G_0_1")
		(symbol "TLP161G_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP175A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 4.953 0)
		)
		(property "Value" "TLP175A"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=13665&prodName=TLP175A"
			(at 0 0 0)
		)
		(property "Description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP175A_0_1")
		(symbol "TLP175A_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP222A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP222A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=17036&prodName=TLP222A"
			(at 0 0 0)
		)
		(property "Description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 0,5A, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP222A_0_1")
		(symbol "TLP222A_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP222A-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP222A-2"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=17036&prodName=TLP222A"
			(at 0 0 0)
		)
		(property "Description" "Dual MOSFET Photorelay 1-Form-A, Voff 60V, Ion 0,5A, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP222A-2_0_1")
		(symbol "TLP222A-2_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TLP222A-2_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP3123"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP3123"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.9mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=10047&prodName=TLP3123"
			(at 0 0 0)
		)
		(property "Description" "Solid State Relay (Photo MOSFET) 40V, 1A, 0.1Ohm, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.9mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "TLP3123_0_1")
		(symbol "TLP3123_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP3542"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "TLP3542"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-5-6_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=1284&prodName=TLP3542"
			(at 0 0 0)
		)
		(property "Description" "Photo MOSFET optically coupled, ON 4A, 50mohm, OFF state 20V, Isolation 2500 VRMS, DIP-5-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP3542_0_1")
		(symbol "TLP3542_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP3543"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "TLP3543"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12660&prodName=TLP3543"
			(at 0 0 0)
		)
		(property "Description" "Photo MOSFET optically coupled, ON 4A, 50mohm, OFF state 20V, Isolation 2500 VRMS, DIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP3543_0_1")
		(symbol "TLP3543_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "34.81-7048"
		(extends "34.81-9024")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "34.81-7048"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Finder_34.81"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Slim Solid-State Relay, 0.1A, 48V DC output switching"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Finder*34.81*"
			(at 0 0 0)
		)
	)
	(symbol "AQH1213"
		(extends "AQH0213")
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "AQH1213"
			(at -2.54 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 600mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH1213A"
		(extends "AQH0213A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH1213A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 600mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH1223"
		(extends "AQH0223")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH1223"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -17.78 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 600mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH1223A"
		(extends "AQH0223A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH1223A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 600mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH2213"
		(extends "AQH0213")
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "AQH2213"
			(at -2.54 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 900mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH2213A"
		(extends "AQH0213A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH2213A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 900mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH2223"
		(extends "AQH0223")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH2223"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -17.78 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 900mA, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH2223A"
		(extends "AQH0223A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH2223A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 900mA, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH3213"
		(extends "AQH0213")
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "AQH3213"
			(at -2.54 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -19.05 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 1.2A, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH3213A"
		(extends "AQH0213A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH3213A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 1.2A, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH3223"
		(extends "AQH0223")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH3223"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8-N7_W7.62mm"
			(at -17.78 -7.62 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 1.2A, DIP-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*N7*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AQH3223A"
		(extends "AQH0223A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "AQH3223A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-7-8_6.4x9.78mm_P2.54mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://mediap.industry.panasonic.eu/assets/imported/industrial.panasonic.com/ac/cdn/e/control/relay/solid-state/catalog/semi_eng_aqh.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, IT 1.2A, SOIC-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.78mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "BC2213A"
		(extends "AQH0213A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "BC2213A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SSO-8-7_6.4x9.7mm_P2.54mm"
			(at -5.08 5.08 0)
		)
		(property "Datasheet" "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2312161855_BC-BC2213A_C596512.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, IT 900mA, SSO-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.4x9.7mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "CPC1117N"
		(extends "CPC1017N")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CPC1117N"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_3.8x4.1mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/CPC1117N.pdf/$file/CPC1117N.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Form B, Solid State Relay (Photo MOSFET) 60V, 0.15A, 16Ohm, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Output Photorelay 1-Form-B NC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.8x4.1mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "FOD4208"
		(extends "FOD420")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FOD4208"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FOD4218-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 800V, Ift 0.75mA, Itm 300mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FOD4216"
		(extends "FOD420")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FOD4216"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FOD4218-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 0.75mA, Itm 300mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FOD4218"
		(extends "FOD420")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FOD4218"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FOD4218-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 800V, Ift 0.75mA, Itm 300mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM3012"
		(extends "FODM3011")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3012"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 250V, Ift 5mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM3022"
		(extends "FODM3011")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3022"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 400V, Ift 10mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM3023"
		(extends "FODM3011")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3023"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 400V, Ift 5mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM3052"
		(extends "FODM3011")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3052"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM3053"
		(extends "FODM3011")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM3053"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Full Pitch Mini-Flat Random Phase Opto-Triac, Vdrm 600V, Ift 5mA, MFP 4L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Mini-Flat"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HHG1D-1"
		(extends "S102S02")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "HHG1D-1"
			(at 0 5.08 0)
		)
		(property "Footprint" "Relay_THT:Relay_NCR_HHG1D-1"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://ncr.hk/uploads/Relays/Solid_State_Relays/HHG1D-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "NCR zero cross solid state relay 1A, 2A, 3A, 4A"
			(at 0 0 0)
		)
		(property "ki_keywords" "ssr"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Relay*HHG1D*"
			(at 0 0 0)
		)
	)
	(symbol "LAA110"
		(extends "TLP222A-2")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LAA110"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.clare.com/home/pdfs.nsf/www/LAA110.pdf/$file/LAA110.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Single-Pole, Normally Open OptoMOS® Relay, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual MOSFET Output Photorelay 1-Form-A"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LBB110"
		(extends "TLP222A-2")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LBB110"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/LBB110.pdf/$file/LBB110.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Single-Pole, Normally Closed OptoMOS® Relay, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual MOSFET Output Photorelay 1-Form-B"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3011M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3011M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 250V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3012M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3012M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 250V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3020M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3020M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 30mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3021M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3021M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3022M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3022M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3023M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3023M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3032M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3032M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 250V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3033M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3033M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 250V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3041M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3041M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3042M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3042M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3043M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3043M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3043M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3051M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3051M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3052M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3052M"
		(extends "MOC3010M")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "MOC3052M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3052M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3061M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3061M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3062M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3062M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3063M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3063M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3081M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3081M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3083M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 800V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3082M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3082M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3083M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 800V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3083M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3083M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3083M-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 800V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3162M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3162M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 10mA, dv/dt 1000, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOC3163M"
		(extends "MOC3031M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOC3163M"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3163M-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 5mA, dv/dt 1000, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "S112S01"
		(extends "S102S01")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S112S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s112s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 8mA, IT 12A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S116S01"
		(extends "S102S01")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S116S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s116s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 400V, Ift 8mA, IT 16A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S116S02"
		(extends "S102S02")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S116S02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s116s02_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 400V, Ift 8mA, IT 16A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S202S01"
		(extends "S102S01")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S202S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 8mA, IT 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S202S02"
		(extends "S102S02")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S202S02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s02_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 8mA, IT 8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S212S01"
		(extends "S102S01")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S212S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s112s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 8mA, IT 12A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S216S01"
		(extends "S102S01")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S216S01"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s116s01_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 8mA, IT 16A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random Phase Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "S216S02"
		(extends "S102S02")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "S216S02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SIP:SIP4_Sharp-SSR_P7.62mm_Straight"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/s116s02_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 8mA, IT 16A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross Solid State Relays"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SIP4*Sharp*SSR*P7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP148G"
		(extends "TLP141G")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP148G"
			(at -5.08 -5.207 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=1019&prodName=TLP148G"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Thyristor Based, Vdrm 400V, It 150mA, Viso 2500V, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptoThyristor DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP160J"
		(extends "TLP160G")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP160J"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16919&prodName=TLP160J"
			(at 0 0 0)
		)
		(property "Description" "Random Phase Opto-Triac, Vdrm 600V, Ift 7mA, SOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Random"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP161J"
		(extends "TLP161G")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP161J"
			(at -4.699 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=4207&prodName=TLP161J"
			(at 0 0 0)
		)
		(property "Description" "Zero Cross Opto-Triac, Vdrm 600V, Ift 7mA, SOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Opto-Triac Opto Triac Zero Cross"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP3544"
		(extends "TLP3543")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "TLP3544"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12661&prodName=TLP3544"
			(at 0 0 0)
		)
		(property "Description" "Photo MOSFET optically coupled, ON 3.5A, 60mohm, OFF state 40V, Isolation 2500 VRMS, DIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP3545"
		(extends "TLP3543")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "TLP3545"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12663&prodName=TLP3545"
			(at 0 0 0)
		)
		(property "Description" "Photo MOSFET optically coupled, ON 3A, 70mohm, OFF state 60V, Isolation 2500 VRMS, DIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP3546"
		(extends "TLP3543")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "TLP3546"
			(at -1.27 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12671&prodName=TLP3546"
			(at 0 0 0)
		)
		(property "Description" "Photo MOSFET optically coupled, ON 2A, 200mohm, OFF state 100V, Isolation 2500 VRMS, DIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
)
