(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LV25-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LV25-P"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Sensor_Voltage:LEM_LV25-P"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.lem.com/sites/default/files/products_datasheets/lv_25-p.pdf"
			(at 0 0 0)
		)
		(property "Description" "LEM Voltage transducer LV 25-P"
			(at 0 0 0)
		)
		(property "ki_keywords" "Voltage transducer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LEM?LV25?P*"
			(at 0 0 0)
		)
		(symbol "LV25-P_0_1")
		(symbol "LV25-P_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "HV+")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "HV-")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "V-")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "M")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
