(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "0896BM15A0001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "0896BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0896BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0896BM15A0001/0896BM15A0001.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "863-928MHz 1:1 RF Transformer, Unbalanced to Balanced"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0896BM15A0001*"
			(at 0 0 0)
		)
		(symbol "0896BM15A0001_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "30F-51NL"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at -6.35 21.59 0)
		)
		(property "Value" "30F-51NL"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_YDS_30F-51NL_SO-24_7.1x15.1mm"
			(at -7.62 7.62 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811051610_Shanghai-YDS-Tech-30F-51NL_C123168.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "1CT:1CT 10/100/1000 Base-T Ethernet Transformer, SMD-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "gigabit RJ45 transformer ethernet lan"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*YDS*30F?51NL*"
			(at 0 0 0)
		)
		(symbol "30F-51NL_0_1"
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "TD1+")
				(number "2")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "CT")
				(number "1")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "TD1-")
				(number "3")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TD2+")
				(number "5")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CT")
				(number "4")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TD2-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TD3+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TD3-")
				(number "9")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "TD4+")
				(number "11")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "CT")
				(number "10")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "TD4-")
				(number "12")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "MX1+")
				(number "23")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "CT")
				(number "24")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "MX1-")
				(number "22")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "MX2+")
				(number "20")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "CT")
				(number "21")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "MX2-")
				(number "19")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "MX3+")
				(number "17")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CT")
				(number "18")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "MX3-")
				(number "16")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "MX4+")
				(number "14")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "CT")
				(number "15")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "MX4-")
				(number "13")
			)
		)
		(symbol "30F-51NL_1_1")
		(embedded_fonts no)
	)
	(symbol "5400BL15B050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "5400BL15B050"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_5400BL15B050E"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/5400BL15B050/5400BL15B050.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "4.9-5.9GHz 1:1 RF Transformer, Unbalanced to Balanced"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*5400BL15B050E*"
			(at 0 0 0)
		)
		(symbol "5400BL15B050_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.15-400MHz 1:1 RF Transformer, Balanced to Balanced, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1-1_0_1")
		(symbol "ADT1-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1-1WT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1-1WT"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1-1WT.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.005-125MHz 1:1 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1-1WT_0_1")
		(symbol "ADT1-1WT_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1-1WT-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1-1WT-1"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1-1WT-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-400MHz 1:1 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1-1WT-1_0_1")
		(symbol "ADT1-1WT-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1-6T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1-6T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1-6T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.06-160MHz 1:1 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
		(symbol "ADT1-6T_0_1")
		(symbol "ADT1-6T_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1.5-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1.5-1"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1.5-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5-650MHz 1:1.5 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1.5-1_0_1")
		(symbol "ADT1.5-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1.5-122"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADT1.5-122"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1.5-122+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "20-1200MHz 1:1.5 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1.5-122_0_1")
		(symbol "ADT1.5-122_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1.5-17"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1.5-17"
			(at 0 8.89 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1.5-17+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5-1700MHz 1:1.5 RF Transformer, Unbalanced to Unbalanced, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT1.5-17_0_1")
		(symbol "ADT1.5-17_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT1.5-2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT1.5-2"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT1.5-2+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.3-225MHz 1:1.5 RF Transformer, Balanced to Balanced, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
		(symbol "ADT1.5-2_0_1")
		(symbol "ADT1.5-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT2-1T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT2-1T"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT2-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.40-450MHz 1:2 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADT2-1T_0_1")
		(symbol "ADT2-1T_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT3-6T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT3-6T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT3-6T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-600MHz 1:3 RF Transformer, Unbalanced to Balanced Center Tap, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
		(symbol "ADT3-6T_0_1")
		(symbol "ADT3-6T_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADT4-6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-6"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-6+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.07-250MHz 1:4 RF Transformer, Balanced to Balanced, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
		(symbol "ADT4-6_0_1")
		(symbol "ADT4-6_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADTL1-15-75"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADTL1-15-75"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTL1-15-75+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "10-1500MHz 1:1 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADTL1-15-75_0_1")
		(symbol "ADTL1-15-75_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADTL1-4-75"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADTL1-4-75"
			(at 0 -3.81 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTL1-4-75+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "0.5-1000MHz 1:1 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADTL1-4-75_0_1")
		(symbol "ADTL1-4-75_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADTT1-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADTT1-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTT1-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.3-300MHz 1:1 RF Transformer, Unbalanced to Balanced Center Tap at Primary/Secondary, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
		(symbol "ADTT1-1_0_1")
		(symbol "ADTT1-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADTT1-6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADTT1-6"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTT1-6+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.015-100MHz 1:1 RF Transformer, Unbalanced to Balanced Center Tap at Primary/Secondary, CD637"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
		(symbol "ADTT1-6_0_1")
		(symbol "ADTT1-6_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADTT1.5-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADTT1.5-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTT1.5-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.25-300MHz 1:1.5 RF Transformer, Unbalanced to Balanced Center Tap at Primary/Secondary, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
		(symbol "ADTT1.5-1_0_1")
		(symbol "ADTT1.5-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B0322J5050AHF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "B0322J5050AHF"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Anaren_0805_2012Metric-6"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://cdn.ttm.com/repository/products/wireless-xinger/balun-transformers/B0322J5050AHF/B0322J5050AHF.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "300MHz to 2200MHz 1:1 RF Transformer, 50 ohm, Unbalanced to Balanced"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Anaren*0805*2012Metric*"
			(at 0 0 0)
		)
		(symbol "B0322J5050AHF_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST1"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "CST1"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 20A, 1:20 to 1:125"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST1*"
			(at 0 0 0)
		)
		(symbol "CST1_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "CST1_1_1"
			(pin no_connect line
				(at -2.54 5.08 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "2")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 5.08 180)
				(length 2.54)
				(hide yes)
				(name "3")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST1_Split"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 3.175 0)
		)
		(property "Value" "CST1_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 20A, 1:20 to 1:125"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST1*"
			(at 0 0 0)
		)
		(symbol "CST1_Split_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
		)
		(symbol "CST1_Split_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "6")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "2")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST2"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "CST2"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 20A, 1:20 to 1:125"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST2*"
			(at 0 0 0)
		)
		(symbol "CST2_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(symbol "CST2_1_1"
			(pin no_connect line
				(at -2.54 5.08 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "2")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 5.08 180)
				(length 2.54)
				(hide yes)
				(name "6")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST2010"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "CST2010"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST2010"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst2010.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 40A, 1:20 to 1:200"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST2010*"
			(at 0 0 0)
		)
		(symbol "CST2010_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "CST2010_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "7")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "1")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "8")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "3")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 0)
				(length 2.54)
				(hide yes)
				(name "9")
				(number "9")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "10")
				(number "10")
			)
			(pin no_connect line
				(at 2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST2010_Split"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 3.175 0)
		)
		(property "Value" "CST2010_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST2010"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst2010.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 40A, 1:20 to 1:200"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST2010*"
			(at 0 0 0)
		)
		(symbol "CST2010_Split_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
		)
		(symbol "CST2010_Split_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "1")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "7")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "3")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 0)
				(length 2.54)
				(hide yes)
				(name "8")
				(number "8")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 2.54 0)
				(length 2.54)
				(hide yes)
				(name "9")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CST2_Split"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 3.175 0)
		)
		(property "Value" "CST2_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Coilcraft_CST2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/cst.pdf"
			(at 0 0 0)
		)
		(property "Description" "Coilcraft Current Sense Transformer, SMD, 20A, 1:20 to 1:125"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Coilcraft*CST2*"
			(at 0 0 0)
		)
		(symbol "CST2_Split_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "5")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
		)
		(symbol "CST2_Split_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 0 0)
				(length 2.54)
				(hide yes)
				(name "2")
				(number "2")
			)
			(pin no_connect line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ED8_4"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "ED8_4"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_ED8_4-Lead_10.5x8mm_P5mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://gitlab.com/kicad/libraries/kicad-footprints/-/merge_requests/3626"
			(at 0 -13.97 0)
		)
		(property "Description" "600:600 Impedance Permalloy Core 1:1 Isolated Audio Transformer"
			(at 0 -8.89 0)
		)
		(property "ki_keywords" "ED8 4-lead body 10.5x8mm body pitch 5mm height 5mm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*ED8*4*Lead*10.5x8mm*P5mm*"
			(at 0 0 0)
		)
		(symbol "ED8_4_0_1")
		(symbol "ED8_4_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ETC1-1-13"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ETC1-1-13"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_MACOM_SM-22"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://cdn.macom.com/datasheets/ETC1-1-13.pdf"
			(at 0 0 90)
		)
		(property "Description" "4.5-4000MHz 1:1 RF Transformer, Balanced Transmission Line, SM-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "MACOM RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*MACOM*SM?22*"
			(at 0 0 0)
		)
		(symbol "ETC1-1-13_0_0"
			(text "Mounting"
				(at 3.429 0 900)
			)
		)
		(symbol "ETC1-1-13_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 1.27)
				(name "MP")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LL1587"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 1.27 -11.43 0)
		)
		(property "Value" "LL1587"
			(at 0 11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Microphone_Lundahl_LL1587"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.lundahl.se/wp-content/uploads/datasheets/1587.pdf"
			(at 0 0 0)
		)
		(property "Description" "Lundahl Transformers, Microphone Transformer"
			(at 0 0 0)
		)
		(property "ki_keywords" "microphone transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Microphone*Lundahl*LL1587*"
			(at 0 0 0)
		)
		(symbol "LL1587_0_0"
			(text "+"
				(at -2.54 8.89 0)
			)
			(text "+"
				(at -2.54 -1.27 0)
			)
			(text "+"
				(at 2.54 6.35 0)
			)
		)
		(symbol "LL1587_0_1")
		(symbol "LL1587_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 7.62)
				(name "P1+")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 7.62)
				(name "P1-")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 7.62)
				(name "P2+")
				(number "4")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 7.62)
				(name "P2-")
				(number "3")
			)
			(pin input line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 7.62)
				(name "S+")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 7.62)
				(name "S-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P0926NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "P0926NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_P0926NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*P0926NL*"
			(at 0 0 0)
		)
		(symbol "P0926NL_0_1")
		(symbol "P0926NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA1323NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA1323NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA1323NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA1323NL*"
			(at 0 0 0)
		)
		(symbol "PA1323NL_0_1")
		(symbol "PA1323NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2001NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA2001NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2001NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2001NL*"
			(at 0 0 0)
		)
		(symbol "PA2001NL_0_1")
		(symbol "PA2001NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2002NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA2002NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
		(symbol "PA2002NL_0_1")
		(symbol "PA2002NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2004NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA2004NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2004NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2004NL*"
			(at 0 0 0)
		)
		(symbol "PA2004NL_0_1")
		(symbol "PA2004NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2005NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA2005NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2005NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2005NL*"
			(at 0 0 0)
		)
		(symbol "PA2005NL_0_1")
		(symbol "PA2005NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2006NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA2006NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2006NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2006NL*"
			(at 0 0 0)
		)
		(symbol "PA2006NL_0_1")
		(symbol "PA2006NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2007NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA2007NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2007NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2007NL*"
			(at 0 0 0)
		)
		(symbol "PA2007NL_0_1")
		(symbol "PA2007NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA2777NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA2777NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2777NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2777NL*"
			(at 0 0 0)
		)
		(symbol "PA2777NL_0_1")
		(symbol "PA2777NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PA3493NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA3493NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA3493NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1.25:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA3493NL*"
			(at 0 0 0)
		)
		(symbol "PA3493NL_0_1")
		(symbol "PA3493NL_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PT61017PEL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 10.795 0)
		)
		(property "Value" "PT61017PEL"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_Bourns_PT61017PEL"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/PT61017PEL.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Ethernet LAN 10/100 Base-Tx Transformer with Center Taps"
			(at 0 0 0)
		)
		(property "ki_keywords" "single port ethernet transformer poe center-tap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*Bourns*PT61017PEL*"
			(at 0 0 0)
		)
		(symbol "PT61017PEL_0_1")
		(symbol "PT61017PEL_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RD-")
				(number "8")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "C_RD")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RD+")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TD-")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "C_TD")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RX-")
				(number "9")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C_RX")
				(number "10")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "RX+")
				(number "11")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TX-")
				(number "14")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "C_TX")
				(number "15")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "TX+")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PT61020EL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at -6.35 20.32 0)
		)
		(property "Value" "PT61020EL"
			(at 6.35 20.32 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_Bourns_PT61020EL"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.bourns.com/pdfs/PT61020.pdf"
			(at 0 0 0)
		)
		(property "Description" "10/100/1000 Base-T Ethernet Transformer, SMD-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gigabit PoE RJ45 Transformer Ethernet Lan"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*Bourns*PT61020EL*"
			(at 0 0 0)
		)
		(symbol "PT61020EL_0_1"
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "TD1+")
				(number "2")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "TCT1")
				(number "1")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "TD1-")
				(number "3")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TD2+")
				(number "5")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "TCT2")
				(number "4")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TD2-")
				(number "6")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TD3+")
				(number "8")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "TCT3")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "TD3-")
				(number "9")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "TD4+")
				(number "11")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "TCT4")
				(number "10")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "TD4-")
				(number "12")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "MX1+")
				(number "23")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "MCT1")
				(number "24")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "MX1-")
				(number "22")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "MX2+")
				(number "20")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "MCT2")
				(number "21")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "MX2-")
				(number "19")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "MX3+")
				(number "17")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "MCT3")
				(number "18")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "MX3-")
				(number "16")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "MX4+")
				(number "14")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "MCT4")
				(number "15")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "MX4-")
				(number "13")
			)
		)
		(symbol "PT61020EL_1_1")
		(embedded_fonts no)
	)
	(symbol "TC1-1-13M+"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "TC1-1-13M+"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_MiniCircuits_AT224-1A"
			(at 0 6.35 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/TC1-1-13M+.pdf"
			(at 0 0 0)
		)
		(property "Description" "4.5-3000MHz 1:1 RF Transformer, Balanced Transmission Line, AT224-1A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*AT224*"
			(at 0 0 0)
		)
		(symbol "TC1-1-13M+_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ0.5-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ0.5-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-22x24"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ0.5/D/x, 0.5VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "0.5VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*22x24*"
			(at 0 0 0)
		)
		(symbol "TEZ0.5-D-1_0_1")
		(symbol "TEZ0.5-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ0.5-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ0.5-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-22x24"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ0.5/D/x-x, 0.5VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "0.5VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*22x24*"
			(at 0 0 0)
		)
		(symbol "TEZ0.5-D-2_0_1")
		(symbol "TEZ0.5-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ1.5-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ1.5-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ1.5/D/x, 1.5VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ1.5-D-1_0_1")
		(symbol "TEZ1.5-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ1.5-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ1.5-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ1.5/D/x-x, 1.5VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "1.5VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ+28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ1.5-D-2_0_1")
		(symbol "TEZ1.5-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ10.0-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ10.0-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-44x52"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ10.0/D/x, 10VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "10VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*44x52*"
			(at 0 0 0)
		)
		(symbol "TEZ10.0-D-1_0_1")
		(symbol "TEZ10.0-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ10.0-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ10.0-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-44x52"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ10.0/D/x-x, 10VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "10VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*44x52*"
			(at 0 0 0)
		)
		(symbol "TEZ10.0-D-2_0_1")
		(symbol "TEZ10.0-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ16.0-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ16.0-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-47x57"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ16.0/D/x, 16VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "16VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*47x57*"
			(at 0 0 0)
		)
		(symbol "TEZ16.0-D-1_0_1")
		(symbol "TEZ16.0-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ16.0-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ16.0-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-47x57"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ16.0/D/x-x, 16VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "16VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*47x57*"
			(at 0 0 0)
		)
		(symbol "TEZ16.0-D-2_0_1")
		(symbol "TEZ16.0-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.0-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ2.0-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.0/D/x, 2VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.0-D-1_0_1")
		(symbol "TEZ2.0-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.0-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ2.0-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.0/D/x-x, 2VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.0-D-2_0_1")
		(symbol "TEZ2.0-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.5-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ2.5-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.5/D/x, 2.5VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.5-D-1_0_1")
		(symbol "TEZ2.5-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.5-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ2.5-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.5/D/x-x, 2.5VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.5-D-2_0_1")
		(symbol "TEZ2.5-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.6-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ2.6-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.6/D/x, 2.6VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.6VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.6-D-1_0_1")
		(symbol "TEZ2.6-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ2.6-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ2.6-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-28x33"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ2.6/D/x-x, 2.6VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.6VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*28x33*"
			(at 0 0 0)
		)
		(symbol "TEZ2.6-D-2_0_1")
		(symbol "TEZ2.6-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ4.0-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ4.0-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-35x42"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ4.0/D/x, 4VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "4VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*35x42*"
			(at 0 0 0)
		)
		(symbol "TEZ4.0-D-1_0_1")
		(symbol "TEZ4.0-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ4.0-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ4.0-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-35x42"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ4.0/D/x-x, 4VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "4VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*35x42*"
			(at 0 0 0)
		)
		(symbol "TEZ4.0-D-2_0_1")
		(symbol "TEZ4.0-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ6.0-D-1"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TEZ6.0-D-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-38x45"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ6.0/D/x, 6VA, Single Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "6VA PCB Transformer Single Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*38x45*"
			(at 0 0 0)
		)
		(symbol "TEZ6.0-D-1_0_1")
		(symbol "TEZ6.0-D-1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEZ6.0-D-2"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TEZ6.0-D-2"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Breve_TEZ-38x45"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.breve.pl/pdf/ANG/TEZ_ang.pdf"
			(at 0 0 0)
		)
		(property "Description" "TEZ6.0/D/x-x, 6VA, Dual Secondary, Cast Resin Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "6VA PCB Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Breve*TEZ*38x45*"
			(at 0 0 0)
		)
		(symbol "TEZ6.0-D-2_0_1")
		(symbol "TEZ6.0-D-2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TG110-E050N5xx"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 10.795 0)
		)
		(property "Value" "TG110-E050N5xx"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_Halo_N5_SO-16_7.11x12.7mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/discrete-ultra-100baset.pdf"
			(at 0 21.59 0)
		)
		(property "Description" "Ethernet LAN 10/100 Base-Tx Transformer"
			(at 0 0 0)
		)
		(property "ki_keywords" "single port ethernet transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*Halo*N5*"
			(at 0 0 0)
		)
		(symbol "TG110-E050N5xx_0_1")
		(symbol "TG110-E050N5xx_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "TD-")
				(number "16")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "C_TD")
				(number "15")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TD+")
				(number "14")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RD-")
				(number "11")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "C_RD")
				(number "10")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RD+")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "TX-")
				(number "1")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C_TX")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "TX+")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RX-")
				(number "6")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "C_RX")
				(number "7")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "RX+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TG111-MSC13LF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at -7.62 21.59 0)
		)
		(property "Value" "TG111-MSC13LF"
			(at 8.89 21.59 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_HALO_TG111-MSC13"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/discrete-genesus.pdf"
			(at 2.54 24.13 0)
		)
		(property "Description" "Single Port Gigabit Ethernet Transformers"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single Port Gigabit Ethernet Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*HALO*TG111*"
			(at 0 0 0)
		)
		(symbol "TG111-MSC13LF_0_1"
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "MX4-")
				(number "13")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "MCT4")
				(number "15")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "MX4+")
				(number "14")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MTX3-")
				(number "16")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MCT3")
				(number "18")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MTX3+")
				(number "17")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "MTX2-")
				(number "19")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MCT2")
				(number "21")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MTX2+")
				(number "20")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "MTX1-")
				(number "22")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MTC1")
				(number "24")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "MTX1+")
				(number "23")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "TD4-")
				(number "12")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "TCT4")
				(number "10")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "TD4+")
				(number "11")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "TD3-")
				(number "9")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TCT3")
				(number "7")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TD3+")
				(number "8")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TD2-")
				(number "6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TCT2")
				(number "4")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TD2+")
				(number "5")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "TD1-")
				(number "3")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "TCT1")
				(number "1")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "TD1+")
				(number "2")
			)
		)
		(symbol "TG111-MSC13LF_1_1")
		(embedded_fonts no)
	)
	(symbol "TR1-SO8"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TR1-SO8"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TR1-SO8_0_1")
		(symbol "TR1-SO8_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TR60_FC"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TR60_FC"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TR60_FC_0_1")
		(symbol "TR60_FC_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TR60_IC"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TR60_IC"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TR60_IC_0_1")
		(symbol "TR60_IC_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TR60_IC2"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TR60_IC2"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TR60_IC2_0_1")
		(symbol "TR60_IC2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF1"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TRANSF1"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF1_0_1")
		(symbol "TRANSF1_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF2"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TRANSF2"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF2_0_1")
		(symbol "TRANSF2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "0")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF3"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TRANSF3"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF3_0_1")
		(symbol "TRANSF3_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF4"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TRANSF4"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF4_0_1")
		(symbol "TRANSF4_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF5"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "TRANSF5"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF5_0_1")
		(symbol "TRANSF5_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF6"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 10.16 0)
		)
		(property "Value" "TRANSF6"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF6_0_1")
		(symbol "TRANSF6_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF7"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 13.97 0)
		)
		(property "Value" "TRANSF7"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF7_0_1")
		(symbol "TRANSF7_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TRANSF8"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "TRANSF8"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TRANSF8_0_1")
		(symbol "TRANSF8_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Triad_VPP16-310"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 12.7 0)
		)
		(property "Value" "Triad_VPP16-310"
			(at 0 10.16 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Triad_VPP16-310"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://catalog.triadmagnetics.com/Asset/VPP16-310.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Power transformer, 2x Pri, 2x Sec, 230/115 VAC to 16/8V (0.31/0.62 A)"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "power center-tap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Triad*VPP16?310*"
			(at 0 0 0)
		)
		(symbol "Triad_VPP16-310_0_0"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "Triad_VPP16-310_0_1")
		(symbol "Triad_VPP16-310_1_1")
		(embedded_fonts no)
	)
	(symbol "Wuerth_750315371"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 5.08 0)
		)
		(property "Value" "Wuerth_750315371"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Wuerth_750315371"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://www.we-online.com/catalog/datasheet/750315371.pdf"
			(at 0 0 0)
		)
		(property "Description" "5V, 1A , 320 - 480kHz, 1:1.1, Center Tapped, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Center Tapped Flyback Transformer AEC-Q200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Wuerth*750315371*"
			(at 0 0 0)
		)
		(symbol "Wuerth_750315371_0_1")
		(symbol "Wuerth_750315371_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Wuerth_750343373"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "Wuerth_750343373"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Wuerth_750343373"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://katalog.we-online.com/ctm/datasheet/750343373.pdf"
			(at 0 0 0)
		)
		(property "Description" "Primary 18-60V 300kHz, Dual Secondary 12V-3A/12V-1A, Flyback Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCB Flyback Transformer Dual Secondary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Wuerth*750343373*"
			(at 0 0 0)
		)
		(symbol "Wuerth_750343373_0_1")
		(symbol "Wuerth_750343373_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at 0 2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at 0 0 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin no_connect line
				(at 0 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "9")
			)
			(pin no_connect line
				(at 0 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Wuerth_760871131"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 8.89 0)
		)
		(property "Value" "Wuerth_760871131"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Wuerth_760871131"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.we-online.com/catalog/datasheet/760871131.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Primary 120-420V 60kHz, Dual Secondary 12V-0.5A/12V-0.5A, Single Aux 15V 0.1A, Flyback Transformer, PCB"
			(at 0 0 0)
		)
		(property "ki_keywords" "flyback dual secondary single aux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Wuerth*760871131*"
			(at 0 0 0)
		)
		(symbol "Wuerth_760871131_0_1")
		(symbol "Wuerth_760871131_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 0 5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at 0 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Wurth_750319177"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 4.064 5.842 0)
		)
		(property "Value" "Wurth_750319177"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Wurth_WE-AGDT-EP7"
			(at 0 -7.874 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/750319177.pdf"
			(at 2.54 10.16 0)
		)
		(property "Description" "WE-AGDT Auxiliary Gate Drive, WE-AGDT-EP7"
			(at 0 0 0)
		)
		(property "ki_keywords" "auxiliary gate drive transformer low insulation capacitance"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Wurth*WE*AGDT*EP7*"
			(at 0 0 0)
		)
		(symbol "Wurth_750319177_0_1")
		(symbol "Wurth_750319177_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -1.27 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -1.27 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 1.27 2.54 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 1.27 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZMCT103C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ZMCT103C"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Zeming_ZMCT103C"
			(at 0 0 0)
		)
		(property "Datasheet" "https://5krorwxhmqqirik.leadongcdn.com/ZMCT103C+specification-aidirBqoKomRilSjpimnokp.pdf"
			(at 0 6.985 0)
		)
		(property "Description" "Qingxian Zeming Langxi Electronic ZMCT103C current transformer 1000:1 10A"
			(at 0 0 0)
		)
		(property "ki_keywords" "current sense transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*ZMCT103C*"
			(at 0 0 0)
		)
		(symbol "ZMCT103C_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZMPT101K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TR"
			(at 0 4.445 0)
		)
		(property "Value" "ZMPT101K"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Transformer_THT:Transformer_Zeming_ZMPT101K"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://5krorwxhmqqirik.leadongcdn.com/ZMPT101K+specification-aidikBqoKomRilSkopqmikp.pdf"
			(at 1.905 7.62 0)
		)
		(property "Description" "Qingxian Zeming Langxi Electronic ZMPT101K voltage transformer 1000:1000 2mA:2mA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*ZMPT101K*"
			(at 0 0 0)
		)
		(symbol "ZMPT101K_0_1")
		(symbol "ZMPT101K_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "0433BM15A0001"
		(extends "0896BM15A0001")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "0433BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0896BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0433BM15A0001/0433BM15A0001.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "430-435MHz 1:1 RF Transformer, Unbalanced to Balanced, with integrated DC blocking capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0896BM15A0001*"
			(at 0 0 0)
		)
	)
	(symbol "0868BM15C0001"
		(extends "0896BM15A0001")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "0868BM15C0001"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0896BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0868BM15C0001/0868BM15C0001.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "863-873MHz 1:1 RF Transformer, Unbalanced to Balanced, with integrated DC blocking capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0896BM15A0001*"
			(at 0 0 0)
		)
	)
	(symbol "0915BM15A0001"
		(extends "0896BM15A0001")
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "0915BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0896BM15A0001"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0915BM15A0001/0915BM15A0001.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "902-928MHz 1:1 RF Transformer, Unbalanced to Balanced, with integrated DC blocking capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "balun rf transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0896BM15A0001*"
			(at 0 0 0)
		)
	)
	(symbol "ADT16-1T"
		(extends "ADT1-1WT-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT16-1T"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT16-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5-160MHz 1:16 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT16-6"
		(extends "ADT1.5-2")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT16-6"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT16-6+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.25-105MHz 1:16 RF Transformer, Balanced to Balanced, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
	)
	(symbol "ADT16-6T"
		(extends "ADT1-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT16-6T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT16-6T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.10-400MHz 1:16 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
	)
	(symbol "ADT2-1T-1P"
		(extends "ADT1-1WT-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT2-1T-1P"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT2-1T-1P+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-600MHz 1:2 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT2-71T"
		(extends "ADT1-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT2-71T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT2-71T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.40-500MHz 1:2 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
	)
	(symbol "ADT3-1T"
		(extends "ADT2-1T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT3-1T"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT3-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-500MHz 1:3 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT3-1T-75"
		(extends "ADT2-1T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT3-1T-75"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT3-1T-75+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-500MHz 1:3 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT4-1T"
		(extends "ADT1-1WT-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-1T"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "9-625MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT4-1WT"
		(extends "ADT1-1WT-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-1WT"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-1WT+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-775MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADT4-5WT"
		(extends "ADT1-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-5WT"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-5WT+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-650MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap, CD637"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
	)
	(symbol "ADT4-6T"
		(extends "ADT1-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-6T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-6T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5-70MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap, CD637"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
	)
	(symbol "ADT4-6WT"
		(extends "ADT3-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT4-6WT"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT4-6WT+.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-70MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap, CD637"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
	)
	(symbol "ADT8-1T"
		(extends "ADT1-6T")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT8-1T"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD637_H5.23mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT8-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-775MHz 1:8 RF Transformer, Unbalanced to Balanced Center Tap, CD637"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD637*"
			(at 0 0 0)
		)
	)
	(symbol "ADT9-1T"
		(extends "ADT1-1WT-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADT9-1T"
			(at 0 -6.985 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADT9-1T+.pdf"
			(at 0 0 0)
		)
		(property "Description" "1-250MHz 1:9 RF Transformer, Unbalanced to Balanced Center Tap, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADTL1-12"
		(extends "ADTL1-4-75")
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADTL1-12"
			(at 0 -3.81 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTL1-12+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "20-1200MHz 1:1 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADTL1-18-75"
		(extends "ADTL1-4-75")
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADTL1-18-75"
			(at 0 -3.81 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTL1-18-75+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "5-1800MHz 1:1 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADTL2-18"
		(extends "ADTL1-4-75")
		(property "Reference" "TR"
			(at 0 3.81 0)
		)
		(property "Value" "ADTL2-18"
			(at 0 -3.81 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD542_H2.84mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTL2-18+.pdf"
			(at -3.81 0 90)
		)
		(property "Description" "30-1800MHz 1:2 RF Transformer, Balanced Transmission Line, CD542"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD542*"
			(at 0 0 0)
		)
	)
	(symbol "ADTT3-2"
		(extends "ADTT1.5-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADTT3-2"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTT3-2+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2-210MHz 1:3 RF Transformer, Unbalanced to Balanced Center Tap at Primary/Secondary, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
	)
	(symbol "ADTT4-1"
		(extends "ADTT1.5-1")
		(property "Reference" "TR"
			(at 0 6.35 0)
		)
		(property "Value" "ADTT4-1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "RF_Mini-Circuits:Mini-Circuits_CD636_H4.11mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADTT4-1+.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2-120MHz 1:4 RF Transformer, Unbalanced to Balanced Center Tap at Primary/Secondary, CD636"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-Circuits RF Transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Mini?Circuits*CD636*"
			(at 0 0 0)
		)
	)
	(symbol "P0544NL"
		(extends "PA2002NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "P0544NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0173NL"
		(extends "PA2005NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA0173NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2005NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2005NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0184NL"
		(extends "PA2007NL")
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA0184NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2007NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2007NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0184NL1"
		(extends "PA2777NL")
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA0184NL1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2777NL"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2777NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0185NL"
		(extends "PA2006NL")
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA0185NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2006NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2006NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0185NL1"
		(extends "PA3493NL")
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PA0185NL1"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA3493NL"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1.25:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA3493NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0264NL"
		(extends "PA2004NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA0264NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2004NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2004NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0297NL"
		(extends "PA2002NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA0297NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 2:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA0510NL"
		(extends "PA2002NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA0510NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 2.5:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA2008NL"
		(extends "PA2002NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA2008NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 2:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
	)
	(symbol "PA2009NL"
		(extends "PA2002NL")
		(property "Reference" "T"
			(at 0 13.97 0)
		)
		(property "Value" "PA2009NL"
			(at 0 -13.97 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2002NL-PA2008NL-PA2009NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/P663.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 2.5:1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2002NL*PA2008NL*PA2009NL*"
			(at 0 0 0)
		)
	)
	(symbol "PE-68386NL"
		(extends "PA2001NL")
		(property "Reference" "T"
			(at 0 6.35 0)
		)
		(property "Value" "PE-68386NL"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Transformer_SMD:Pulse_PA2001NL"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/products/datasheets/SPM2007_61.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "SMT Gate Drive Transformer, 1:1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pulse*PA2001NL*"
			(at 0 0 0)
		)
	)
	(symbol "TG110-S050N2xx"
		(extends "TG110-E050N5xx")
		(property "Reference" "TR"
			(at 0 10.795 0)
		)
		(property "Value" "TG110-S050N2xx"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_Halo_N2_SO-16_7.11x12.7mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/discrete-ultra-100baset.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Ethernet LAN 10/100 Base-Tx Transformer"
			(at 0 0 0)
		)
		(property "ki_keywords" "single port ethernet transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*Halo*N2*"
			(at 0 0 0)
		)
	)
	(symbol "Wuerth_749013011A"
		(extends "PT61017PEL")
		(property "Reference" "TR"
			(at 0 10.795 0)
		)
		(property "Value" "Wuerth_749013011A"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Transformer_SMD:Transformer_Ethernet_Wuerth_749013011A"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.we-online.com/katalog/datasheet/749013011A.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Ethernet LAN 10/100 Base-Tx Transformer CT, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "single port ethernet transformer poe center tap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Transformer*Ethernet*Wuerth*749013011A*"
			(at 0 0 0)
		)
	)
)
