(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "2N2646"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N2646"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bucek.name/pdf/2n2646,2647.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unijunction Transistor, TO-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "UJT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
		(symbol "2N2646_0_1")
		(symbol "2N2646_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "E")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "B2")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "B1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "320S14-U"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "320S14-U"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 5.461 0)
		)
		(property "Datasheet" "https://www.thatcorp.com/datashts/THAT_300-Series_Datasheet.pdf"
			(at 0 -5.842 0)
		)
		(property "Description" "4 Matched PNP Transistors, hfe=75, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual pair pnp matched transistors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "320S14-U_0_1"
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "4")
			)
		)
		(symbol "320S14-U_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "")
				(number "3")
			)
		)
		(symbol "320S14-U_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "")
				(number "13")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "")
				(number "14")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "")
				(number "12")
			)
		)
		(symbol "320S14-U_3_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "")
				(number "5")
			)
		)
		(symbol "320S14-U_4_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA113T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA113T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 1k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA113T_0_0"
			(text "1k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA113T_0_1")
		(symbol "DTA113T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA113Z"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA113Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 1k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA113Z_0_0"
			(text "1k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA113Z_0_1")
		(symbol "DTA113Z_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA114E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA114E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA114E_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA114E_0_1")
		(symbol "DTA114E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA114G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA114G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA114G_0_0"
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA114G_0_1")
		(symbol "DTA114G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA114T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA114T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA114T_0_0"
			(text "10k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA114T_0_1")
		(symbol "DTA114T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA114W"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA114W"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/4.7k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA114W_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA114W_0_1")
		(symbol "DTA114W_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA114Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA114Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA114Y_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA114Y_0_1")
		(symbol "DTA114Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA115E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA115E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 100k/100k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA115E_0_0"
			(text "100k"
				(at -2.921 0.889 0)
			)
			(text "100k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA115E_0_1")
		(symbol "DTA115E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA115G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA115G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k/100k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA115G_0_0"
			(text "100k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA115G_0_1")
		(symbol "DTA115G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA115T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA115T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 100k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA115T_0_0"
			(text "100k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA115T_0_1")
		(symbol "DTA115T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA115U"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA115U"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 100k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA115U_0_0"
			(text "100k"
				(at -2.921 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA115U_0_1")
		(symbol "DTA115U_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA123E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA123E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/2k2, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA123E_0_0"
			(text "2k2"
				(at -2.921 0.889 0)
			)
			(text "2k2"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA123E_0_1")
		(symbol "DTA123E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA123J"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA123J"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA123J_0_0"
			(text "2k2"
				(at -2.921 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA123J_0_1")
		(symbol "DTA123J_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA123Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA123Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA123Y_0_0"
			(text "2k2"
				(at -2.921 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA123Y_0_1")
		(symbol "DTA123Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA124E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA124E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 22k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA124E_0_0"
			(text "22k"
				(at -2.921 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA124E_0_1")
		(symbol "DTA124E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA124G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA124G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA124G_0_0"
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA124G_0_1")
		(symbol "DTA124G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA124T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA124T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 22k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA124T_0_0"
			(text "22k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA124T_0_1")
		(symbol "DTA124T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA124X"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA124X"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 22k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA124X_0_0"
			(text "22k"
				(at -2.921 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA124X_0_1")
		(symbol "DTA124X_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA125T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA125T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 200k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA125T_0_0"
			(text "200k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA125T_0_1")
		(symbol "DTA125T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA143E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA143E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/4k7, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA143E_0_0"
			(text "4k7"
				(at -2.921 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA143E_0_1")
		(symbol "DTA143E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA143T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA143T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA143T_0_0"
			(text "4k7"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA143T_0_1")
		(symbol "DTA143T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA143X"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA143X"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA143X_0_0"
			(text "4k7"
				(at -2.921 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA143X_0_1")
		(symbol "DTA143X_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA143Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA143Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA143Y_0_0"
			(text "4k7"
				(at -2.921 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA143Y_0_1")
		(symbol "DTA143Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA143Z"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA143Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA143Z_0_0"
			(text "4k7"
				(at -2.921 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA143Z_0_1")
		(symbol "DTA143Z_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA144E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA144E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 47k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA144E_0_0"
			(text "47k"
				(at -2.921 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA144E_0_1")
		(symbol "DTA144E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA144G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA144G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA144G_0_0"
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA144G_0_1")
		(symbol "DTA144G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA144T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA144T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 47k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA144T_0_0"
			(text "47k"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTA144T_0_1")
		(symbol "DTA144T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA144V"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA144V"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 47k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA144V_0_0"
			(text "47k"
				(at -2.921 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA144V_0_1")
		(symbol "DTA144V_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA144W"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA144W"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 47k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA144W_0_0"
			(text "47k"
				(at -2.921 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA144W_0_1")
		(symbol "DTA144W_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA1D3R"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA1D3R"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k7/1k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA1D3R_0_0"
			(text "2k7"
				(at -2.921 0.889 0)
			)
			(text "1k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA1D3R_0_1")
		(symbol "DTA1D3R_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTA214Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTA214Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTA214Y_0_0"
			(text "10k"
				(at -2.921 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTA214Y_0_1")
		(symbol "DTA214Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB113E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB113E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 1k/1k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB113E_0_0"
			(text "1k"
				(at -3.302 0.889 0)
			)
			(text "1k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTB113E_0_1")
		(symbol "DTB113E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB122J"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB122J"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k22/4k7, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB122J_0_0"
			(text "220R"
				(at -3.302 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTB122J_0_1")
		(symbol "DTB122J_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB123E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB123E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/2k2, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB123E_0_0"
			(text "2k2"
				(at -3.302 0.889 0)
			)
			(text "2k2"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTB123E_0_1")
		(symbol "DTB123E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB123T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB123T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB123T_0_0"
			(text "2k2"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTB123T_0_1")
		(symbol "DTB123T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB123Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB123Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 2k2/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB123Y_0_0"
			(text "2k2"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTB123Y_0_1")
		(symbol "DTB123Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB133H"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB133H"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 3k3/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB133H_0_0"
			(text "3k3"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTB133H_0_1")
		(symbol "DTB133H_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTB163T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB163T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 6k8/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTB163T_0_0"
			(text "6k8"
				(at -2.921 0.889 0)
			)
		)
		(symbol "DTB163T_0_1")
		(symbol "DTB163T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC113T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC113T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 1k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC113T_0_0"
			(text "1k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC113T_0_1")
		(symbol "DTC113T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC113Z"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC113Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 1k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC113Z_0_0"
			(text "1k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC113Z_0_1")
		(symbol "DTC113Z_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC114E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC114E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC114E_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC114E_0_1")
		(symbol "DTC114E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC114G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC114G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC114G_0_0"
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC114G_0_1")
		(symbol "DTC114G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC114T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC114T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC114T_0_0"
			(text "10k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC114T_0_1")
		(symbol "DTC114T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC114W"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC114W"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/4k7, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC114W_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC114W_0_1")
		(symbol "DTC114W_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC114Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC114Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC114Y_0_0"
			(text "10k"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC114Y_0_1")
		(symbol "DTC114Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC115E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC115E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 100k/100k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC115E_0_0"
			(text "100k"
				(at -3.302 0.889 0)
			)
			(text "100k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC115E_0_1")
		(symbol "DTC115E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC115G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC115G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k/100k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC115G_0_0"
			(text "100k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC115G_0_1")
		(symbol "DTC115G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC115T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC115T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 100k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC115T_0_0"
			(text "100k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC115T_0_1")
		(symbol "DTC115T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC115U"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC115U"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 100k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC115U_0_0"
			(text "100k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC115U_0_1")
		(symbol "DTC115U_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC123E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC123E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/2k2, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC123E_0_0"
			(text "2k2"
				(at -3.302 0.889 0)
			)
			(text "2k2"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC123E_0_1")
		(symbol "DTC123E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC123J"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC123J"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC123J_0_0"
			(text "2k2"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC123J_0_1")
		(symbol "DTC123J_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC123Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC123Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC123Y_0_0"
			(text "2k2"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC123Y_0_1")
		(symbol "DTC123Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC124E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC124E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 22k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC124E_0_0"
			(text "22k"
				(at -3.302 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC124E_0_1")
		(symbol "DTC124E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC124G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC124G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC124G_0_0"
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC124G_0_1")
		(symbol "DTC124G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC124T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC124T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 22k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC124T_0_0"
			(text "22k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC124T_0_1")
		(symbol "DTC124T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC124X"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC124X"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 22k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC124X_0_0"
			(text "22k"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC124X_0_1")
		(symbol "DTC124X_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC125T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC125T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 200k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC125T_0_0"
			(text "200k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC125T_0_1")
		(symbol "DTC125T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC143E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC143E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/4k7, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC143E_0_0"
			(text "4k7"
				(at -3.302 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC143E_0_1")
		(symbol "DTC143E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC143T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC143T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC143T_0_0"
			(text "4k7"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC143T_0_1")
		(symbol "DTC143T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC143X"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC143X"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC143X_0_0"
			(text "4k7"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC143X_0_1")
		(symbol "DTC143X_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC143Y"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC143Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC143Y_0_0"
			(text "4k7"
				(at -3.302 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC143Y_0_1")
		(symbol "DTC143Y_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC143Z"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC143Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC143Z_0_0"
			(text "4k7"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC143Z_0_1")
		(symbol "DTC143Z_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC144E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC144E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 47k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC144E_0_0"
			(text "47k"
				(at -3.302 0.889 0)
			)
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC144E_0_1")
		(symbol "DTC144E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC144G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC144G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC144G_0_0"
			(text "47k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC144G_0_1")
		(symbol "DTC144G_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC144T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC144T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 47k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC144T_0_0"
			(text "47k"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTC144T_0_1")
		(symbol "DTC144T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC144V"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC144V"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 47k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC144V_0_0"
			(text "47k"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC144V_0_1")
		(symbol "DTC144V_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC144W"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC144W"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 47k/22k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC144W_0_0"
			(text "47k"
				(at -3.302 0.889 0)
			)
			(text "22k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC144W_0_1")
		(symbol "DTC144W_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTC1D3R"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC1D3R"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k7/1k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTC1D3R_0_0"
			(text "2k7"
				(at -3.302 0.889 0)
			)
			(text "1k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTC1D3R_0_1")
		(symbol "DTC1D3R_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTD113E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD113E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 1k/1k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTD113E_0_0"
			(text "1k"
				(at -3.302 0.889 0)
			)
			(text "1k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTD113E_0_1")
		(symbol "DTD113E_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTD122J"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD122J"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k22/4k7, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTD122J_0_0"
			(text "220R"
				(at -3.302 0.889 0)
			)
			(text "4k7"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTD122J_0_1")
		(symbol "DTD122J_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTD123T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD123T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTD123T_0_0"
			(text "2k2"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTD123T_0_1")
		(symbol "DTD123T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTD133H"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD133H"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 3k3/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTD133H_0_0"
			(text "3k3"
				(at -3.302 0.889 0)
			)
			(text "10k"
				(at -2.159 -1.524 900)
			)
		)
		(symbol "DTD133H_0_1")
		(symbol "DTD133H_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DTD163T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD163T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 6k8/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
		(symbol "DTD163T_0_0"
			(text "6k8"
				(at -3.048 0.889 0)
			)
		)
		(symbol "DTD163T_0_1")
		(symbol "DTD163T_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAT02"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MAT02"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-78-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.elenota.pl/datasheet_download/93431/MAT02"
			(at 0 0 0)
		)
		(property "Description" "20mA Ic, 40V Vce, Precision Dual Monolithic Low Noise, Low Offset Transistor, TO-78"
			(at 0 0 0)
		)
		(property "ki_keywords" "Precision Dual Monolithic Transistor Low Noise EOL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?78*"
			(at 0 0 0)
		)
		(symbol "MAT02_0_1")
		(symbol "MAT02_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(symbol "MAT02_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_C2C1E1E2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_C2C1E1E2"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at -2.54 0 0)
		)
		(property "Description" "Double NPN transistors, current mirror configuration"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_C2C1E1E2_0_1")
		(symbol "Q_Dual_NPN_C2C1E1E2_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "C2")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at 5.08 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_B1E2B2C2E1C1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_B1E2B2C2E1C1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_B1E2B2C2E1C1_0_1")
		(symbol "Q_Dual_NPN_NPN_B1E2B2C2E1C1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "5")
			)
		)
		(symbol "Q_Dual_NPN_NPN_B1E2B2C2E1C1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN bias resistor transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN bias resistor transistor without a base-emitter resistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1_0_1")
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "6")
			)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN bias resistor transistor without a base-emitter resistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_C1E1C2E2B2B1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_C1E1C2E2B2B1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_C1E1C2E2B2B1_0_1")
		(symbol "Q_Dual_NPN_NPN_C1E1C2E2B2B1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "2")
			)
		)
		(symbol "Q_Dual_NPN_NPN_C1E1C2E2B2B1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_NPN_E1B1C2E2B2C1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_NPN_E1B1C2E2B2C1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_NPN_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_NPN_NPN_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_NPN_NPN_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_PNP_B1E2B2C2E1C1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_PNP_B1E2B2C2E1C1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN/PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_PNP_B1E2B2C2E1C1_0_1")
		(symbol "Q_Dual_NPN_PNP_B1E2B2C2E1C1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "5")
			)
		)
		(symbol "Q_Dual_NPN_PNP_B1E2B2C2E1C1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN/PNP bias resistor transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NPN_PNP_E1B1C2E2B2C1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_NPN_PNP_E1B1C2E2B2C1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN/PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NPN_PNP_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_NPN_PNP_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_NPN_PNP_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_C2C1E1E2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_C2C1E1E2"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at -2.54 0 0)
		)
		(property "Description" "Double PNP transistors, current mirror configuration"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_C2C1E1E2_0_1")
		(symbol "Q_Dual_PNP_C2C1E1E2_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "E2")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "C2")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "E1")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 90)
				(length 2.54)
				(name "C1")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_NPN_BRT_E1B1C2E2B2C1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_NPN_BRT_E1B1C2E2B2C1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP/NPN bias resistor transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_NPN_BRT_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_PNP_NPN_BRT_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_PNP_NPN_BRT_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP bias resistor transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_PNP_C1B1B2C2E2E1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_PNP_C1B1B2C2E2E1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_PNP_C1B1B2C2E2E1_0_1")
		(symbol "Q_Dual_PNP_PNP_C1B1B2C2E2E1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "6")
			)
		)
		(symbol "Q_Dual_PNP_PNP_C1B1B2C2E2E1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_PNP_C1E1C2E2B2B1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_PNP_C1E1C2E2B2B1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_PNP_C1E1C2E2B2B1_0_1")
		(symbol "Q_Dual_PNP_PNP_C1E1C2E2B2B1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "2")
			)
		)
		(symbol "Q_Dual_PNP_PNP_C1E1C2E2B2B1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PNP_PNP_E1B1C2E2B2C1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_Dual_PNP_PNP_E1B1C2E2B2C1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PNP_PNP_E1B1C2E2B2C1_0_1")
		(symbol "Q_Dual_PNP_PNP_E1B1C2E2B2C1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "1")
			)
		)
		(symbol "Q_Dual_PNP_PNP_E1B1C2E2B2C1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_BCE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_BCE"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, base/collector/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_BCE_0_1")
		(symbol "Q_NPN_BCE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_BCEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_BCEC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, base/collector/emitter, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_BCEC_0_1")
		(symbol "Q_NPN_BCEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_BEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_BEC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_BEC_0_1")
		(symbol "Q_NPN_BEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_BRT_BEC"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_NPN_BRT_BEC"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN bias resistor transistor, base/emitter/collector"
			(at -3.81 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_BRT_BEC_0_1")
		(symbol "Q_NPN_BRT_BEC_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_BRT_ECB"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_NPN_BRT_ECB"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, emitter/collector/base"
			(at 3.81 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_BRT_ECB_0_1")
		(symbol "Q_NPN_BRT_ECB_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_CBE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_CBE"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, collector/base/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_CBE_0_1")
		(symbol "Q_NPN_CBE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_CEB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_CEB"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, collector/emitter/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_CEB_0_1")
		(symbol "Q_NPN_CEB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_BCE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_BCE"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, base/collector/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_BCE_0_1")
		(symbol "Q_NPN_Darlington_BCE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_BCEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.588 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_BCEC"
			(at 5.588 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, base/collector/emitter, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_BCEC_0_1")
		(symbol "Q_NPN_Darlington_BCEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_BEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_BEC"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, base/emitter/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_BEC_0_1")
		(symbol "Q_NPN_Darlington_BEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_CBE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_CBE"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, collector/base/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_CBE_0_1")
		(symbol "Q_NPN_Darlington_CBE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_CEB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_CEB"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, collector/emitter/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_CEB_0_1")
		(symbol "Q_NPN_Darlington_CEB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_EBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_EBC"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, emitter/base/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_EBC_0_1")
		(symbol "Q_NPN_Darlington_EBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_ECB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_ECB"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, emitter/collector/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_ECB_0_1")
		(symbol "Q_NPN_Darlington_ECB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_Darlington_ECBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.588 1.27 0)
		)
		(property "Value" "Q_NPN_Darlington_ECBC"
			(at 5.588 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, emitter/collector/base, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_Darlington_ECBC_0_1")
		(symbol "Q_NPN_Darlington_ECBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_EBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_EBC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, emitter/base/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_EBC_0_1")
		(symbol "Q_NPN_EBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_ECB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_ECB"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, emitter/collector/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_ECB_0_1")
		(symbol "Q_NPN_ECB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NPN_ECBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_NPN_ECBC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "NPN transistor, emitter/collector/base, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_NPN_ECBC_0_1")
		(symbol "Q_NPN_ECBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_BCE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_BCE"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, base/collector/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_BCE_0_1")
		(symbol "Q_PNP_BCE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_BCEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_BCEC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, base/collector/emitter, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_BCEC_0_1")
		(symbol "Q_PNP_BCEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_BEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_BEC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, base/emitter/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_BEC_0_1")
		(symbol "Q_PNP_BEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_BRT_BEC"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_PNP_BRT_BEC"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP bias resistor transistor, base/emitter/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_BRT_BEC_0_1")
		(symbol "Q_PNP_BRT_BEC_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_BRT_ECB"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "Q_PNP_BRT_ECB"
			(at 3.81 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP bias resistor transistor, emitter/collector/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_BRT_ECB_0_1")
		(symbol "Q_PNP_BRT_ECB_1_1"
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 1.27 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_CBE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_CBE"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, collector/base/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_CBE_0_1")
		(symbol "Q_PNP_CBE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_CEB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_CEB"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, collector/emitter/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_CEB_0_1")
		(symbol "Q_PNP_CEB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_BCE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_BCE"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, base/collector/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_BCE_0_1")
		(symbol "Q_PNP_Darlington_BCE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_BCEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.588 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_BCEC"
			(at 5.588 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, base/collector/emitter, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_BCEC_0_1")
		(symbol "Q_PNP_Darlington_BCEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_BEC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_BEC"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, base/emitter/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_BEC_0_1")
		(symbol "Q_PNP_Darlington_BEC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_CBE"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_CBE"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, collector/base/emitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_CBE_0_1")
		(symbol "Q_PNP_Darlington_CBE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_CEB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_CEB"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, collector/emitter/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_CEB_0_1")
		(symbol "Q_PNP_Darlington_CEB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_EBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_EBC"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, emitter/base/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_EBC_0_1")
		(symbol "Q_PNP_Darlington_EBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_ECB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_ECB"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, emitter/collector/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_ECB_0_1")
		(symbol "Q_PNP_Darlington_ECB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_Darlington_ECBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.588 1.27 0)
		)
		(property "Value" "Q_PNP_Darlington_ECBC"
			(at 5.588 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP Darlington transistor, emitter/collector/base, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_Darlington_ECBC_0_1")
		(symbol "Q_PNP_Darlington_ECBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_EBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_EBC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, emitter/base/collector"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_EBC_0_1")
		(symbol "Q_PNP_EBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_ECB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_ECB"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, emitter/collector/base"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_ECB_0_1")
		(symbol "Q_PNP_ECB_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PNP_ECBC"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "Q_PNP_ECBC"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "PNP transistor, emitter/collector/base, collector connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "BJT"
			(at 0 0 0)
		)
		(symbol "Q_PNP_ECBC_0_1")
		(symbol "Q_PNP_ECBC_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2210"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SSM2210"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/SSM2210.pdf"
			(at 0 0 0)
		)
		(property "Description" "Audio Dual Matched NPN transistor, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio npn dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm* DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2210_0_1")
		(symbol "SSM2210_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "3")
			)
		)
		(symbol "SSM2210_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SSM2220"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SSM2220"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/SSM2220.pdf"
			(at 0 0 0)
		)
		(property "Description" "Audio Dual Matched PNP transistor, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio pnp dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm* DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SSM2220_0_1")
		(symbol "SSM2220_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E1")
				(number "3")
			)
		)
		(symbol "SSM2220_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B2")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C2")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TIP120"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP120"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 60V Vce, Silicon Darlington Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TIP120_0_1")
		(symbol "TIP120_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 3.81)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.667)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TIP125"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP125"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 60V Vce, Silicon Darlington Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TIP125_0_1")
		(symbol "TIP125_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 3.81)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.667)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2N2219"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N2219"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/2N2219-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "800mA Ic, 50V Vce, NPN Transistor, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "2N2647"
		(extends "2N2646")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N2647"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bucek.name/pdf/2n2646,2647.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unijunction Transistor, TO-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "UJT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "2N3055"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N3055"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/2N3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "15A Ic, 60V Vce, Power NPN Transistor, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "2N3904"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N3904"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2N3905"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N3905"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nteinc.com/specs/original/2N3905_06.pdf"
			(at 0 0 0)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2N3906"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N3906"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2SA1015"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SA1015"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.datasheetcatalog.org/datasheet/toshiba/905.pdf"
			(at 0 0 0)
		)
		(property "Description" "-0.15A Ic, -50V Vce, Low Noise Audio PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Audio PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2SB631"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SB631"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/sanyo/ds_pdf_e/2SB631.pdf"
			(at 0 0 0)
		)
		(property "Description" "-1A Ic, -100V Vce, High Voltage Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "2SB817"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SB817"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3PB-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://skory.gylcomp.hu/alkatresz/2SB817.pdf"
			(at 0 0 0)
		)
		(property "Description" "-12A Ic, -140V Vce, Silicon Power PNP Transistors, TO-3PB"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3PB*"
			(at 0 0 0)
		)
	)
	(symbol "2SC1815"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SC1815"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Toshiba%20PDFs/2SC1815.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.15A Ic, 50V Vce, Low Noise Audio NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Noise Audio NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2SC1941"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SC1941"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://rtellason.com/transdata/2sc1941.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Ic, 160V Vce, Audio High Voltage NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Audio High Voltage NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2SC1945"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SC1945"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://rtellason.com/transdata/2sc1945.pdf"
			(at 0 0 0)
		)
		(property "Description" "6A Ic, 80V Vce, Silicon 27MHz RF Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "2SC4213"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SC4213"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=19305&prodName=2SC4213"
			(at 0 0 0)
		)
		(property "Description" "0.3A Ic, 20V Vce, NPN Transistor, For Muting and Switching, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "2SD1047"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "2SD1047"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3PB-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/2sd1047.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 140V Vce, Silicon Power NPN Transistors, TO-3PB"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3PB*"
			(at 0 0 0)
		)
	)
	(symbol "2SD600"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2SD600"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/sanyo/ds_pdf_e/2SB631.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 100V Vce, High Voltage Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage Power Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BC107"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC107"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Transistor/BC108.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 50V Vce, Low Noise General Purpose NPN Transistor, TO-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN low noise transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "BC108"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC108"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Transistor/BC108.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Low Noise General Purpose NPN Transistor, TO-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN low noise transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "BC109"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC109"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/296634.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2A Ic, 25V Vce, Low Noise General Purpose NPN Transistor, TO-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN low noise transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "BC140"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC140"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/296634.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "BC141"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC141"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/296634.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 60V Vce, NPN Transistor, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "BC160"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC160"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1697389.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 40V Vce, Power PNP Transistor, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "BC161"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC161"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-39-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1697389.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 60V Vce, Power PNP Transistor, TO-39"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?39*"
			(at 0 0 0)
		)
	)
	(symbol "BC212"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC212"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Fairchild%20PDFs/BC212.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.3A Ic, 50V Vce, PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC237"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC237"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC237-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA Ic, 50V Vce, Epitaxial Silicon NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Epitaxial Silicon NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC240"
		(extends "Q_NPN_CEB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC240"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BF420-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "50mA Ic, 40V Vce, RF Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC307"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC307"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC307-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA Ic, 45V Vce, Epitaxial Silicon PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "Epitaxial Silicon PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC327"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC327"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC327-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC328"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC328"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.redrok.com/PNP_BC327_-45V_-800mA_0.625W_Hfe100_TO-92.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC337"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC337"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC338"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC338"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC413"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC413"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC413B"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC413B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC413C"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC413C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC414"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC414"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC414B"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC414B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC414C"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC414C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bc413_14_b_c.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC516"
		(extends "Q_PNP_Darlington_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC516"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC516-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 30V Vce, Darlington PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Darlington Darl Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC517"
		(extends "Q_NPN_Darlington_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC517"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC517-D74Z-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 30V Vce, Darlington NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington Darl Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC546"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC546"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC550-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 65V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC547"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC547"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC550-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC548"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC548"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC550-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC549"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC549"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC550-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC550"
		(extends "Q_NPN_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC550"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC550-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC556"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC556"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC556BTA-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 65V Vce, PNP Small Signal Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC557"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC557"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC556BTA-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC558"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC558"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC556BTA-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC559"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC559"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC556BTA-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC560"
		(extends "Q_PNP_CBE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC560"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC556BTA-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC636"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC636"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC636-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 45V Vce, PNP Medium Power Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BC807"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC807"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC808-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC807W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC807W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC808-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, PNP Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC808"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC808"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC808-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC808W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC808W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC808-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, PNP Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC817"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC817"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC817W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC817W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC818"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC818"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC818W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC818W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.8A Ic, 25V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC846"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC846"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846_SER.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 65V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC846BDW1"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC846BDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC846BDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC846BPDW1"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC846BPDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC846BPDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC846BPN"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC846BPN"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846BPN.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC846BS"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC846BS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846BS.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC847"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC847"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC847BDW1"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC847BDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC846BDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC847BPDW1"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC847BPDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC846BPDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC847BPN"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC847BPN"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC847BPN.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC847BS"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC847BS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC847BS.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC847W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC847W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC848"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC848"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC848W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC848W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC849"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC849"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC849W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC849W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC850"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC850"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC850W"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC850W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Small Signal Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC856"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC856"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 65V Vce, PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC856BDW1"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC856BDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC856BDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC856BS"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC856BS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC856BS.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 65V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC856W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC856W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 65V Vce, PNP Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC857"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC857"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC857BDW1"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC857BDW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BC856BDW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC857BS"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BC857BS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC857BS.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 45V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BC857W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC857W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC858"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC858"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC860-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC858W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC858W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC859"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC859"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC859W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC859W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 30V Vce, PNP Small Signal Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BC860"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC860"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BC860W"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BC860W"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC857SERIES_BC858SERIES_BC859SERIES_BC860SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541da0e3a1661"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BCP51"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCP51"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BCP51-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 45V Vce, PNP Medium Power Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "BCP53"
		(extends "Q_PNP_BCEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCP53"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BCP53T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 80V Vce, PNP Medium Power Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "BCP56"
		(extends "Q_NPN_BCEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCP56"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BCP56_BCX56_BC56PA.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 80V Vce, NPN Medium Power Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "BCV29"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "BCV29"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BCV29_49.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, 30Vce, 500mA, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NPN Darlington"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BCV49"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 4.572 1.27 0)
		)
		(property "Value" "BCV49"
			(at 4.572 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BCV29_49.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN Darlington transistor, 60Vce, 500mA, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NPN Darlington"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BCV61"
		(extends "Q_Dual_NPN_C2C1E1E2")
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "BCV61"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BCV61.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "100mA IC, 30V Vce, Double NPN Transistors, Current mirror configuration, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Transistor Double NPN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?143*"
			(at 0 0 0)
		)
	)
	(symbol "BCV62"
		(extends "Q_Dual_PNP_C2C1E1E2")
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "BCV62"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BCV62.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "100mA IC, 30V Vce, Double PNP Transistors, Current mirror configuration, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Transistor Double PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?143*"
			(at 0 0 0)
		)
	)
	(symbol "BCX51"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCX51"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/bcx51_bcx52_bcx53.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 45V Vce, PNP Medium Power Transistor, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BCX52"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCX52"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/bcx51_bcx52_bcx53.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 60V Vce, PNP Medium Power Transistor, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BCX53"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCX53"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/bcx51_bcx52_bcx53.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 80V Vce, PNP Medium Power Transistor, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BCX56"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BCX56"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BCP56_BCX56_BC56PA.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 80V Vce, NPN Medium Power Transistor, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "BD135"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD135"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 45V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD136"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD136"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 45V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD137"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD137"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 60V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD138"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD138"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 60V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD139"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD139"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD140"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD140"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001225.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD233"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD233"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Micro%20Commercial%20PDFs/BD233,235,237.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Ic, 45V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD234"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD234"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.electronica-pt.com/datasheets/bd/BD234.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Ic, 45V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD235"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD235"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Micro%20Commercial%20PDFs/BD233,235,237.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Ic, 60V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD236"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD236"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.electronica-pt.com/datasheets/bd/BD234.pdf"
			(at 0 0 0)
		)
		(property "Description" "60V Vce, 2A, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD237"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD237"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Micro%20Commercial%20PDFs/BD233,235,237.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD238"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD238"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.electronica-pt.com/datasheets/bd/BD234.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A Ic, 80V Vce, Low Voltage Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD249"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD249"
			(at 6.35 0 0)
		)
		(property "Footprint" ""
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 55V Vce, Silicon Power NPN Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD249A"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD249A"
			(at 6.35 0 0)
		)
		(property "Footprint" ""
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 70V Vce, Silicon Power NPN Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD249B"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD249B"
			(at 6.35 0 0)
		)
		(property "Footprint" ""
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 90V Vce, Silicon Power NPN Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD249C"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD249C"
			(at 6.35 0 0)
		)
		(property "Footprint" ""
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 115V Vce, Silicon Power NPN Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD250"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.207 1.778 0)
		)
		(property "Value" "BD250"
			(at 5.207 -0.127 0)
		)
		(property "Footprint" ""
			(at 5.207 -2.032 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 55V Vce, Silicon Power PNP Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD250A"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.207 1.778 0)
		)
		(property "Value" "BD250A"
			(at 5.207 -0.127 0)
		)
		(property "Footprint" ""
			(at 5.207 -2.032 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 70V Vce, Silicon Power PNP Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD250B"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.207 1.778 0)
		)
		(property "Value" "BD250B"
			(at 5.207 -0.127 0)
		)
		(property "Footprint" ""
			(at 5.207 -2.032 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 90V Vce, Silicon Power PNP Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD250C"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.207 1.778 0)
		)
		(property "Value" "BD250C"
			(at 5.207 -0.127 0)
		)
		(property "Footprint" ""
			(at 5.207 -2.032 0)
		)
		(property "Datasheet" "http://www.mospec.com.tw/pdf/power/BD249.pdf"
			(at 0 0 0)
		)
		(property "Description" "25A Ic, 115V Vce, Silicon Power PNP Transistors, SOT-93/TO247"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218* TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "BD433"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD433"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 22V Vce, Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD434"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD434"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 22V Vce, Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD435"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD435"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 32V Vce, Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD436"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD436"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 32V Vce, Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD437"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD437"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 45V Vce, Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD438"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD438"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 45V Vce, Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD439"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD439"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 60V Vce, Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD440"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD440"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 60V Vce, Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD441"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD441"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 80V Vce, Power NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD442"
		(extends "Q_PNP_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BD442"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.cdil.com/datasheets/bd433_42.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 80V Vce, Power PNP Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BD909"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD909"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001277.pdf"
			(at 0 0 0)
		)
		(property "Description" "15A, Silicon Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BD910"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD910"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001277.pdf"
			(at 0 0 0)
		)
		(property "Description" "15A, Silicon Power PNP Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BD911"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD911"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001277.pdf"
			(at 0 0 0)
		)
		(property "Description" "15A, Silicon Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BD912"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "BD912"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00001277.pdf"
			(at 0 0 0)
		)
		(property "Description" "BD910, 15A, Silicon Power PNP Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW93"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW93"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BDW93C-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 45V Vce, Power Darlington NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW93A"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW93A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BDW93C-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 60V Vce, Power Darlington NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW93B"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW93B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BDW93C-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 80V Vce, Power Darlington NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW93C"
		(extends "Q_NPN_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW93C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BDW93C-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 100V Vce, Power Darlington NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW94"
		(extends "Q_PNP_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW94"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bourns.com/data/global/pdfs/bdw94.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 45V Vce, Power Darlington PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW94A"
		(extends "Q_PNP_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW94A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bourns.com/data/global/pdfs/bdw94.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 60V Vce, Power Darlington PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW94B"
		(extends "Q_PNP_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW94B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bourns.com/data/global/pdfs/bdw94.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 80V Vce, Power Darlington PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BDW94C"
		(extends "Q_PNP_Darlington_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BDW94C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.bourns.com/data/global/pdfs/bdw94.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 100V Vce, Power Darlington PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BF199"
		(extends "Q_NPN_CEB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF199"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/BF199.pdf"
			(at 0 0 0)
		)
		(property "Description" "50mA Ic, 25V Vce, NPN Radio Frequency Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BF457"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF457"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.pcpaudio.com/pcpfiles/transistores/BF457-8-9.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 160V Vce, High Voltage NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN HV High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BF458"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF458"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.pcpaudio.com/pcpfiles/transistores/BF457-8-9.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 250V Vce, High Voltage NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN HV High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BF459"
		(extends "Q_NPN_ECB")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF459"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.pcpaudio.com/pcpfiles/transistores/BF457-8-9.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.1A Ic, 300V Vce, High Voltage NPN Transistor, TO-126"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN HV High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "BFR92"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BFR92"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BFR92A_N.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.025A Ic, 15V Vce, 5GHz Wideband NPN Transistor, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF 5GHz NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "BFT92"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BFT92"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BFT92_CNV.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.025A Ic, 15V Vce, 5GHz Wideband PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF 5GHz NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BUT11"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUT11"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BUT11A-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 400V Vce, Silicon Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BUT11A"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUT11A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BUT11A-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 450V Vce, Silicon Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Voltage Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "DMMT5401"
		(extends "Q_Dual_PNP_PNP_C1B1B2C2E2E1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "DMMT5401"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30437.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DTB113Z"
		(extends "DTA113Z")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB113Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 1k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTB114E"
		(extends "DTA114E")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB114E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTB114G"
		(extends "DTA114G")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB114G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 0k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTB114T"
		(extends "DTA114T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB114T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 10k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTB143T"
		(extends "DTA143T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTB143T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital PNP Transistor, 4k7/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTC214Y"
		(extends "DTC114Y")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTC214Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/47k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD113Z"
		(extends "DTC113Z")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD113Z"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 1k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD114E"
		(extends "DTC114E")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD114E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD114G"
		(extends "DTC114G")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD114G"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 0k/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD114T"
		(extends "DTC114T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD114T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 10k/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD123E"
		(extends "DTC123E")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD123E"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/2k2, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD123Y"
		(extends "DTC123Y")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD123Y"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 2k2/10k, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "DTD143T"
		(extends "DTC143T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DTD143T"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Digital NPN Transistor, 4k7/NONE, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROHM Digital NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SC?59*"
			(at 0 0 0)
		)
	)
	(symbol "EMH3"
		(extends "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "EMH3"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/transistor/digital/emh3t2r-e.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "0.1A Ic, 50V Vce, Dual NPN Input Resistor Transistors, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "FFB2222A"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB2222A"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMPQ2222A-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FFB2227A"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB2227A"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FMB2227A-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "500mA IC, 30V Vce, Dual NPN/PNP Transistors, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FFB3904"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB3904"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMPQ3904-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FFB3906"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB3906"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMPQ3906-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FFB3946"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB3946"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FMB3946-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FFB5551"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FFB5551"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FFB5551-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 160V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FMB2227A"
		(extends "Q_Dual_NPN_PNP_B1E2B2C2E1C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FMB2227A"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SuperSOT-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FMB2227A-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "500mA IC, 30V Vce, Dual NPN/PNP Transistors, SuperSOT-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SuperSOT*"
			(at 0 0 0)
		)
	)
	(symbol "FMB3946"
		(extends "Q_Dual_NPN_PNP_B1E2B2C2E1C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "FMB3946"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SuperSOT-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FMB3946-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/PNP Transistors, SuperSOT-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SuperSOT*"
			(at 0 0 0)
		)
	)
	(symbol "IMH3A"
		(extends "Q_Dual_NPN_NPN_BRT_No_R2_C1B2E2C2B1E1")
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "IMH3A"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:ROHM_SOT-457_ClockwisePinNumbering"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/transistor/digital/emh3t2r-e.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "0.1A Ic, 50V Vce, Dual NPN Input Resistor Transistors, SOT-457"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ROHM*SOT?457*"
			(at 0 0 0)
		)
	)
	(symbol "KTD1624"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "KTD1624"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www2.kec.co.kr/data/databook/pdf/KTD/Eng/KTD1624.pdf"
			(at 0 0 0)
		)
		(property "Description" "Epitaxial Planar NPN Transistor, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "MBT2222ADW1T1"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MBT2222ADW1T1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBT2222ADW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "600mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MBT3904DW1"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MBT3904DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBT3904DW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MBT3906DW1"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MBT3906DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBT3906DW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MBT3946DW1T1"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MBT3946DW1T1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MBT3946DW1T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MJ2955"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MJ2955"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-3"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/2N3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "-15A Ic, -60V Vce, Power PNP Transistor, TO-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?3*"
			(at 0 0 0)
		)
	)
	(symbol "MJE13003"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MJE13003"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-126-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13003-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1.5A Ic, 400V Vce, Silicon Switching Power NPN Transistor, TO-225"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Power High Voltage NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?126*"
			(at 0 0 0)
		)
	)
	(symbol "MJE13005G"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "MJE13005G"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13005-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "4A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MJE13007G"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "MJE13007G"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13007-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MJE13009G"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "MJE13009G"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MJE13009-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "12A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "MMBT2222A"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBT2222A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/MMBT2222A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA Ic, 40V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBT3904"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBT3904"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBT3906"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBT3906"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3906-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBT5550L"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBT5550L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "www.onsemi.com/pub/Collateral/MMBT5550LT1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.6A Ic, 140V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBT5551L"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBT5551L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "www.onsemi.com/pub/Collateral/MMBT5550LT1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.6A Ic, 160V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA06"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA06"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/mmbta06.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 80V Vce, general purpose NPN"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA42"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA42"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBTA42LT1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, NPN High Voltage Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA44"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA44"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/mmbta42.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.3A Ic, 400V Vce, NPN High Voltage Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA56"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA56"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/mmbta56.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 80V Vce, general purpose PNP"
			(at 1.27 0 0)
		)
		(property "ki_keywords" "SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA92"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA92"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBTA92LT1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, PNP High Voltage Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBTA94"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBTA94"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://diotec.com/request/datasheet/mmbta92.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.3A Ic, 400V Vce, PNP High Voltage Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT2222A"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT2222A"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30125.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT3904"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT3904"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30088.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT3906"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT3906"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30124.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT3946"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT3946"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30123.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT5401"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT5401"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30169.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 160V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDT5551"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MMDT5551"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds30172.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 160V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "MMDTA06"
		(extends "Q_Dual_NPN_NPN_B1E2B2C2E1C1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMDTA06"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-74-6_1.55x2.9mm_P0.95mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/MMDTA06.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "500mA IC, 80V Vce, Dual NPN transistor, SC-74"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual transistor NPN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?74*"
			(at 0 0 0)
		)
	)
	(symbol "MPSA42"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MPSA42"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MPSA42-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, NPN High Voltage Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MPSA92"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MPSA92"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MPSA92-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, PNP High Voltage Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5111DW1"
		(extends "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5111DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dta114ed-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 10kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5112DW1"
		(extends "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5112DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dta124ed-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 22kohms, R2 = 22kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5113DW1"
		(extends "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5113DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dta144ed-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 47kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5114DW1"
		(extends "Q_Dual_PNP_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5114DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dta114yd-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual PNP Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5211DW1"
		(extends "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5211DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/DTC114ED-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 10kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5212DW1"
		(extends "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5212DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc124ed-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 22kohms, R2 = 22kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5213DW1"
		(extends "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5213DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc144ed-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 47kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5214DW1"
		(extends "Q_Dual_NPN_NPN_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5214DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc114yd-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual NPN Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5311DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5311DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc114ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 10kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5312DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5312DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc124ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 22kohms, R2 = 22kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5313DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5313DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc144ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 47kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5314DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5314DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc114yp-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 10kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5330DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5330DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc113ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 10V, R1 = 1kohms, R2 = 1kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5331DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5331DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc123ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 12V, R1 = 2.2kohms, R2 = 2.2kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5332DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5332DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc143ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 30V, R1 = 4.7kohms, R2 = 4.7kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5333DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5333DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc143zp-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 30V, R1 = 4.7kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5334DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5334DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc124xp-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 22kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5335DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5335DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc123jp-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 12V, R1 = 2.2kohms, R2 = 47kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "MUN5336DW1"
		(extends "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "MUN5336DW1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/dtc115ep-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Complementary Bias Resistor Transistors, Ic 100mA, Vce 50V, Vin(fwd) 40V, R1 = 100kohms, R2 = 100kohms, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "BRT Digital Transistor NPN PNP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*363*"
			(at 0 0 0)
		)
	)
	(symbol "PBSS301PZ"
		(extends "Q_PNP_BCEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PBSS301PZ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PBSS301PZ.pdf"
			(at 0 0 0)
		)
		(property "Description" "-5.7A Ic, -12V Vce, Small Signal PNP Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "PMBT2222A"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PMBT2222A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMBT2222A.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA Ic, 40V Vce, NPN Transistor, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PMBT2222AYS"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PMBT2222AYS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMBT2222AYS.pdf"
			(at 0 0 0)
		)
		(property "Description" "600mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PMBT3904YS"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PMBT3904YS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMBT3904YS.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PMBT3906YS"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PMBT3906YS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMBT3906YS.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PMBT3946YPN"
		(extends "Q_Dual_NPN_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PMBT3946YPN"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMBT3946YPN.pdf"
			(at 0 0 0)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PN2222A"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PN2222A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "PUMT1"
		(extends "Q_Dual_PNP_PNP_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PUMT1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PUMT1.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 40V Vce, Dual PNP/PNP Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP/PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PUMX1"
		(extends "Q_Dual_NPN_NPN_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PUMX1"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PUMX1.pdf"
			(at 0 0 0)
		)
		(property "Description" "100mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN/NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "PZT2222A"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PZT2222A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN General Puprose Transistor SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "PZT3904"
		(extends "Q_NPN_BCEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PZT3904"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "PZT3906"
		(extends "Q_PNP_BCEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PZT3906"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3906-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "PZTA42"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PZTA42"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PZTA42T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, NPN High Voltage Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN High Voltage Transistor SMD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "PZTA92"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PZTA92"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PZTA92T1-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ic, 300V Vce, PNP High Voltage Transistor, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "PNP High Voltage Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "S8050"
		(extends "Q_NPN_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "S8050"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.unisonic.com.tw/datasheet/S8050.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.7A Ic, 20V Vce, Low Voltage High Current NPN Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "S8050 NPN Low Voltage High Current Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "S8550"
		(extends "Q_PNP_EBC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "S8550"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.unisonic.com.tw/datasheet/S8550.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.7A Ic, 20V Vce, Low Voltage High Current PNP Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "S8550 PNP Low Voltage High Current Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "SS8050"
		(extends "Q_NPN_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SS8050"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -7.366 0)
		)
		(property "Datasheet" "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf"
			(at 5.08 -4.826 0)
		)
		(property "Description" "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"
			(at 34.036 -2.286 0)
		)
		(property "ki_keywords" "SS8050 NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "SS8550"
		(extends "Q_PNP_BEC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SS8550"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -7.366 0)
		)
		(property "Datasheet" "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8550.pdf"
			(at 5.08 -4.826 0)
		)
		(property "Description" "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23"
			(at 34.036 -2.286 0)
		)
		(property "ki_keywords" "SS8550 PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TIP121"
		(extends "TIP120")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP121"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 80V Vce, Silicon Darlington Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP122"
		(extends "TIP120")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP122"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 100V Vce, Silicon Darlington Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP126"
		(extends "TIP125")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP126"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 80V Vce, Silicon Darlington Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP127"
		(extends "TIP125")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP127"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/TIP120-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "5A Ic, 100V Vce, Silicon Darlington Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington Power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP2955"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP2955"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-218-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/TIP3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "-15A Ic, -60V Vce, Power PNP Transistor, TO-218"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218*"
			(at 0 0 0)
		)
	)
	(symbol "TIP2955G"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP2955G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/TIP3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "-15A Ic, -60V Vce, Power PNP Transistor, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "TIP3055"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP3055"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-218-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/TIP3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "15A Ic, 60V Vce, Power NPN Transistor, TO-218"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?218*"
			(at 0 0 0)
		)
	)
	(symbol "TIP3055G"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIP3055G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/TIP3055-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "15A Ic, 60V Vce, Power NPN Transistor, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "TIP41"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP41"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=tip41.PDF"
			(at 0 0 0)
		)
		(property "Description" "6A Ic, 40V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP41A"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP41A"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=tip41.PDF"
			(at 0 0 0)
		)
		(property "Description" "6A Ic, 60V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP41B"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP41B"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=tip41.PDF"
			(at 0 0 0)
		)
		(property "Description" "6A Ic, 80V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP41C"
		(extends "Q_NPN_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP41C"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=tip41.PDF"
			(at 0 0 0)
		)
		(property "Description" "6A Ic, 100V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP42"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP42"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=TIP42.PDF"
			(at 0 0 0)
		)
		(property "Description" "-6A Ic, -40V Vce, Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP42A"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP42A"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=TIP42.PDF"
			(at 0 0 0)
		)
		(property "Description" "-6A Ic, -60V Vce, Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP42B"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP42B"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=TIP42.PDF"
			(at 0 0 0)
		)
		(property "Description" "-6A Ic, -80V Vce, Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIP42C"
		(extends "Q_PNP_BCE")
		(property "Reference" "Q"
			(at 6.35 1.905 0)
		)
		(property "Value" "TIP42C"
			(at 6.35 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 6.35 -1.905 0)
		)
		(property "Datasheet" "https://www.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=TIP42.PDF"
			(at 0 0 0)
		)
		(property "Description" "-6A Ic, -100V Vce, Power PNP Transistor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "power PNP Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "UMH3N"
		(extends "Q_Dual_NPN_NPN_BRT_No_R2_E1B1C2E2B2C1")
		(property "Reference" "Q"
			(at 7.62 1.27 0)
		)
		(property "Value" "UMH3N"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0.127 -11.176 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/discrete/transistor/digital/emh3t2r-e.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "0.1A Ic, 50V Vce, Dual NPN Input Resistor Transistors, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual NPN Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
)
