(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "2N7000"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N7000"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/70226/70226.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.2A Id, 200V Vds, N-Channel MOSFET, 2.6V Logic Level, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "2N7000_0_1")
		(symbol "2N7000_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "3SK263"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "3SK263"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/EN4423-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30mA Id, 15V Vds, N-Channel Dual Gate MOSFET, SOT-143/343"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET Dual Gate"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?143*"
			(at 0 0 0)
		)
		(symbol "3SK263_0_1")
		(symbol "3SK263_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "G1")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AON6411"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "AON6411"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:AO_DFN-8-1EP_5.55x5.2mm_P1.27mm_EP4.12x4.6mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.aosmd.com/res/data_sheets/AON6411.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-85A Id, -20V Vds, P-Channel MOSFET, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AO*DFN*8*1EP*5.55x5.2mm*P1.27mm*EP4.12x4.6mm*"
			(at 0 0 0)
		)
		(symbol "AON6411_0_1")
		(symbol "AON6411_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BF244A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF244A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Fairchild%20PDFs/BF244x.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "BF244A_0_1")
		(symbol "BF244A_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BF245A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF245A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BF245A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "BF245A_0_1")
		(symbol "BF245A_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BF545A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF545A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BF545A_BF545B_BF545C.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5mA Idss, 30V Vgs, N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BF545A_0_1")
		(symbol "BF545A_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BF994S"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 3.175 0)
		)
		(property "Value" "BF994S"
			(at 5.207 1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 5.207 -3.81 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BF994S.pdf"
			(at 5.207 -1.27 0)
		)
		(property "Description" "VHF N-channel dual-gate MOS-FET, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
		(symbol "BF994S_0_1")
		(symbol "BF994S_1_1"
			(pin input line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "G2")
				(number "3")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "4")
			)
			(pin passive line
				(at 2.54 8.89 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -8.89 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BS107"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS107"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BS107-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.25A Id, 200V Vds, N-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "BS107_0_1")
		(symbol "BS107_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BS250"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS250"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70209/70209.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.18A Id, -45V Vds, P-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "BS250_0_1")
		(symbol "BS250_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSB008NE2LX"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB008NE2LX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB008NE2LX-DS-v02_00-EN.pdf?fileId=db3a30432e564707012e5745ca7d000e"
			(at 5.08 -3.81 0)
		)
		(property "Description" "180A Id, 25V Vds, 0.8mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
		(symbol "BSB008NE2LX_0_1")
		(symbol "BSB008NE2LX_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSB028N06NN3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB028N06NN3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB028N06NN3-DS-v02_00-en.pdf?fileId=db3a30432e25b009012e29fda4e23838"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 60V Vds, 2.8mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
		(symbol "BSB028N06NN3_0_1")
		(symbol "BSB028N06NN3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSB104N08NP3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB104N08NP3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MP"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB104N08NP3_G-DS-v02_01-en.pdf?fileId=db3a304341e0aed00141efc548ca1b2b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 80V Vds, 10.4mOhm Rds, N-Channel MOSFET, DirectFET MP"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MP*"
			(at 0 0 0)
		)
		(symbol "BSB104N08NP3_0_1")
		(symbol "BSB104N08NP3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSB165N15NZ3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB165N15NZ3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB165N15NZ3-DS-v02_02-en.pdf?fileId=db3a30432e779412012e7b04a1353843"
			(at 5.08 -3.81 0)
		)
		(property "Description" "45A Id, 150V Vds, 16.5mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
		(symbol "BSB165N15NZ3_0_1")
		(symbol "BSB165N15NZ3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSC13DN30NSFD"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC13DN30NSFD"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSC13DN30NSFD-DS-v02_01-EN.pdf?fileId=5546d46259b0420a0159d5c940fc0d9a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 300V Vds, OptiMOS N-Channel Power MOSFET, 130mOhm Ron, Qg (typ) 30.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
		(symbol "BSC13DN30NSFD_0_1")
		(symbol "BSC13DN30NSFD_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSD235C"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "BSD235C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSD235C-DS-v02_04-EN.pdf?fileId=db3a30433580b371013585a2d0d53326"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.53/+0.95A Id, -20/+20V Vds, P/N-Channel MOSFET, SOT-363, Infineon"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS MOSFET complementary nmos pmos enhanced avalanche AEC Q101 super logic infineon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "BSD235C_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "GN")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "DN")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "SN")
				(number "1")
			)
		)
		(symbol "BSD235C_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "GP")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "SP")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "DP")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSF030NE2LQ"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSF030NE2LQ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSF030NE2LQ-DS-v02_03-en.pdf?fileId=db3a30432e398416012e47a8f0792588"
			(at 5.08 -3.81 0)
		)
		(property "Description" "75A Id, 25V Vds, 3mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
		(symbol "BSF030NE2LQ_0_1")
		(symbol "BSF030NE2LQ_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSF450NE7NH3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSF450NE7NH3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ST"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSF450NE7NH3-DS-v02_02-EN.pdf?fileId=db3a30433a047ba0013a687e2ae403da"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15A Id, 75V Vds, 45mOhm Rds, N-Channel MOSFET, DirectFET ST"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ST*"
			(at 0 0 0)
		)
		(symbol "BSF450NE7NH3_0_1")
		(symbol "BSF450NE7NH3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSP129"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSP129"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSP129-DS-v01_42-en.pdf?fileId=db3a30433c1a8752013c1fc296d2395f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.35A Id, 240V Vds, N-Channel MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BSP129_0_1")
		(symbol "BSP129_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSP89"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSP89"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSP89-DS-v02_02-en.pdf?fileId=db3a30433b47825b013b4b8a07f90d55"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.35A Id, 240V Vds, N-Channel Enhancement Mode MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BSP89_0_1")
		(symbol "BSP89_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSR56"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSR56"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BSR56_57_58.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50mA min, 40V, 25mOhm max, 4-10V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BSR56_0_1")
		(symbol "BSR56_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSS138"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS138"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "BSS138_0_1")
		(symbol "BSS138_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSS214NW"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS214NW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSS214NW-DS-v02_02-en.pdf?fileId=db3a30431b3e89eb011b695aebc01bde"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20V Vds, 1.5A Id, N-Channel MOSFET, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
		(symbol "BSS214NW_0_1")
		(symbol "BSS214NW_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUK9M53-60EX"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M53-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M53-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "17A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 46mOhm Ron, 6nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
		(symbol "BUK9M53-60EX_0_1")
		(symbol "BUK9M53-60EX_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BUZ11"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUZ11"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Fairchild%20PDFs/BUZ11.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "BUZ11_0_1")
		(symbol "BUZ11_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3M0030090K"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0030090K"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-4_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/1185/C3M0030090K.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "63A Id, 900V Vds, 30mOhm, N-Channel SiC MOSFET, TO-247-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
		(symbol "C3M0030090K_0_1")
		(symbol "C3M0030090K_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "DS")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3M0065090D"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0065090D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/176/C3M0065090D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "36A Id, 900V Vds, 65mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
		(symbol "C3M0065090D_0_1")
		(symbol "C3M0065090D_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C3M0065090J"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0065090J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/145/C3M0065090J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 900V Vds, 65mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
		(symbol "C3M0065090J_0_1")
		(symbol "C3M0065090J_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "DS")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD13380F3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD13380F3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_PicoStar_DFN-3_0.69x0.60mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd13380f3.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.6A Id, 12V Vds, N-Channel MOSFET, 76mOhm Ron,max @ 4.5Vgs, 0.91nC Qg,typ @ 4.5Vgs, PicoStar 0.73x0.64mm max, 0.69x0.60mm nom"
			(at 48.26 0 0)
		)
		(property "ki_keywords" "Texas NMOS single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PicoStar*DFN?3*"
			(at 0 0 0)
		)
		(symbol "CSD13380F3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD16301Q2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16301Q2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Texas_DQK"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/csd16301q2.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5A Id, 25V Vds, NexFET N-Channel Power MOSFET, 19mOhm Ron, SON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DQK*"
			(at 0 0 0)
		)
		(symbol "CSD16301Q2_0_1")
		(symbol "CSD16301Q2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD17578Q5A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17578Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17578q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25A Id, 30V Vds, NexFET N-Channel Power MOSFET, 6.9mOhm Ron, Qg (typ) 7.9nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
		(symbol "CSD17578Q5A_0_1")
		(symbol "CSD17578Q5A_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD19537Q3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19537Q3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/csd19537q3.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 100V Vds, NexFET N-Channel Power MOSFET, 13mOhm Ron, Qg Typ 16.0nC, VSON8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
		(symbol "CSD19537Q3_0_1")
		(symbol "CSD19537Q3_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD25302Q2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD25302Q2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Texas_DQK"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/slps234b/slps234b.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-5A Id, -20V Vds, NexFET P-Channel Power MOSFET, 39mOhm Ron, SON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET P-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DQK*"
			(at 0 0 0)
		)
		(symbol "CSD25302Q2_0_1")
		(symbol "CSD25302Q2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD25402Q3A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.715 1.905 0)
		)
		(property "Value" "CSD25402Q3A"
			(at 11.811 -0.127 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 30.353 -4.699 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd25402q3a.pdf"
			(at 31.115 -2.413 0)
		)
		(property "Description" "-76A Id, -20V Vds, NexFET P-Channel Power MOSFET, 7.7mOhm Ron, Qg (typ) 7.5 nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-MOS PMOS single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
		(symbol "CSD25402Q3A_0_1")
		(symbol "CSD25402Q3A_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CSD25480F3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.715 1.905 0)
		)
		(property "Value" "CSD25480F3"
			(at 11.811 -0.127 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_PicoStar_DFN-3_0.69x0.60mm"
			(at 30.353 -4.699 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd25480f3.pdf"
			(at 31.115 -2.413 0)
		)
		(property "Description" "-1.7A Id, -20V Vds, P-Channel MOSFET, 159mOhm Ron,max @ 4.5Vgs, 0.70nC Qg,typ @ 4.5Vgs, PicoStar 0.73x0.64mm max, 0.69x0.60mm nom"
			(at 0 0 0)
		)
		(property "ki_keywords" "Texas PMOS single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PicoStar*DFN?3*"
			(at 0 0 0)
		)
		(symbol "CSD25480F3_0_1")
		(symbol "CSD25480F3_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMC2053UVT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "DMC2053UVT"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMC2053UVT.pdf"
			(at 2.54 -3.81 0)
		)
		(property "Description" "4.6A/-3.2A Id, 20V Vds, Complementary pair enhancement mode P-Channel and N-Channel MOSFET, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "complementary mosfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "DMC2053UVT_0_1")
		(symbol "DMC2053UVT_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
		)
		(symbol "DMC2053UVT_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMG1012T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG1012T"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-523"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds31783.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20V Vds, 0.63 Id, N-Channel MOSFET with ESD protection, SOT-523"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?523*"
			(at 0 0 0)
		)
		(symbol "DMG1012T_0_1")
		(symbol "DMG1012T_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMG9926UDM"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 6.985 0)
		)
		(property "Value" "DMG9926UDM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds31770.pdf"
			(at 2.54 -5.715 0)
		)
		(property "Description" "4.2A Id, 20V Vds, Common-Drain, Dual Half Bridge N-Channel MOSFET, 28mOhm Ron, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Half Bridge N-Channel MOSFET Logic Level Common Drain"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DMG9926UDM_0_1")
		(symbol "DMG9926UDM_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "G1")
				(number "6")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "D1")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "S2")
				(number "3")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "S1/D2")
				(number "2")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(hide yes)
				(name "S1/D2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMN3008SFG"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3008SFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Diodes_PowerDI3333-8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMN3008SFG.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "17.6A Id, 30V Vds, N-Channel Power MOSFET, 4.4mOhm Ron, 86nC Qg (typ), PowerDI3333-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*PowerDI3333*"
			(at 0 0 0)
		)
		(symbol "DMN3008SFG_0_1")
		(symbol "DMN3008SFG_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMN3033LDM"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3033LDM"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds31345.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.9A Id, 30V Vds, N-Channel MOSFET, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DMN3033LDM_0_1")
		(symbol "DMN3033LDM_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMN32D2LDF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 2.54 0)
		)
		(property "Value" "DMN32D2LDF"
			(at 7.62 -3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 1.27 -5.715 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds31238.pdf"
			(at 1.27 -7.62 0)
		)
		(property "Description" "Common Source Dual 400mA Id, 30V Vds, N-Channel MOSFET, 1.5Ohm Ron, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-FET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "DMN32D2LDF_0_1")
		(symbol "DMN32D2LDF_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "D2")
				(number "4")
			)
			(pin input line
				(at -5.08 7.62 270)
				(length 2.54)
				(name "G2")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin input line
				(at 5.08 7.62 270)
				(length 2.54)
				(name "G1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "D1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMP3013SFV"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMP3013SFV"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Diodes_PowerDI3333-8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-12A Id, -30V Vds, P-Channel Power MOSFET, 9.5mOhm Ron, 33.7nC Qg (typ), PowerDI3333-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*PowerDI3333*"
			(at 0 0 0)
		)
		(symbol "DMP3013SFV_0_1")
		(symbol "DMP3013SFV_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DMT6008LFG"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMT6008LFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Diodes_PowerDI3333-8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMT6008LFG.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 60V Vds, N-Channel Enhancement Mode MOSFET, 7.5mOhm Ron, 50.4nC Qg(typ), PowerDI-3333-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*PowerDI3333*"
			(at 0 0 0)
		)
		(symbol "DMT6008LFG_0_1")
		(symbol "DMT6008LFG_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EPC2035"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2035"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2035_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60 V E-mode GaN transistor, RdsOn 45 mOhm, 1.7A Id, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
		(symbol "EPC2035_0_1")
		(symbol "EPC2035_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDC2512"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDC2512"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SuperSOT-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDC2512-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.4A Id, 150V Vds, N-Channel MOSFET, 425mOhm Ron, SuperSOT-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SuperSOT*"
			(at 0 0 0)
		)
		(symbol "FDC2512_0_1")
		(symbol "FDC2512_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDC6330L"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.175 1.905 0)
		)
		(property "Value" "FDC6330L"
			(at 3.175 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 3.175 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDC6330L-D.PDF"
			(at 3.175 -3.81 0)
		)
		(property "Description" "-2.3A, 20V Vds, Integrated load switch, P-Channel MOSFET driven by small N-Channel MOSFET, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "complementary mosfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "FDC6330L_0_1")
		(symbol "FDC6330L_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "S2")
				(number "4")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "G1")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "S1")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "D2")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "D2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDG1024NZ"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDG1024NZ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDG1024NZ-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.2A Id, 20V Vds, Dual N-Channel MOSFET, 175mOhm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET Logic Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "FDG1024NZ_0_1")
		(symbol "FDG1024NZ_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(symbol "FDG1024NZ_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDMC8032L"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMC8032L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Fairchild_DualPower33-6_3x3mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMC8032L-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7A Id, 40V Vds, Dual N-Channel MOSFET, 20mOhm Ron, Power33 Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Fairchild*DualPower33*3x3mm*"
			(at 0 0 0)
		)
		(symbol "FDMC8032L_0_1")
		(symbol "FDMC8032L_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D1")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S1")
				(number "2")
			)
		)
		(symbol "FDMC8032L_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDMT80060DC"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT80060DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT80060DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "43A Id, 60V Vds, PowerTrench N-Channel Power MOSFET, 6.9mOhm Ron, Qg (typ) 7.9nC 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "PowerTrench Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
		(symbol "FDMT80060DC_0_1")
		(symbol "FDMT80060DC_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FDS6890A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS6890A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS6890A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7.5A Id, 20V Vds, Dual N-Channel MOSFET, 18mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FDS6890A_0_1")
		(symbol "FDS6890A_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D1")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S1")
				(number "1")
			)
		)
		(symbol "FDS6890A_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GS66502B"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "GS66502B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Transistor_Power:GaN_Systems_GaNPX-3_5x6.6mm_Drain2.93x0.6mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://gansystems.com/wp-content/uploads/2020/04/GS66502B-DS-Rev-200402.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Bottom-side cooled 650 V E-mode GaN transistor, 7.5A Id, GaN_PX"
			(at 0 0 0)
		)
		(property "ki_keywords" "gan hemt bottom-side-cooled enhancement-mode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "GaN?Systems?GaNPX*5x6.6mm*Drain2.93x0.6mm*"
			(at 0 0 0)
		)
		(symbol "GS66502B_0_1")
		(symbol "GS66502B_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GS66508B"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "GS66508B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Transistor_Power:GaN_Systems_GaNPX-4_7x8.4mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://gansystems.com/wp-content/uploads/2020/04/GS66508B-DS-Rev-200402.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Bottom-side cooled 650 V E-mode GaN transistor, 30A Id, GaN_PX"
			(at 0 0 0)
		)
		(property "ki_keywords" "gan hemt bottom side cooled 650v enhancement mode 30a Id"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "GaN?Systems?GaNPX*7x8.4mm*"
			(at 0 0 0)
		)
		(symbol "GS66508B_0_1")
		(symbol "GS66508B_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IF3602"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 4.445 0)
		)
		(property "Value" "IF3602"
			(at 5.08 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-78-8"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.interfet.com/jfet-datasheets/jfet-if3602-interfet.pdf"
			(at 5.08 -2.54 0)
		)
		(property "Description" "Ultra Low Noise: 0.35 nV/√Hz Typical, Dual Matched N-Channel JFET, TO-78-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ultra low noise dual matched n-channel jfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?78?8*"
			(at 0 0 0)
		)
		(symbol "IF3602_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D1")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S1")
				(number "1")
			)
		)
		(symbol "IF3602_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G2")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "5")
			)
		)
		(symbol "IF3602_3_1"
			(text "CASE"
				(at 0 0 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "CASE")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IGLD60R070D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGLD60R070D1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Infineon_PG-LSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGLD60R070D1-DataSheet-v02_00-EN.pdf?fileId=5546d46265f064ff016685f03f056511"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15A Id, 600V Vds, 70mOhm, N-Channel GaN MOSFET, LSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*LSON*1*"
			(at 0 0 0)
		)
		(symbol "IGLD60R070D1_0_1")
		(symbol "IGLD60R070D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IGO60R070D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGO60R070D1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-20-85"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGO60R070D1-DataSheet-v02_01-EN.pdf?fileId=5546d46265f064ff016685f053216514"
			(at 5.08 -3.81 0)
		)
		(property "Description" "31A Id, 600V Vds, 70mOhm, N-Channel GaN MOSFET, PD-DSO-20-85"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*85*"
			(at 0 0 0)
		)
		(symbol "IGO60R070D1_0_1")
		(symbol "IGO60R070D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "13")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "14")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "15")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "16")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "17")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "18")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "21")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IGOT60R070D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGOT60R070D1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-20-87"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGOT60R070D1-DataSheet-v02_11-EN.pdf?fileId=5546d46265f064ff016685fa65066523"
			(at 5.08 -3.81 0)
		)
		(property "Description" "31A Id, 600V Vds, 70mOhm, N-Channel GaN MOSFET, PD-DSO-20-87"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*DSO*87*"
			(at 0 0 0)
		)
		(symbol "IGOT60R070D1_0_1")
		(symbol "IGOT60R070D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "8")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "13")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "14")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "15")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "16")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "17")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "18")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IGT60R070D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGT60R070D1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-3_ThermalVias"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGT60R070D1-DataSheet-v02_01-EN.pdf?fileId=5546d46265f064ff016686028dd56526"
			(at 5.08 -3.81 0)
		)
		(property "Description" "31A Id, 600V Vds, 70mOhm, N-Channel GaN MOSFET, HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*3*"
			(at 0 0 0)
		)
		(symbol "IGT60R070D1_0_1")
		(symbol "IGT60R070D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "SS")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPB180N10S4-02"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPB180N10S4-02"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPB180N10S4_02-DS-v01_00-en.pdf?fileId=db3a30433d1d0bbe013d2129cf8a2f88"
			(at 5.08 -3.81 0)
		)
		(property "Description" "180A Id, 100V Vds, OptiMOS-T2 N-Channel Power MOSFET, 2.5mOhm Ron, Qg (typ) 156nC, TO-263-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS-T2 Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263?6*"
			(at 0 0 0)
		)
		(symbol "IPB180N10S4-02_0_1")
		(symbol "IPB180N10S4-02_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPD50R380CE"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPD50R380CE"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPD50R380CE-DS-v02_01-en.pdf?fileId=db3a30433ecb86d4013ed0a2ef580f38"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14.1A Id, 500V Vds, CoolMOS N-Channel Power MOSFET, 380mOhm Ron, 24.8nC Qg (typ), TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "CoolMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "IPD50R380CE_0_1")
		(symbol "IPD50R380CE_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPDD60R050G7"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R050G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R050G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a0161707eb2f97810"
			(at 5.08 -3.81 0)
		)
		(property "Description" "47A Id, 600V Vds, 50mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
		(symbol "IPDD60R050G7_0_1")
		(symbol "IPDD60R050G7_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "DS")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "10")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "9")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "PS")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "PS")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "PS")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPT012N08N5"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPT012N08N5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-IPT012N08N5-DS-v02_01-EN.pdf?fileId=5546d4624a75e5f1014aca59127a1eb9"
			(at 5.08 -3.81 0)
		)
		(property "Description" "300A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 1.2mOhm Ron, Qg (typ) 178.0nC, PG-HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*"
			(at 0 0 0)
		)
		(symbol "IPT012N08N5_0_1")
		(symbol "IPT012N08N5_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF40DM229"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF40DM229"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MF"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF40DM229-DS-v02_00-EN.pdf?fileId=5546d462557e6e890155a15c899160ea"
			(at 5.08 -3.81 0)
		)
		(property "Description" "159A Id, 40V Vds, 1.85mOhm Rds, N-Channel MOSFET, DirectFET MF"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MF*"
			(at 0 0 0)
		)
		(symbol "IRF40DM229_0_1")
		(symbol "IRF40DM229_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF60DM206"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF60DM206"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ME"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf60dm206.pdf?fileId=5546d462533600a4015355e433aa19ca"
			(at 5.08 -3.81 0)
		)
		(property "Description" "130A Id, 60V Vds, 2.9mOhm Rds, N-Channel MOSFET, DirectFET ME"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ME*"
			(at 0 0 0)
		)
		(symbol "IRF60DM206_0_1")
		(symbol "IRF60DM206_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6613"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6613"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MT"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6613pbf.pdf?fileId=5546d462533600a4015355e82b9b1a0d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "150A Id, 40V Vds, 3.4mOhm Rds, N-Channel MOSFET, DirectFET MT"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MT*"
			(at 0 0 0)
		)
		(symbol "IRF6613_0_1")
		(symbol "IRF6613_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6655"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6655"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SH"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6655pbf.pdf?fileId=5546d462533600a4015355ec76961a5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.2A Id, 100V Vds, 62mOhm Rds, N-Channel MOSFET, DirectFET SH"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SH*"
			(at 0 0 0)
		)
		(symbol "IRF6655_0_1")
		(symbol "IRF6655_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6710S2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6710S2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_S1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6710s2pbf.pdf?fileId=5546d462533600a4015355ece3db1a78"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12A Id, 25V Vds, 5.9mOhm Rds, N-Channel MOSFET, DirectFET S1"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*S1*"
			(at 0 0 0)
		)
		(symbol "IRF6710S2_0_1")
		(symbol "IRF6710S2_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6718L2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6718L2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6718l2pbf.pdf?fileId=5546d462533600a4015355ed25bd1a88"
			(at 5.08 -3.81 0)
		)
		(property "Description" "61A Id, 25V Vds, 0.7mOhm Rds, N-Channel MOSFET, DirectFET L6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L6*"
			(at 0 0 0)
		)
		(symbol "IRF6718L2_0_1")
		(symbol "IRF6718L2_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6802SD"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6802SD"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SA"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6802sdpbf.pdf?fileId=5546d462533600a4015355f0a3021ab2"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 25V Vds, 4.2mOhm Rds, Dual N-Channel MOSFET, DirectFET SA"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SA*"
			(at 0 0 0)
		)
		(symbol "IRF6802SD_0_1")
		(symbol "IRF6802SD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S1")
				(number "3")
			)
		)
		(symbol "IRF6802SD_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF6892S"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6892S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_S3C"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6892spbf.pdf?fileId=5546d462533600a4015355f0bb961ab8"
			(at 5.08 -3.81 0)
		)
		(property "Description" "28A Id, 25V Vds, 1.7mOhm Rds, N-Channel MOSFET, DirectFET S3C"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*S3C*"
			(at 0 0 0)
		)
		(symbol "IRF6892S_0_1")
		(symbol "IRF6892S_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7309IPBF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7309IPBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf7309ipbf.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3A Id, 30V Vds, Dual HEXFET N- and P-Channel MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual HEXFET N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRF7309IPBF_0_1")
		(symbol "IRF7309IPBF_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(symbol "IRF7309IPBF_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7324"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7324"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irf7324pbf.pdf?fileId=5546d462533600a4015355f5f0861b4b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-9A Id, -20V Vds, Dual HEXFET P-Channel MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual HEXFET P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRF7324_0_1")
		(symbol "IRF7324_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D1")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S1")
				(number "1")
			)
		)
		(symbol "IRF7324_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G2")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7404"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7404"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irf7404.pdf?fileId=5546d462533600a4015355fa2b5b1b9e"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-6.7A Id, -20V Vds, P-Channel HEXFET Power MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRF7404_0_1")
		(symbol "IRF7404_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7606PBF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7606PBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf7606pbf.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.6A Id, -30V Vds, HexFET P-MOS Power MOSFET, Ronon 0.09R, Micro8"
			(at 0 0 0)
		)
		(property "ki_keywords" "HexFET Power MOSFET P-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IRF7606PBF_0_1")
		(symbol "IRF7606PBF_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7607PBF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7607PBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf7607pbf.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.2A Id, 20V Vds, HexFET N-MOS Power MOSFET, Ronon 0.03R, Micro8"
			(at 0 0 0)
		)
		(property "ki_keywords" "HexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IRF7607PBF_0_1")
		(symbol "IRF7607PBF_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7665S2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7665S2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SB"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7665s2pbf.pdf?fileId=5546d462533600a401535603d3ba1c86"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14.4A Id, 100V Vds, 62mOhm Rds, N-Channel MOSFET, DirectFET SB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SB*"
			(at 0 0 0)
		)
		(symbol "IRF7665S2_0_1")
		(symbol "IRF7665S2_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF7739L1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7739L1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7739l1pbf.pdf?fileId=5546d462533600a40153560423d91c9a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "270A Id, 40V Vds, 1.0mOhm Rds, N-Channel MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
		(symbol "IRF7739L1_0_1")
		(symbol "IRF7739L1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF8721PBF-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "IRF8721PBF-1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf8721pbf-1.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 30V Vds, HEXFET N-Channel MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "HEXFET N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRF8721PBF-1_0_1")
		(symbol "IRF8721PBF-1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF9383M"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF9383M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf9383mpbf.pdf?fileId=5546d462533600a40153561169a11dab"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-22A Id, -30V Vds, 2.9mOhm Rds, P-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
		(symbol "IRF9383M_0_1")
		(symbol "IRF9383M_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRF9540N"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF9540N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf9540n.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-23A Id, -100V Vds, 117mOhm Rds, P-Channel HEXFET Power MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET HEXFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "IRF9540N_0_1")
		(symbol "IRF9540N_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRFI4019H"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 4.445 0)
		)
		(property "Value" "IRFI4019H"
			(at 5.08 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfi4019h-117p.pdf?fileId=5546d462533600a401535623d74d1f6f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "8.7A Id, 150V Vds, 80mOhm Rds, Dual Half Bridge N-Channel MOSFET, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET Half-Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*P3.4x2.06mm*StaggerEven*Lead1.86mm*"
			(at 0 0 0)
		)
		(symbol "IRFI4019H_0_1")
		(symbol "IRFI4019H_1_1"
			(pin input line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "G1")
				(number "4")
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "G2")
				(number "2")
			)
			(pin passive line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "D1")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "S2")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "S1/D2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRFTS9342PBF"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFTS9342PBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfts9342pbf.pdf?fileId=5546d462533600a40153563aeabc21f3"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-5.8A Id, -30V Vds, 40mOhm Rds, P-Channel HEXFET Power MOSFET, TSOP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET HEXFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "IRFTS9342PBF_0_1")
		(symbol "IRFTS9342PBF_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRL6283M"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRL6283M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MD"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irl6283mpbf.pdf?fileId=5546d462533600a40153565fe9452573"
			(at 5.08 -3.81 0)
		)
		(property "Description" "38A Id, 20V Vds, 0.75mOhm Rds, N-Channel HEXFET Power MOSFET, DirectFET MD"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET IRFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MD*"
			(at 0 0 0)
		)
		(symbol "IRL6283M_0_1")
		(symbol "IRL6283M_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRLIZ44N"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLIZ44N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irliz44n.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 55V Vds, 22mOhm Rds, N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*"
			(at 0 0 0)
		)
		(symbol "IRLIZ44N_0_1")
		(symbol "IRLIZ44N_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JFE150DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "JFE150DBV"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/jfe150.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low-Noise, Low-Gate-Current, Audio, N-Channel JFET, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise n-channel jfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "JFE150DBV_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.334)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(symbol "JFE150DBV_2_0"
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCH")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(name "VCL")
				(number "2")
			)
		)
		(symbol "JFE150DBV_2_1")
		(embedded_fonts no)
	)
	(symbol "JFE2140D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "JFE2140D"
			(at 8.89 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/jfe2140.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low Noise, Matched, Dual, Low-Gate Current, Discrete, Audio, N‑Channel JFET, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise n-channel dual matched jfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "JFE2140D_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.334)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "JFE2140D_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.334)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(symbol "JFE2140D_3_0"
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(name "VCH")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(name "VCL")
				(number "7")
			)
		)
		(symbol "JFE2140D_3_1")
		(embedded_fonts no)
	)
	(symbol "PGA26E07BA"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PGA26E07BA"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:Panasonic_HSON-8_8x8mm_P2.00mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/PGA26E07BA_E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "26A Id, 600V Vds, 56mOhm, N-Channel GaN MOSFET, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Panasonic*HSON*8x8mm*P2.00mm*"
			(at 0 0 0)
		)
		(symbol "PGA26E07BA_0_1")
		(symbol "PGA26E07BA_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "S1")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S2")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S2")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMN48XP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PMN48XP"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMN48XP.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-4.1A Id, -20V Vds, P-Channel Power MOSFET, 48mOhm Ron, TSOP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "PMN48XP_0_1")
		(symbol "PMN48XP_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PSMN5R2-60YL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.715 1.905 0)
		)
		(property "Value" "PSMN5R2-60YL"
			(at 12.7 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK56"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PSMN5R2-60YL.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A, 60V Vds, N-Channel MOSFET, 5.2mOhm Ron, LFPAK56"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK56*"
			(at 0 0 0)
		)
		(symbol "PSMN5R2-60YL_0_1")
		(symbol "PSMN5R2-60YL_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QM6015D"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "QM6015D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.jaolen.com/images/pdf/QM6015D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-35A Id, -60V Vds, P-Channel Power MOSFET, 25mOhm Ron, 25.0nC Qg (typ), TO252"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "QM6015D_0_1")
		(symbol "QM6015D_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NMOS_G1S2G2D2S1D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_NMOS_G1S2G2D2S1D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "Dual NMOS transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NMOS_G1S2G2D2S1D1_0_1")
		(symbol "Q_Dual_NMOS_G1S2G2D2S1D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
		)
		(symbol "Q_Dual_NMOS_G1S2G2D2S1D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NMOS_S1G1D2S2G2D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_NMOS_S1G1D2S2G2D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "Dual NMOS transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NMOS_S1G1D2S2G2D1_0_1")
		(symbol "Q_Dual_NMOS_S1G1D2S2G2D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(symbol "Q_Dual_NMOS_S1G1D2S2G2D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NMOS_S1G1S2G2D2D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_NMOS_S1G1S2G2D2D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "Dual NMOS transistor, 6 pin package"
			(at 2.286 -12.192 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D1_0_1")
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_NMOS_S1G1S2G2D2D2D1D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_NMOS_S1G1S2G2D2D2D1D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "Dual NMOS transistor, 8 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D2D1D1_0_1")
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D2D1D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
		)
		(symbol "Q_Dual_NMOS_S1G1S2G2D2D2D1D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PMOS_G1S2G2D2S1D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_PMOS_G1S2G2D2S1D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" "~"
			(at 1.27 0 0)
		)
		(property "Description" "Dual PMOS transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PMOS_G1S2G2D2S1D1_0_1")
		(symbol "Q_Dual_PMOS_G1S2G2D2S1D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "5")
			)
		)
		(symbol "Q_Dual_PMOS_G1S2G2D2S1D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PMOS_S1G1D2S2G2D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_PMOS_S1G1D2S2G2D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" "~"
			(at 1.27 0 0)
		)
		(property "Description" "Dual PMOS transistor, 6 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PMOS_S1G1D2S2G2D1_0_1")
		(symbol "Q_Dual_PMOS_S1G1D2S2G2D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(symbol "Q_Dual_PMOS_S1G1D2S2G2D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_Dual_PMOS_S1G1S2G2D2D2D1D1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_Dual_PMOS_S1G1S2G2D2D2D1D1"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" "~"
			(at 1.27 0 0)
		)
		(property "Description" "Dual PMOS transistor, 8 pin package"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_Dual_PMOS_S1G1S2G2D2D2D1D1_0_1")
		(symbol "Q_Dual_PMOS_S1G1S2G2D2D2D1D1_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "8")
			)
		)
		(symbol "Q_Dual_PMOS_S1G1S2G2D2D2D1D1_2_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_DGS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_DGS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, drain/gate/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_DGS_0_1")
		(symbol "Q_NMOS_DGS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_DSG"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_DSG"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_DSG_0_1")
		(symbol "Q_NMOS_DSG_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_GDS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_GDS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, gate/drain/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_GDS_0_1")
		(symbol "Q_NMOS_GDS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_GDSD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_GDSD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, gate/drain/source, drain connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_GDSD_0_1")
		(symbol "Q_NMOS_GDSD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_GSD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_GSD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_GSD_0_1")
		(symbol "Q_NMOS_GSD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_SDGD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_SDGD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, source/drain/gate, drain connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_SDGD_0_1")
		(symbol "Q_NMOS_SDGD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_SGD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_SGD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "N-MOSFET transistor, source/gate/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_SGD_0_1")
		(symbol "Q_NMOS_SGD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_DGS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_DGS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, drain/gate/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_DGS_0_1")
		(symbol "Q_PMOS_DGS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_DSG"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_DSG"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_DSG_0_1")
		(symbol "Q_PMOS_DSG_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_GDS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_GDS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, gate/drain/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_GDS_0_1")
		(symbol "Q_PMOS_GDS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_GDSD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_GDSD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, gate/drain/source, drain connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_GDSD_0_1")
		(symbol "Q_PMOS_GDSD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_GSD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_GSD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, gate/source/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_GSD_0_1")
		(symbol "Q_PMOS_GSD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_SDG"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_SDG"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, source/drain/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_SDG_0_1")
		(symbol "Q_PMOS_SDG_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_SDGD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_SDGD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, source/drain/gate, drain connected to mounting plane"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_SDGD_0_1")
		(symbol "Q_PMOS_SDGD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_PMOS_SGD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_PMOS_SGD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "P-MOSFET transistor, source/gate/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET"
			(at 0 0 0)
		)
		(symbol "Q_PMOS_SGD_0_1")
		(symbol "Q_PMOS_SGD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SCTL35N65G2V"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SCTL35N65G2V"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:ST_PowerFLAT_HV-5_8x8mm"
			(at -23.622 -15.875 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sctl35n65g2v.pdf"
			(at -29.972 -17.78 0)
		)
		(property "Description" "Silicon carbide Power MOSFET 650 V, 55 mΩ typ., 40 A, ST_PowerFLAT_HV-5"
			(at 0.508 -13.716 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?PowerFLAT?HV*8x8mm*"
			(at 0 0 0)
		)
		(symbol "SCTL35N65G2V_0_1")
		(symbol "SCTL35N65G2V_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "DS")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SGT65R65AL"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SGT65R65AL"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:ST_PowerFLAT_HV-8_5x6mm"
			(at -18.288 -15.494 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/sgt65r65al.pdf"
			(at -24.13 -17.78 0)
		)
		(property "Description" "650V, 49mΩ typ., 25A Id, enhancement mode PowerGaN transistor, ST_PowerFLAT_HV-8"
			(at 0.254 -13.208 0)
		)
		(property "ki_keywords" "gan hemt bottom-side-cooled e-mode kelvin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?PowerFLAT?HV*5x6mm*"
			(at 0 0 0)
		)
		(symbol "SGT65R65AL_0_1")
		(symbol "SGT65R65AL_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "KS")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SQJQ160E"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ160E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/63059/sqjq160e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "602A Id, 60V Vds, N-Channel TrenchFET MOSFET, 0.85mOhm Ron, 42nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
		(symbol "SQJQ160E_0_1")
		(symbol "SQJQ160E_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STB15N80K5"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "STB15N80K5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stb15n80k5.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 800V Vds, N-Channel MOSFET, 375mOhm Ron, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
		(symbol "STB15N80K5_0_1")
		(symbol "STB15N80K5_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STD7NK40Z"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "STD7NK40Z"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/std7nk40zt4.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.4A Id, 400V Vds, N-Channel MOSFET, 1Ohm Ron, DPAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "STD7NK40Z_0_1")
		(symbol "STD7NK40Z_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SUD19P06-60"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD19P06-60"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/69253/sud19p06.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-19A Id, -60V Vds, TrenchFET P-Channel Power MOSFET, 60mOhm Ron, 40nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "SUD19P06-60_0_1")
		(symbol "SUD19P06-60_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si1442DH"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si1442DH"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/63772/si1442dh.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12V Vds, TrenchFET N-Channel Power MOSFET, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET N-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "Si1442DH_0_1")
		(symbol "Si1442DH_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si3456DDV"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si3456DDV"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/69075/si3456ddv.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30V Vds, 6.3A Id, N-Channel MOSFET, TSOP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOP*1.65x3.05mm*P0.95mm*"
			(at 0 0 0)
		)
		(symbol "Si3456DDV_0_1")
		(symbol "Si3456DDV_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7141DP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si7141DP"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:PowerPAK_SO-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65596/si7141dp.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-60A Id, -20V Vds, 1.9 mOhm Ron, PowerPAK-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerPAK*SO*Single*"
			(at 0 0 0)
		)
		(symbol "Si7141DP_0_1")
		(symbol "Si7141DP_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7336ADP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si7336ADP"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:PowerPAK_SO-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/73152/si7336adp.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 30V Vds, 2.4mOhm Ron, PowerPAK-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerPAK*SO*Single*"
			(at 0 0 0)
		)
		(symbol "Si7336ADP_0_1")
		(symbol "Si7336ADP_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiA453EDJ"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiA453EDJ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Vishay_PowerPAK_SC70-6L_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/62864/sia453edj.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-10A Id, -30V Vds, P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*SC70*Single*"
			(at 0 0 0)
		)
		(symbol "SiA453EDJ_0_1")
		(symbol "SiA453EDJ_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiA462DJ"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.715 1.905 0)
		)
		(property "Value" "SiA462DJ"
			(at 9.525 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Vishay_PowerPAK_SC70-6L_Single"
			(at 5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/63269/sia462dj.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "12A Id, 30V Vds, N-Channel MOSFET, Rds 18mΩ PowerPAK, SC70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS NFET Vishay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*SC70*Single*"
			(at 0 0 0)
		)
		(symbol "SiA462DJ_0_1")
		(symbol "SiA462DJ_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiS415DNT"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiS415DNT"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Vishay_PowerPAK_1212-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/63684/sis415dnt.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-35A Id, -20V Vds, P-Channel MOSFET, PowerPAK 1212-8 Single"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*1212*Single*"
			(at 0 0 0)
		)
		(symbol "SiS415DNT_0_1")
		(symbol "SiS415DNT_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SiS454DN"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiS454DN"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Vishay_PowerPAK_1212-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/66707/sis454dn.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 20V Vds, N-Channel MOSFET, PowerPAK 1212-8 Single"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*1212*Single*"
			(at 0 0 0)
		)
		(symbol "SiS454DN_0_1")
		(symbol "SiS454DN_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TP0610L"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TP0610L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70209/70209.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.18A Id, -60V Vds, P-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92L*"
			(at 0 0 0)
		)
		(symbol "TP0610L_0_1")
		(symbol "TP0610L_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TP0610T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TP0610T"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70209/70209.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.18A Id, -60V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TP0610T_0_1")
		(symbol "TP0610T_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXMP4A16G"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMP4A16G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXMP4A16G.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-6.4A Id, -40V Vds, P-Channel MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "ZXMP4A16G_0_1")
		(symbol "ZXMP4A16G_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2N3819"
		(extends "BF244A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N3819"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://my.centralsemi.com/datasheets/2N3819.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20mA Id, 25V Vgs, N-Channel JFET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel JFET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "2N7002"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N7002"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS7002A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Switching MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "2N7002E"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N7002E"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds30376.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.24A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "2N7002H"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N7002H"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/2N7002H.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.21A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "2N7002K"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "2N7002K"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30896.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.38A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AO3400A"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "AO3400A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AO3401A"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "AO3401A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "AO4842"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "AO4842"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://aosmd.com/sites/default/files/res/data_sheets/AO4842.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7.7A Id, 30V Vds, Dual N-Channel MOSFET, 21mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AO4892"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "AO4892"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://aosmd.com/sites/default/files/res/datasheets/AO4892.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 100V Vds, Dual N-Channel MOSFET, 68mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS Alpha-Omega"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "BF244B"
		(extends "BF244A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF244B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Fairchild%20PDFs/BF244x.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BF244C"
		(extends "BF244A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF244C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Fairchild%20PDFs/BF244x.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BF245B"
		(extends "BF245A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF245B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BF245A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BF245C"
		(extends "BF245A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF245C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BF245A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10mA Id, 30V Vgs, N-Channel FET Transistor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BF545B"
		(extends "BF545A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF545B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BF545A_BF545B_BF545C.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15mA Idss, 30V Vgs, N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BF545C"
		(extends "BF545A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BF545C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BF545A_BF545B_BF545C.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25mA Idss, 30V Vgs, N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor Low Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BS108"
		(extends "BS107")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS108"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.redrok.com/MOSFET_BS108_200V_250mA_8O_Vth1.5_TO-92.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.25A Id, 200V Vds, N-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BS170"
		(extends "BS107")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS170"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BS170-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.5A Id, 60V Vds, N-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
	(symbol "BS170F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS170F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/BS170F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.15A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BS870"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BS870"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds11302.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.25A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSB012NE2LXI"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB012NE2LXI"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB012NE2LXI-DS-v02_01-EN.pdf?fileId=db3a30433f764301013f805e3eb247c1"
			(at 5.08 -3.81 0)
		)
		(property "Description" "170A Id, 25V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "BSB013NE2LXI"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB013NE2LXI"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB013NE2LXI-DS-v02_04-en.pdf?fileId=db3a30432e398416012e47a158802577"
			(at 5.08 -3.81 0)
		)
		(property "Description" "163A Id, 25V Vds, 1.3mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "BSB014N04LX3"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB014N04LX3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB014N04LX3G-DS-v02_03-en.pdf?fileId=db3a304320d39d590121a02c6c737a9b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "180A Id, 40V Vds, 1.4mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "BSB015N04NX3"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB015N04NX3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB015N04NX3G-DS-v02_04-en.pdf?fileId=db3a304320d39d590121a03bbfcd7aac"
			(at 5.08 -3.81 0)
		)
		(property "Description" "180A Id, 40V Vds, 1.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "BSB044N08NN3"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB044N08NN3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB044N08NN3_G-DS-v02_00-en.pdf?fileId=db3a30435819ae2e012e385cde7b70d4"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 80V Vds, 4.4mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "BSB056N10NN3"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB056N10NN3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB056N10NN3_G-DS-v02_05-en.pdf?fileId=db3a30442e152e91012e390b9a631459"
			(at 5.08 -3.81 0)
		)
		(property "Description" "83A Id, 100V Vds, 5.1mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "BSB280N15NZ3"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSB280N15NZ3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSB280N15NZ3-DS-v02_05-en.pdf?fileId=db3a30432e779412012e7b0b544c3852"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 150V Vds, 28mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "BSC026N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC026N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC026N08NS5-DS-v02_01-EN.pdf?fileId=5546d4624ad04ef9014ae2eace7629e0"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 2.6mOhm Ron, Qg (typ) 74.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC028N06LS3"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC028N06LS3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC028N06LS3-DS-v02_02-en.pdf?fileId=db3a30431ddc9372011ebafa4c607f8c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, OptiMOS N-Channel Power MOSFET, 2.8mOhm Ron, Qg (typ) 31.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC030N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC030N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC030N08NS5-DS-v02_02-EN.pdf?fileId=5546d4624ad04ef9014aed52f4210acf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 3.0mOhm Ron, Qg (typ) 61.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC035N10NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC035N10NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC035N10NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae8b5f3bc1b6f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 3.5mOhm Ron, Qg (typ) 70.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC037N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC037N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC037N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae9ad3b8e1c33"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 3.7mOhm Ron, Qg (typ) 46.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC040N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC040N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC040N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae3065a7e2a05"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 4.0mOhm Ron, Qg (typ) 43.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC040N10NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC040N10NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC040N10NS5-DS-v02_01-EN.pdf?fileId=5546d4624a0bf290014a0fbcee2e6b38"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 4.0mOhm Ron, Qg (typ) 58.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC046N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC046N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC046N10NS3-DS-v02_00-en.pdf?fileId=db3a304332fc1ee7013316f966a4713c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 4.6mOhm Ron, Qg (typ) 63.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC047N08NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC047N08NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC047N08NS3G-DS-v02_07-en.pdf?fileId=db3a30431add1d95011ae7e8dacf5611"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 4.7mOhm Ron, Qg (typ) 52.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC052N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC052N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC052N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae38fc94f2b40"
			(at 5.08 -3.81 0)
		)
		(property "Description" "95A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 5.2mOhm Ron, Qg (typ) 32.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC057N08NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC057N08NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC057N08NS3G-DS-v02_04-en.pdf?fileId=db3a30431add1d95011ae803c9345616"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 5.7mOhm Ron, Qg (typ) 42.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC060N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC060N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC060N10NS3-DS-v02_04-en.pdf?fileId=db3a30431ce5fb52011d1aab7f90133a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 6.0mOhm Ron, Qg (typ) 51.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC061N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC061N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC061N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae3ab1bb62b69"
			(at 5.08 -3.81 0)
		)
		(property "Description" "82A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 6.1mOhm Ron, Qg (typ) 27.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC070N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC070N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC070N10NS3-DS-v02_01-en.pdf?fileId=db3a304327b89750012824712c6c6f2f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 7.0mOhm Ron, Qg (typ) 42.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC070N10NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC070N10NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC070N10NS5-DS-v02_01-EN.pdf?fileId=5546d4624a0bf290014a0fc62d9d6b3c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "80A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 7.0mOhm Ron, Qg (typ) 30.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC072N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC072N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC072N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae3d8e8192c7c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "74A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 7.2mOhm Ron, Qg (typ) 24.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC079N10NSG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC079N10NSG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC079N10NS-DS-v01_06-en.pdf?fileId=db3a3043163797a601167b174f951147"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 7.9mOhm Ron, Qg (typ) 66.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC082N10LSG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC082N10LSG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC082N10LS-DS-v01_07-en.pdf?fileId=db3a3043163797a6011647faad240719"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 8.2mOhm Ron, Qg (typ) 78.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC098N10NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC098N10NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC098N10NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae95ab4221bfd"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 9.8mOhm Ron, Qg (typ) 22.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC100N10NSFG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC100N10NSFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC100N10NSF-DS-v02_08-en.pdf?fileId=db3a30431b3e89eb011b49a75b607b57"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 10.0mOhm Ron, Qg (typ) 33.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC105N10LSFG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC105N10LSFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC105N10LSF-DS-v02_09-en.pdf?fileId=db3a30431b3e89eb011b499b2aa07b26"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 10.5mOhm Ron, Qg (typ) 40.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC109N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC109N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC109N10NS3-DS-v02_00-en.pdf?fileId=db3a304327b897500128247bdae36f3f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "63A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 10.9mOhm Ron, Qg (typ) 26.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC117N08NS5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC117N08NS5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC117N08NS5-DS-v02_00-EN.pdf?fileId=5546d4624ad04ef9014ae97632721c1b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "49A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 11.7mOhm Ron, Qg (typ) 15.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC118N10NSG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC118N10NSG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC118N10NS-DS-v01_08-en.pdf?fileId=db3a3043163797a6011647fdc2d4071c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "71A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 11.8mOhm Ron, Qg (typ) 42.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC123N08NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC123N08NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC123N08NS3G-DS-v02_05-en.pdf?fileId=db3a30431add1d95011ae80eb8555625"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 12.3mOhm Ron, Qg (typ) 19.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC123N10LSG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC123N10LSG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC123N10LS-DS-v02_08-en.pdf?fileId=db3a30431b3e89eb011b4626974b7df5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "71A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 12.3mOhm Ron, Qg (typ) 51.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC159N10LSFG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC159N10LSFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC159N10LSF-DS-v02_09-en.pdf?fileId=db3a30431b3e89eb011b499f85d47b36"
			(at 5.08 -3.81 0)
		)
		(property "Description" "63A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 15.9mOhm Ron, Qg (typ) 26.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC160N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC160N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC160N10NS3-DS-v02_04-en.pdf?fileId=db3a30432239cccd01226040189a7f47"
			(at 5.08 -3.81 0)
		)
		(property "Description" "42A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 16.0mOhm Ron, Qg (typ) 19.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC196N10NSG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC196N10NSG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC196N10NS-DS-v01_07-en.pdf?fileId=db3a3043163797a601164800549d071f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "45A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 19.6mOhm Ron, Qg (typ) 25.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC252N10NSFG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC252N10NSFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC252N10NSF-DS-v02_08-en.pdf?fileId=db3a30431b3e89eb011b498909e97b17"
			(at 5.08 -3.81 0)
		)
		(property "Description" "40A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 25.2mOhm Ron, Qg (typ) 13.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC265N10LSFG"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC265N10LSFG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC265N10LSFG-DS-v02_08-en.pdf?fileId=db3a30431b3e89eb011b49a375207b46"
			(at 5.08 -3.81 0)
		)
		(property "Description" "40A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 26.5mOhm Ron, Qg (typ) 16.0nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC340N08NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC340N08NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC340N08NS3G-DS-v02_06-en.pdf?fileId=db3a30431add1d95011ae81c21f2563a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "23A Id, 80V Vds, OptiMOS N-Channel Power MOSFET, 34.0mOhm Ron, Qg (typ) 6.8nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSC440N10NS3G"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSC440N10NS3G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BSC440N10NS3-DS-v02_04-en.pdf?fileId=db3a30432239cccd0122604520d47f56"
			(at 5.08 -3.81 0)
		)
		(property "Description" "18A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 44.0mOhm Ron, Qg (typ) 8.1nC, PG-TDSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "BSD840N"
		(extends "FDG1024NZ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSD840N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/BSD840N_Rev2%204.pdf?fileId=db3a30431b0626df011b12b4486c7c02"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.88A Id, 20V Vds, Dual N-Channel MOSFET, 560mOhm Ron at 1.8V Vgs (ultra logic level), SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "nfet pair"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "BSF035NE2LQ"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSF035NE2LQ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSF035NE2LQ-DS-v01_03-en.pdf?fileId=db3a30433f764301013f7fe8a925463c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "69A Id, 25V Vds, 3.5mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "BSN20"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSN20"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31898.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.5A Id, 50V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSR57"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSR57"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BSR56_57_58.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20mA min, 40V, 40mOhm max, 2-6V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSR58"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSR58"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/BSR56_57_58.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "80mA min, 40V, 60mOhm max, 0.8-4V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSS123"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS123"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds30366.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.17A Id, 100V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSS127S"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS127S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/BSS127.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.07A Id, 600V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSS83P"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS83P"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/1835997.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.33A Id, -60V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BSS84"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BSS84"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://assets.nexperia.com/documents/data-sheet/BSS84.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.13A Id, -50V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7880-55A"
		(extends "BSP89")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7880-55A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7880-55A.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7A Id, 55V Vds, N-Channel Enhancement Mode MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "n-channel n channel mosfet enhancement mode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M10-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M10-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M10-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "56A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 10mOhm Ron, 19.5nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M12-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M12-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M12-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "48A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 12mOhm Ron, 15.8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M12-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M12-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M12-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "53A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 12mOhm Ron, 24.8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M15-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M15-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M15-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "42.9A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 15mOhm Ron, 19.4nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M17-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M17-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M17-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "43A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 17mOhm Ron, 29.6nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M19-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M19-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M19-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35.8A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 19mOhm Ron, 17.3nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M21-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M21-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M21-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "33A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 21mOhm Ron, 10.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M22-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M22-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M22-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "37A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 22mOhm Ron, 23.9nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M27-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M27-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M27-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 27mOhm Ron, 19.5nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M33-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M33-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M33-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "24A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 33mOhm Ron, 10.9nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M42-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M42-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M42-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 42mOhm Ron, 9nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M45-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M45-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M45-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 45mOhm Ron, 6.2nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M67-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M67-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M67-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 67mOhm Ron, 6.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M6R3-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M6R3-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M6R3-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "70A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 6.3mOhm Ron, 28.1nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M8R0-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M8R0-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M8R0-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "69A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 8mOhm Ron, 23.8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK7M9R9-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK7M9R9-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK7M9R9-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 9.9mOhm Ron, 30.1nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9832-55A"
		(extends "BSP89")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9832-55A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9832-55A.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12A Id, 55V Vds, RdsOn 25mOhm, N-Channel Enhancement Mode MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "n-channel n channel mosfet enhancement mode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M10-30EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M10-30EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M10-30E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "54A Id, 30V Vds, N-Channel TrenchMOS MOSFET, 7.8mOhm Ron, 12.2nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M11-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M11-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M11-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "53A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 9mOhm Ron, 13.4nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M12-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M12-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M12-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "54A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 11mOhm Ron, - Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M120-100EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M120-100EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M120-100E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "11.5A Id, 100V Vds, N-Channel TrenchMOS MOSFET, 119mOhm Ron, 8.8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M14-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M14-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M14-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "44A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 11mOhm Ron, 11.3nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M15-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M15-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M15-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "47A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 13mOhm Ron, 17nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M156-100EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M156-100EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M156-100E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "9.3A Id, 100V Vds, N-Channel TrenchMOS MOSFET, 150mOhm Ron, 7.4nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M17-30EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M17-30EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M17-30E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "37A Id, 30V Vds, N-Channel TrenchMOS MOSFET, 14mOhm Ron, 8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M19-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M19-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M19-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "38A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 17mOhm Ron, 13.8nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M23-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M23-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M23-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "37A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 20mOhm Ron, 20nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M24-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M24-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M24-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 20mOhm Ron, 7.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M24-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M24-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M24-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 21mOhm Ron, 12.4nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M28-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M28-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M28-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "33A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 25mOhm Ron, 16.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M34-100EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M34-100EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M34-100E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "29A Id, 100V Vds, N-Channel TrenchMOS MOSFET, 34mOhm Ron, 24.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M35-80EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M35-80EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M35-80E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "26A Id, 80V Vds, N-Channel TrenchMOS MOSFET, 31mOhm Ron, 13.5nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M42-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M42-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M42-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "22A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 37mOhm Ron, 8.3nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M43-100EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M43-100EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M43-100E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25A Id, 100V Vds, N-Channel TrenchMOS MOSFET, 43mOhm Ron, 20.2nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M52-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M52-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M52-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "17.6A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 40mOhm Ron, 4.5nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M5R2-30EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M5R2-30EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M5R2-30E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "70A Id, 30V Vds, N-Channel TrenchMOS MOSFET, 4.1mOhm Ron, 22.5nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M6R6-30EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M6R6-30EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M6R6-30E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "70A Id, 30V Vds, N-Channel TrenchMOS MOSFET, 5.3mOhm Ron, 18nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M7R2-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M7R2-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M7R2-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "70A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 5.8mOhm Ron, 19.7nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M85-60EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M85-60EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M85-60E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12.8A Id, 60V Vds, N-Channel TrenchMOS MOSFET, 73mOhm Ron, 4.4nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "BUK9M9R1-40EX"
		(extends "BUK9M53-60EX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BUK9M9R1-40EX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK33"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BUK9M9R1-40E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "64A Id, 40V Vds, N-Channel TrenchMOS MOSFET, 7.3mOhm Ron, 16.2nC Qqd, -55 to 175 °C, LFPAK33"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK33*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0025120D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0025120D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/161/C2M0025120D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "90A Id, 1200V Vds, 25mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0040120D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0040120D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/165/C2M0040120D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 1200V Vds, 40mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0045170D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0045170D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/960/C2M0045170D.000.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "72A Id, 1700V Vds, 45mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0080120D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0080120D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/167/C2M0080120D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "36A Id, 1200V Vds, 80mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0160120D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0160120D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/169/C2M0160120D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 1200V Vds, 160mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M0280120D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M0280120D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/171/C2M0280120D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 1200V Vds, 280mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M1000170D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M1000170D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/173/C2M1000170D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5A Id, 1700V Vds, 1000mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C2M1000170J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C2M1000170J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/820/C2M1000170J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.3A Id, 1700V Vds, 1000mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0065100J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0065100J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/958/C3M0065100J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 1000V Vds, 65mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0065100K"
		(extends "C3M0030090K")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0065100K"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-4_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/961/C3M0065100K.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 1000V Vds, 65mOhm, N-Channel SiC MOSFET, TO-247-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0075120J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0075120J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/997/C3M0075120J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 1200V Vds, 75mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0075120K"
		(extends "C3M0030090K")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0075120K"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-4_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/959/c3m0075120k.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 1200V Vds, 75mOhm, N-Channel SiC MOSFET, TO-247-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0120090D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0120090D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/824/C3M0120090D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "23A Id, 900V Vds, 120mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0120090J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0120090J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/834/C3M0120090J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "22A Id, 900V Vds, 120mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0120100J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0120100J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/957/C3M0120100J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "22A Id, 1000V Vds, 120mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0120100K"
		(extends "C3M0030090K")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0120100K"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-4_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/962/C3M0120100K.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "22A Id, 1000V Vds, 120mOhm, N-Channel SiC MOSFET, TO-247-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0280090D"
		(extends "C3M0065090D")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0280090D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/825/C3M0280090D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "11.5A Id, 900V Vds, 280mOhm, N-Channel SiC MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "C3M0280090J"
		(extends "C3M0065090J")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "C3M0280090J"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-7_TabPin8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.wolfspeed.com/media/downloads/835/C3M0280090J.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "11.5A Id, 900V Vds, 280mOhm, N-Channel SiC MOSFET, TO-263-7"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel SiC MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*TabPin8*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16321Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16321Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16321q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 2.6mOhm Ron, 14nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16322Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16322Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16322q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 5.8mOhm Ron, Qg (typ) 6.8nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16325Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16325Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16325q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 2.2mOhm Ron, 18nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16327Q3"
		(extends "CSD19537Q3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16327Q3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd16327q3.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 25V Vds, NexFET N-Channel Power MOSFET, 3.4mOhm Ron, Qg Typ 6.2nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16342Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16342Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16342q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 5.5mOhm Ron, Qg (typ) 6.5nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16401Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16401Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16401q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 1.6mOhm Ron, 21nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16403Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16403Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16403q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 2.8mOhm Ron, Qg (typ) 13.3nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16404Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16404Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16404q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 5.1mOhm Ron, Qg (typ) 6.5nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16407Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16407Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16407q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 2.4mOhm Ron, Qg (typ) 13.3nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16408Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16408Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16408q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 4.5mOhm Ron, Qg (typ) 6.7nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16410Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16410Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16410q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 8.5mOhm Ron, Qg (typ) 3.9nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16412Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16412Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16412q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 11mOhm Ron, Qg (typ) 2.9nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16413Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16413Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16413q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 3.9mOhm Ron, 9nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16414Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16414Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16414q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 1.9mOhm Ron, Qg (typ) 16.6nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16415Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16415Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16415q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 1.15mOhm Ron, 21nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD16570Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD16570Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd16570q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 25V Vds, NexFET N-Channel Power MOSFET, 0.59mOhm Ron, 95nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17301Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17301Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17301q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3mOhm Ron, 19nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17302Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17302Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17302q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 9mOhm Ron, Qg (typ) 5.4nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17303Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17303Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17303q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2.6mOhm Ron, 18nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17305Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17305Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17305q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2.8mOhm Ron, Qg (typ) 14.1nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17306Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17306Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17306q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 4.2mOhm Ron, Qg (typ) 11.8nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17307Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17307Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17307q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 12.1mOhm Ron, 4nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17310Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17310Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17310q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 5.9mOhm Ron, Qg (typ) 8.9nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17311Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17311Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17311q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2.3mOhm Ron, 24nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17312Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17312Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17312q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 1.7mOhm Ron, 28nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17313Q2"
		(extends "CSD16301Q2")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17313Q2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Texas_DQK"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/csd17313q2.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5A Id, 30V Vds, NexFET N-Channel Power MOSFET, 24mOhm Ron, SON-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DQK*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17322Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17322Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17322q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 12.4mOhm Ron, Qg (typ) 3.6nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17327Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17327Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17327q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 15.5mOhm Ron, Qg (typ) 2.8nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17501Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17501Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17501q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2.9mOhm Ron, Qg (typ) 13.2nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17505Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17505Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17505q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3.5mOhm Ron, 10nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17506Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17506Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17506q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 4mOhm Ron, Qg (typ) 8.3nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17507Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17507Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17507q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 10.8mOhm Ron, Qg (typ) 2.8nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17510Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17510Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17510q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 5.2mOhm Ron, Qg (typ) 6.4nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17522Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17522Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17522q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 8.1mOhm Ron, Qg (typ) 3.6nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17527Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17527Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17527q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 10.8mOhm Ron, Qg (typ) 2.8nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17551Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17551Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17551q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "48A Id, 30V Vds, NexFET N-Channel Power MOSFET, 8.8mOhm Ron, 6nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17552Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17552Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17552q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 30V Vds, NexFET N-Channel Power MOSFET, 6.2mOhm Ron, 9nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17553Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17553Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17553q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3.1mOhm Ron, Qg (typ) 17.5nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17555Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17555Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17555q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2.7mOhm Ron, 23nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17556Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17556Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17556q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 1.4mOhm Ron, Qg (typ) 28.5nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17559Q5"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17559Q5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17559q5"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 1.15mOhm Ron, 39nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17570Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17570Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17570q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 0.69mOhm Ron, 93nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17573Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17573Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17573q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 1mOhm Ron, 49nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17576Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17576Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17576q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 30V Vds, NexFET N-Channel Power MOSFET, 2mOhm Ron, 25nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17577Q3A"
		(extends "CSD19537Q3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17577Q3A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd17577q3a.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 30V Vds, NexFET N-Channel Power MOSFET, 4.0mOhm Ron, Qg Typ 12nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17577Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17577Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17577q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 30V Vds, NexFET N-Channel Power MOSFET, 4.2mOhm Ron, 13nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17579Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17579Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd17579q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25A Id, 30V Vds, NexFET N-Channel Power MOSFET, 9.7mOhm Ron, Qg (typ) 5.4nC, SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD17581Q3A"
		(extends "CSD19537Q3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD17581Q3A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd17581q3a.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 30V Vds, NexFET N-Channel Power MOSFET, 3.2mOhm Ron, Qg Typ 20nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18501Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18501Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18501q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 40V Vds, NexFET N-Channel Power MOSFET, 3.2mOhm Ron, 42nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18502Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18502Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18502q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 40V Vds, NexFET N-Channel Power MOSFET, 2.3mOhm Ron, 52nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18503Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18503Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18503q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 40V Vds, NexFET N-Channel Power MOSFET, 4.3mOhm Ron, 26nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18504Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18504Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18504q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 40V Vds, NexFET N-Channel Power MOSFET, 6.6mOhm Ron, 16nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18509Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18509Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18509q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 40V Vds, NexFET N-Channel Power MOSFET, 1.2mOhm Ron, 150nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18531Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18531Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18531q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 4.6mOhm Ron, 36nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18532NQ5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18532NQ5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18532nq5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 3.4mOhm Ron, 49nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18532Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18532Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18532q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 3.2mOhm Ron, 44nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18533Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18533Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18533q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 5.9mOhm Ron, 29nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18534Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18534Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18534q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 60V Vds, NexFET N-Channel Power MOSFET, 9.8mOhm Ron, 17nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18537NQ5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18537NQ5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18537nq5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 60V Vds, NexFET N-Channel Power MOSFET, 13mOhm Ron, 14nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18540Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18540Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18540q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 2.2mOhm Ron, 41nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18543Q3A"
		(extends "CSD19537Q3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18543Q3A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:VSON-8_3.3x3.3mm_P0.65mm_NexFET"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd18543q3a.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 60V Vds, NexFET N-Channel Power MOSFET, 8.1mOhm Ron, Qg Typ 11.1nC, VSON-8 3.3x3.3mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3.3x3.3mm*P0.65mm*NexFET*"
			(at 0 0 0)
		)
	)
	(symbol "CSD18563Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD18563Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd18563q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 60V Vds, NexFET N-Channel Power MOSFET, 6.8mOhm Ron, 15nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD19502Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19502Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd19502q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 80V Vds, NexFET N-Channel Power MOSFET, 4.1mOhm Ron, 48nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD19531Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19531Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd19531q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, NexFET N-Channel Power MOSFET, 6.4mOhm Ron, 37nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD19532Q5B"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19532Q5B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd19532q5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, NexFET N-Channel Power MOSFET, 4.9mOhm Ron, 48nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD19533Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19533Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd19533q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100A Id, 100V Vds, NexFET N-Channel Power MOSFET, 9.5mOhm Ron, 27nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "CSD19534Q5A"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CSD19534Q5A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/csd19534q5a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50A Id, 100V Vds, NexFET N-Channel Power MOSFET, 15.1mOhm Ron, 17nC Qg(typ), SON8 5x6mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "NexFET Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "DMC3071LVT"
		(extends "DMC2053UVT")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "DMC3071LVT"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMC3071LVT.pdf"
			(at 2.54 -3.81 0)
		)
		(property "Description" "3.4A/-2.7A Id, 30V Vds, Complementary pair enhancement mode P-Channel and N-Channel MOSFET, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "complementary mosfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG2301L"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG2301L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMG2301L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3A Id, -20V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG2302U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG2302U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMG2302U.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG3402L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG3402L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMG3402L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG3404L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG3404L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMG3404L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG3406L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG3406L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMG3406L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.6A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG3414U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG3414U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMG3418L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMG3418L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMG3418L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN10H220L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN10H220L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN10H220L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.6A Id, 100V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN10H700S"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN10H700S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN10H700S.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.7A Id, 100V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN13H750S"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN13H750S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN13H750S.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1A Id, 130V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2040U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2040U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMN2040U.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20V Vds, 6A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2041L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2041L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/products_inactive_data/DMN2041L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2050L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2050L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31502.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.9A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2056U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2056U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN2056U.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2058U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2058U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN2058U.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.6A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2075U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2075U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN2075U.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN2230U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN2230U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31180.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN24H11DS"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN24H11DS"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN24H11DS.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.27A Id, 240V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN24H3D5L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN24H3D5L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN24H3D5L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.48A Id, 240V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3042L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3042L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN3042L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3051L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3051L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31347.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN30H4D0L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN30H4D0L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN30H4D0L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.25A Id, 300V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3110S"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3110S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN3110S.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.3A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3150L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3150L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31126.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3300U"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3300U"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31181.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN3404L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN3404L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31787.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN6075S"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN6075S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN6075S.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2.5A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN60H080DS"
		(extends "DMG1012T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN60H080DS"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMN60H080DS.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "600V Vds, 80mA Id, N-Channel MOSFET with ESD protection, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN6140L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN6140L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN6140L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2.3A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN61D8LQ"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN61D8LQ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMN61D8LQ.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60V Vds, 0.470A Id, N-Channel MOSFET for switching inductive loads , SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET relay logic-level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN67D7L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN67D7L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN67D7L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.21A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMN67D8L"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMN67D8L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN67D8L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.21A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMP3099L"
		(extends "Q_PMOS_GSD")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMP3099L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP3099L.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.8A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "DMP6050SSD"
		(extends "IRF7324")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DMP6050SSD"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP6050SSD.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-11.3A Id, -60V Vds, P-Channel Power MOSFET, 55mOhm Ron, 11.9nC Qg (typ), SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual PMOS P-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC2036"
		(extends "EPC2035")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2036"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2036_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100 V E-mode GaN transistor, RdsOn 73 mOhm, 1.7A Id, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC2037"
		(extends "EPC2035")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2037"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2037_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100 V E-mode GaN transistor, RdsOn 550 mOhm, 1.7A Id, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC2038"
		(extends "EPC2035")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2038"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2038_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "100 V E-mode GaN transistor, RdsOn 3.3 Ohm, 0.5A Id, Integrated Reverse Gate Clamp Diode, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC2203"
		(extends "EPC2035")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2203"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2203_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "80 V E-mode GaN transistor, RdsOn 80 mOhm, 1.7A Id, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "EPC2219"
		(extends "EPC2035")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "EPC2219"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_BGA:EPC_BGA-4_0.9x0.9mm_Layout2x2_P0.45mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2219_datasheet.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "65 V E-mode GaN transistor, RdsOn 3.3 Ohm, 0.5A Id, Integrated Reverse Gate Clamp Diode, EPC_BGA-4_0.9x0.9mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "hemt enhancement"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EPC?BGA*0.9x0.9mm?Layout2x2?P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDC86244"
		(extends "FDC2512")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDC86244"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SuperSOT-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDC86244-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2.3A Id, 150V Vds, N-Channel MOSFET, 144mOhm Ron, SuperSOT-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SuperSOT*"
			(at 0 0 0)
		)
	)
	(symbol "FDG6335N"
		(extends "FDG1024NZ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDG6335N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.gneic.com/product/datasheet/FDG6335N-1122853.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.7A Id, 20V Vds, Dual N-Channel MOSFET, 300mOhm Ron, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS8050"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS8050"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS8050-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 30V Vds, N-Channel PowerTrench MOSFET, 0.65mOhm Ron, 285nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS8050ET30"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS8050ET30"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS8050ET30-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 30V Vds, N-Channel PowerTrench MOSFET, 0.65mOhm Ron, 285nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS8350L"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS8350L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS8350L-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "47A Id, 40V Vds, N-Channel PowerTrench MOSFET, 0.85mOhm Ron, 242nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS8350LET40"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS8350LET40"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS8350LET40-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "49A Id, 40V Vds, N-Channel PowerTrench MOSFET, 0.85mOhm Ron, 242nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench-MOSFET MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86150"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86150"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86150ET100-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 100V Vds, N-Channel PowerTrench MOSFET, 4.85mOhm Ron, 62nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86150ET100"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86150ET100"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.mouser.fr/datasheet/2/308/FDMS86150ET100-D-1807744.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 100V Vds, N-Channel PowerTrench MOSFET, 4.85mOhm Ron, 62nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench-MOSFET MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86152"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86152"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.mouser.fr/datasheet/2/308/FDMS86152-D-1808412.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 100V Vds, N-Channel PowerTrench MOSFET, 6mOhm Ron, 50nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86202"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86202"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.mouser.fr/datasheet/2/308/FDMS86202-D-1808220.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13.5A Id, 120V Vds, N-Channel Shielded Gate PowerTrench MOSFET, 7.2mOhm Ron, 64nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "shielded-gate-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86202ET120"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86202ET120"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86202ET120-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13.5A Id, 120V Vds, N-Channel Shielded Gate PowerTrench MOSFET, 7.2mOhm Ron, 64nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "shielded-gate-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86255"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86255"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86255-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 150V Vds, N-Channel Shielded Gate PowerTrench MOSFET, 12.4mOhm Ron, 63nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "shielded-gate-powertrench-MOSFET MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86255ET150"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86255ET150"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86255ET150-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 150V Vds, N-Channel Shielded Gate PowerTrench MOSFET, 12.4mOhm Ron, 63nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "shielded-gate-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86350"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86350"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86350-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25A Id, 80V Vds, N-Channel PowerTrench MOSFET, 2.4mOhm Ron, 155nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86350ET80"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86350ET80"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86350ET80-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25A Id, 80V Vds, N-Channel PowerTrench MOSFET, 2.4mOhm Ron, 155nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86550"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86550"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86550-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 60V Vds, N-Channel PowerTrench MOSFET, 1.65mOhm Ron, 154nC Qgmax, -55 to 150 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMS86550ET60"
		(extends "CSD17578Q5A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMS86550ET60"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TDSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMS86550ET60-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 60V Vds, N-Channel PowerTrench MOSFET, 1.65mOhm Ron, 154nC Qgmax, -55 to 175 °C, 5x6mm SON8"
			(at 0 0 0)
		)
		(property "ki_keywords" "powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDSON*"
			(at 0 0 0)
		)
	)
	(symbol "FDMT800100DC"
		(extends "FDMT80060DC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT800100DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT800100DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "24A Id, 100V Vds, N-Channel Dual Cool PowerTrench MOSFET, 2.95mOhm Ron, 111nC Qgmax, -55 to 150 °C, 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-cool-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
	)
	(symbol "FDMT800120DC"
		(extends "FDMT80060DC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT800120DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT800120DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20A Id, 120V Vds, N-Channel Dual cool 88 PowerTrench MOSFET, 4.2mOhm Ron, 107nC Qgmax, -55 to 150 °C, 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-cool-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
	)
	(symbol "FDMT800150DC"
		(extends "FDMT80060DC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT800150DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT800150DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15A Id, 150V Vds, N-Channel Dual cool PowerTrench MOSFET, 6.5mOhm Ron, 108nC Qgmax, -55 to 150 °C, 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-cool-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
	)
	(symbol "FDMT800152DC"
		(extends "FDMT80060DC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT800152DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT800152DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 150V Vds, N-Channel Dual Cool PowerTrench MOSFET, 9.0mOhm Ron, 83nC Qgmax, -55 to 150 °C, 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-cool-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
	)
	(symbol "FDMT80080DC"
		(extends "FDMT80060DC")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDMT80080DC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:PQFN_8x8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDMT80080DC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "36A Id, 80V Vds, N-Channel Dual Cool PowerTrench MOSFET, 1.35mOhm Ron, 273nC Qgmax, -55 to 150 °C, 8x8mm MLP"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual-cool-powertrench MOSFET fairchild"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFN*8x8*"
			(at 0 0 0)
		)
	)
	(symbol "FDN340P"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDN340P"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDN340P-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-2A Id, -20V Vds, P-Channel MOSFET, 70mOhm Ron, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "FDS2734"
		(extends "IRF8721PBF-1")
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "FDS2734"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FDS2734-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.0A Id, 250V Vds, N-Channel MOSFET, 117mOhm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS4559"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS4559"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS4559-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.5A Id, 60V Vds, Dual N and P Channel MOSFET, 55mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS4897AC"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS4897AC"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS4897AC-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.1A Id, 40V Vds, Dual N and P Channel MOSFET, 26mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS4897C"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS4897C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS4897C-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.2A Id, 40V Vds, Dual N and P Channel MOSFET, 29mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS6630A"
		(extends "IRF8721PBF-1")
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "FDS6630A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FDS6630A-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.5A Id, 30V Vds, N-Channel MOSFET, 38mOhm Ron, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS6892A"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS6892A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS6892A-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7.5A Id, 20V Vds, Dual N-Channel MOSFET PWM Optimized, 18mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET Low Gate Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS6898A"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS6898A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS6898A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "9.4A Id, 20V Vds, Dual N-Channel MOSFET, 14mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS6930A"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS6930A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FDS6930A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.5A Id, 30V Vds, Dual N-Channel Logic Level MOSFET, 40mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS6930B"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS6930B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FDS6930B-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.5A Id, 30V Vds, Dual N-Channel Logic Level MOSFET, 38mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS8960C"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS8960C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.mouser.fr/datasheet/2/308/FDS8960C-D-1808807.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "7A Id, 35V Vds, Dual N and P Channel MOSFET, 24mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS9435A"
		(extends "IRF7404")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS9435A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS9435A-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-5.3A Id, -30V Vds, P-Channel MOSFET, 50mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS9926A"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS9926A"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS9926A-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.5A Id, 20V Vds, Dual N-Channel MOSFET, 30mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FDS9934C"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FDS9934C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FDS9934C-D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.5A Id, 20V Vds, Dual N and P Channel MOSFET, 30mOhm Ron, 4.5V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FQP27P06"
		(extends "IRF9540N")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "FQP27P06"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FQP27P06-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-27A Id, -60V Vds, QFET P-Channel MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "QFET P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "GS66504B"
		(extends "GS66502B")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "GS66504B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Transistor_Power:GaN_Systems_GaNPX-3_5x6.6mm_Drain3.76x0.6mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://gansystems.com/wp-content/uploads/2020/04/GS66504B-DS-Rev-200402.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Bottom-side cooled 650 V E-mode GaN transistor, 15A Id, GaN_PX"
			(at 0 0 0)
		)
		(property "ki_keywords" "gan hemt bottom-side-cooled enhancement-mode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "GaN?Systems?GaNPX*5x6.6mm*Drain3.76x0.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "IGLD60R190D1"
		(extends "IGLD60R070D1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGLD60R190D1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SON:Infineon_PG-LSON-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGLD60R190D1-DataSheet-v02_00-EN.pdf?fileId=5546d46269e1c019016a6d78ff5e2aba"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 600V Vds, 190mOhm, N-Channel GaN MOSFET, LSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*LSON*1*"
			(at 0 0 0)
		)
	)
	(symbol "IGT40R070D1_E8220"
		(extends "IGT60R070D1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGT40R070D1_E8220"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-3_ThermalVias"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGT40R070D1%20E8220-DataSheet-v02_00-EN.pdf?fileId=5546d4626afcd350016b269dd8f34ec4"
			(at 5.08 -3.81 0)
		)
		(property "Description" "31A Id, 400V Vds, 70mOhm, N-Channel GaN MOSFET, HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*3*"
			(at 0 0 0)
		)
	)
	(symbol "IGT60R190D1S"
		(extends "IGT60R070D1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IGT60R190D1S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-3_ThermalVias"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IGT60R190D1S-DataSheet-v03_01-EN.pdf?fileId=5546d46265f064ff016685fa29796520"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12.5A Id, 600V Vds, 190mOhm, N-Channel GaN MOSFET, HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*3*"
			(at 0 0 0)
		)
	)
	(symbol "IPD50R3K0CE"
		(extends "IPD50R380CE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPD50R3K0CE"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/IPx50R3K0CE_2_0.pdf?folderId=db3a3043163797a6011637d4bae7003b&fileId=db3a304339dcf4b10139e7e9ff592ce4"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.7A Id, 500V Vds, CoolMOS N-Channel Power MOSFET, 3Ohm Ron, 4.3nC Qg (typ), TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "CoolMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "IPDD60R080G7"
		(extends "IPDD60R050G7")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R080G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R080G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a016170882f757a07"
			(at 5.08 -3.81 0)
		)
		(property "Description" "29A Id, 600V Vds, 80mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IPDD60R102G7"
		(extends "IPDD60R050G7")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R102G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R102G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a01617087ee7379ed"
			(at 5.08 -3.81 0)
		)
		(property "Description" "23A Id, 600V Vds, 102mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IPDD60R125G7"
		(extends "IPDD60R050G7")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R125G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R125G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a0161706cba27778f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20A Id, 600V Vds, 125mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IPDD60R150G7"
		(extends "IPDD60R050G7")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R150G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R150G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a016170806aa57863"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 600V Vds, 150mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IPDD60R190G7"
		(extends "IPDD60R050G7")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPDD60R190G7"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HDSOP-10-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPDD60R190G7-DS-v02_00-EN.pdf?fileId=5546d4626102d35a01617087dc0f79ea"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 600V Vds, 190mOhm, N-Channel MOSFET, CoolMOS G7, PG-HDSOP-10-1 (DDPAK)"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HDSOP*"
			(at 0 0 0)
		)
	)
	(symbol "IPP060N06N"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPP060N06N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IPP060N06N-DS-v02_02-en.pdf?fileId=db3a30433727a44301372c06d9d7498a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "45A Id, 60V Vds, Single N-Channel Power MOSFET, 6mOhm Ron, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET Infineon"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IPT015N10N5"
		(extends "IPT012N08N5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPT015N10N5"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-IPT015N10N5-DS-v02_01-EN.pdf?fileId=5546d4624a75e5f1014ac94680661aff"
			(at 5.08 -3.81 0)
		)
		(property "Description" "300A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 1.5mOhm Ron, Qg (typ) 169.0nC, PG-HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*"
			(at 0 0 0)
		)
	)
	(symbol "IPT020N10N3"
		(extends "IPT012N08N5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IPT020N10N3"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Infineon_PG-HSOF-8-1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-IPT020N10N3-DS-v02_00-en.pdf?fileId=db3a30433e9d5d11013e9e58035b0158"
			(at 5.08 -3.81 0)
		)
		(property "Description" "300A Id, 100V Vds, OptiMOS N-Channel Power MOSFET, 2.0mOhm Ron, Qg (typ) 156.0nC, PG-HSOF-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OptiMOS Power MOSFET N-MOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG*HSOF*"
			(at 0 0 0)
		)
	)
	(symbol "IRF3205"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF3205"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf3205.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "110A Id, 55V Vds, Single N-Channel HEXFET Power MOSFET, 8mOhm Ron, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single N-Channel HEXFET Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRF4905"
		(extends "IRF9540N")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF4905"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irf4905.pdf?fileId=5546d462533600a4015355e32165197c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-74A Id, -55V Vds, Single P-Channel HEXFET Power MOSFET, 20mOhm Ron, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single P-Channel HEXFET Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRF540N"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF540N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irf540n.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "33A Id, 100V Vds, HEXFET N-Channel MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "HEXFET N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6614"
		(extends "BSF450NE7NH3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6614"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ST"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6614pbf.pdf?fileId=5546d462533600a4015355e8346c1a0f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12.7A Id, 40V Vds, 8.3mOhm Rds, N-Channel MOSFET, DirectFET ST"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ST*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6616"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6616"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6616pbf.pdf?fileId=5546d462533600a4015355e843461a13"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 40V Vds, 5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6617"
		(extends "BSF450NE7NH3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6617"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ST"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6617pbf.pdf?fileId=5546d462533600a4015355e853f21a17"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 30V Vds, 8.1mOhm Rds, N-Channel MOSFET, DirectFET ST"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ST*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6618"
		(extends "IRF6613")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6618"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MT"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6618pbf.pdf?fileId=5546d462533600a4015355e862c21a1b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "170A Id, 30V Vds, 2.2mOhm Rds, N-Channel MOSFET, DirectFET MT"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MT*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6620"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6620"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6620pbf.pdf?fileId=5546d462533600a4015355e8831d1a23"
			(at 5.08 -3.81 0)
		)
		(property "Description" "150A Id, 20V Vds, 2.7mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6621"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6621"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6621pbf.pdf?fileId=5546d462533600a4015355e8923b1a27"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12A Id, 30V Vds, 9.1mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6622"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6622"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6622pbf.pdf?fileId=5546d462533600a4015355e89a3a1a29"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15A Id, 25V Vds, 6.3mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6623"
		(extends "BSF450NE7NH3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6623"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ST"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6623pbf.pdf?fileId=5546d462533600a4015355e8aa811a2d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 20V Vds, 5.7mOhm Rds, N-Channel MOSFET, DirectFET ST"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ST*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6628"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6628"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6628pbf.pdf?fileId=5546d462533600a4015355e8c0d71a33"
			(at 5.08 -3.81 0)
		)
		(property "Description" "27A Id, 25V Vds, 2.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6631"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6631"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6631pbf.pdf?fileId=5546d462533600a4015355e8d0561a37"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 30V Vds, 7.8mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6635"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6635"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6635pbf.pdf?fileId=5546d462533600a4015355e8e7ab1a3d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 30V Vds, 1.8mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6636"
		(extends "BSF450NE7NH3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6636"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ST"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6636pbf.pdf?fileId=5546d462533600a4015355e8f7b31a41"
			(at 5.08 -3.81 0)
		)
		(property "Description" "18A Id, 20V Vds, 4.5mOhm Rds, N-Channel MOSFET, DirectFET ST"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ST*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6637"
		(extends "BSB104N08NP3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6637"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MP"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6637pbf.pdf?fileId=5546d462533600a4015355ec1fab1a45"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 30V Vds, 7.7mOhm Rds, N-Channel MOSFET, DirectFET MP"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MP*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6641"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6641"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6641pbf.pdf?fileId=5546d462533600a4015355ec30311a49"
			(at 5.08 -3.81 0)
		)
		(property "Description" "26A Id, 200V Vds, 59.9mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6643"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6643"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6643pbf.pdf?fileId=5546d462533600a4015355ec388f1a4b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 150V Vds, 34.5mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6644"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6644"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF6644-DS-v01_01-EN.pdf?fileId=5546d462533600a4015355ec47ac1a4f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "57A Id, 100V Vds, 13mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6646"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6646"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6646pbf.pdf?fileId=5546d462533600a4015355ec5f071a55"
			(at 5.08 -3.81 0)
		)
		(property "Description" "12A Id, 80V Vds, 9.5mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6648"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6648"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF6648-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ec6e561a59"
			(at 5.08 -3.81 0)
		)
		(property "Description" "86A Id, 60V Vds, 7mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6662"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6662"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6662pbf.pdf?fileId=5546d462533600a4015355ec7edc1a5d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "8.3A Id, 100V Vds, 22mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6665"
		(extends "IRF6655")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6665"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SH"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6665pbf.pdf?fileId=5546d462533600a4015355ec8dcb1a62"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 100V Vds, 62mOhm Rds, N-Channel MOSFET, DirectFET SH"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SH*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6668"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6668"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6668pbf.pdf?fileId=5546d462533600a4015355ec96b91a64"
			(at 5.08 -3.81 0)
		)
		(property "Description" "55A Id, 80V Vds, 15mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6674"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6674"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6674pbf.pdf?fileId=5546d462533600a4015355ec9f0d1a66"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13.4A Id, 60V Vds, 11mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6711S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6711S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6711spbf.pdf?fileId=5546d462533600a4015355ecec0b1a7a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 25V Vds, 3.8mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6712S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6712S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6712spbf.pdf?fileId=5546d462533600a4015355ecf4331a7c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "17A Id, 25V Vds, 4.9mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6713S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6713S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6713spbf.pdf?fileId=5546d462533600a4015355ecfc5c1a7e"
			(at 5.08 -3.81 0)
		)
		(property "Description" "22A Id, 25V Vds, 3mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6714M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6714M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6714mpbf.pdf?fileId=5546d462533600a4015355ed04be1a80"
			(at 5.08 -3.81 0)
		)
		(property "Description" "29A Id, 25V Vds, 2.1mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6715M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6715M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6715mpbf.pdf?fileId=5546d462533600a4015355ed0d221a82"
			(at 5.08 -3.81 0)
		)
		(property "Description" "34A Id, 25V Vds, 1.6mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6716M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6716M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6716mpbf.pdf?fileId=5546d462533600a4015355ed15241a84"
			(at 5.08 -3.81 0)
		)
		(property "Description" "39A Id, 25V Vds, 1.6mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6717M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6717M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6717mpbf.pdf?fileId=5546d462533600a4015355ed1d801a86"
			(at 5.08 -3.81 0)
		)
		(property "Description" "38A Id, 25V Vds, 1.25mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6721S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6721S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6721spbf.pdf?fileId=5546d462533600a4015355ed33b51a8c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "14A Id, 30V Vds, 7.3mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6722M"
		(extends "BSB104N08NP3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6722M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MP"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6722mpbf.pdf?fileId=5546d462533600a4015355ed3c661a8e"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 30V Vds, 7.7mOhm Rds, N-Channel MOSFET, DirectFET MP"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MP*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6724M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6724M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6724mpbf.pdf?fileId=5546d462533600a4015355ed51a01a94"
			(at 5.08 -3.81 0)
		)
		(property "Description" "27A Id, 30V Vds, 2.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6725M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6725M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6725mpbf.pdf?fileId=5546d462533600a4015355ed59ca1a96"
			(at 5.08 -3.81 0)
		)
		(property "Description" "28A Id, 30V Vds, 2.2mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6726M"
		(extends "IRF6613")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6726M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MT"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6726mpbf.pdf?fileId=5546d462533600a4015355ed61db1a98"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 30V Vds, 1.7mOhm Rds, N-Channel MOSFET, DirectFET MT"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MT*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6727M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6727M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6727mpbf.pdf?fileId=5546d462533600a4015355ed6a331a9a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 30V Vds, 1.7mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6728M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6728M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6728mpbf.pdf?fileId=5546d462533600a4015355ed73701a9c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "23A Id, 30V Vds, 2.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6775M"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6775M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6775mpbf.pdf?fileId=5546d462533600a4015355ed84751aa0"
			(at 5.08 -3.81 0)
		)
		(property "Description" "28A Id, 150V Vds, 56mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6785"
		(extends "BSB165N15NZ3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6785"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MZ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6785mpbf.pdf?fileId=5546d462533600a4015355ed8cc31aa2"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 200V Vds, 100mOhm Rds, N-Channel MOSFET, DirectFET MZ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MZ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6795M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6795M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6795mpbf.pdf?fileId=5546d462533600a4015355ed99cd1aa6"
			(at 5.08 -3.81 0)
		)
		(property "Description" "32A Id, 25V Vds, 1.8mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6797M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6797M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6797mpbf.pdf?fileId=5546d462533600a4015355eda2091aa9"
			(at 5.08 -3.81 0)
		)
		(property "Description" "36A Id, 25V Vds, 1.4mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6798M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6798M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6798mpbf.pdf?fileId=5546d462533600a4015355edaa4b1aab"
			(at 5.08 -3.81 0)
		)
		(property "Description" "37A Id, 25V Vds, 1.3mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6810S"
		(extends "IRF6710S2")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6810S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_S1"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6810spbf.pdf?fileId=5546d462533600a4015355f0ab331ab4"
			(at 5.08 -3.81 0)
		)
		(property "Description" "16A Id, 25V Vds, 5.2mOhm Rds, N-Channel MOSFET, DirectFET S1"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*S1*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6811S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6811S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6811spbf.pdf?fileId=5546d462533600a4015355f0b3661ab6"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19A Id, 25V Vds, 3.7mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6893M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6893M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6893mpbf.pdf?fileId=5546d462533600a4015355f0c3de1aba"
			(at 5.08 -3.81 0)
		)
		(property "Description" "29A Id, 25V Vds, 1.6mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6894M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6894M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF6894M-DS-v02_00-EN.pdf?fileId=5546d462533600a4015355f0cc041abc"
			(at 5.08 -3.81 0)
		)
		(property "Description" "37A Id, 25V Vds, 1.3mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF6898M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF6898M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf6898mpbf.pdf?fileId=5546d462533600a4015355f0d4611abe"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 25V Vds, 1.1mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7171M"
		(extends "BSB028N06NN3")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7171M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MN"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7171mpbf.pdf?fileId=5546d462533600a4015355f1326f1ad6"
			(at 5.08 -3.81 0)
		)
		(property "Description" "93A Id, 100V Vds, 6.5mOhm Rds, N-Channel MOSFET, DirectFET MN"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MN*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7343PBF"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7343PBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7343pbf.pdf?fileId=5546d462533600a4015355f68c1a1b73"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 55V Vds, Dual HEXFET N- and P-channel MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual HEXFET N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRF740"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF740"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/91054/91054.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 400V Vds, N-Channel Power MOSFET, 500mOhm Rds, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N Channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7403"
		(extends "IRF8721PBF-1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7403"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7403pbf.pdf?fileId=5546d462533600a4015355fa23541b9c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "9.7A Id, 30V Vds, N-Channel HEXFET Power MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7480M"
		(extends "IRF60DM206")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7480M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ME"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF7480M-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ff8fa41c30"
			(at 5.08 -3.81 0)
		)
		(property "Description" "330A Id, 40V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET ME"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ME*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7483M"
		(extends "IRF40DM229")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7483M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MF"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7483mpbf.pdf?fileId=5546d462533600a4015355ff98011c32"
			(at 5.08 -3.81 0)
		)
		(property "Description" "135A Id, 40V Vds, 2.3mOhm Rds, N-Channel MOSFET, DirectFET MF"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MF*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7486M"
		(extends "IRF60DM206")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7486M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ME"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRL7486M-DS-v01_00-EN.pdf?fileId=5546d46258fc0bc10158fec7a83a0629"
			(at 5.08 -3.81 0)
		)
		(property "Description" "209A Id, 40V Vds, 1.25mOhm Rds, N-Channel MOSFET, DirectFET ME"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ME*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7580M"
		(extends "IRF60DM206")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7580M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ME"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7580mpbf.pdf?fileId=5546d462533600a401535603855c1c72"
			(at 5.08 -3.81 0)
		)
		(property "Description" "114A Id, 60V Vds, 3.6mOhm Rds, N-Channel MOSFET, DirectFET ME"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ME*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7748L1"
		(extends "IRF6718L2")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7748L1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7748l1pbf.pdf?fileId=5546d462533600a40153560434c11c9e"
			(at 5.08 -3.81 0)
		)
		(property "Description" "104A Id, 60V Vds, 2.2mOhm Rds, N-Channel MOSFET, DirectFET L6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L6*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7759L2"
		(extends "IRF7739L1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7759L2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7759l2pbf.pdf?fileId=5546d462533600a40153560478171cb0"
			(at 5.08 -3.81 0)
		)
		(property "Description" "160A Id, 75V Vds, 2.3mOhm Rds, N-Channel MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7769L1"
		(extends "IRF7739L1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7769L1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRF7769L1-DS-v02_00-EN.pdf?fileId=5546d462533600a4015356079bd91cb4"
			(at 5.08 -3.81 0)
		)
		(property "Description" "88A Id, 100V Vds, 3.5mOhm Rds, N-Channel MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7779L2"
		(extends "IRF7739L1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7779L2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7779l2pbf.pdf?fileId=5546d462533600a401535607ac011cb8"
			(at 5.08 -3.81 0)
		)
		(property "Description" "67A Id, 150V Vds, 11mOhm Rds, N-Channel MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7780M"
		(extends "IRF60DM206")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7780M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_ME"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7780mpbf.pdf?fileId=5546d462533600a401535607b41f1cba"
			(at 5.08 -3.81 0)
		)
		(property "Description" "89A Id, 75V Vds, 5.7mOhm Rds, N-Channel MOSFET, DirectFET ME"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*ME*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7799L2"
		(extends "IRF7739L1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7799L2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7799l2pbf.pdf?fileId=5546d462533600a401535607bc471cbc"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 250V Vds, 38mOhm Rds, N-Channel MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
	)
	(symbol "IRF7946"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF7946"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf7946pbf.pdf?fileId=5546d462533600a40153560cc0a41d43"
			(at 5.08 -3.81 0)
		)
		(property "Description" "198A Id, 40V Vds, 1.4mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8301M"
		(extends "IRF6613")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8301M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MT"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8301mpbf.pdf?fileId=5546d462533600a40153560d0e7a1d58"
			(at 5.08 -3.81 0)
		)
		(property "Description" "34A Id, 30V Vds, 1.5mOhm Rds, N-Channel MOSFET, DirectFET MT"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MT*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8302M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8302M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8302mpbf.pdf?fileId=5546d462533600a40153560d16e41d5b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "31A Id, 30V Vds, 1.8mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8304M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8304M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8304mpbf.pdf?fileId=5546d462533600a40153560d20db1d5d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "28A Id, 30V Vds, 2.2mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8306M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8306M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8306mpbf.pdf?fileId=5546d462533600a40153560d29371d5f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "23A Id, 30V Vds, 2.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8308M"
		(extends "BSB008NE2LX")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8308M"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_MX"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8308mpbf.pdf?fileId=5546d462533600a40153560d319d1d61"
			(at 5.08 -3.81 0)
		)
		(property "Description" "27A Id, 30V Vds, 2.5mOhm Rds, N-Channel MOSFET, DirectFET MX"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*MX*"
			(at 0 0 0)
		)
	)
	(symbol "IRF8327S"
		(extends "BSF030NE2LQ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRF8327S"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SQ"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irf8327spbf.pdf?fileId=5546d462533600a40153560d40c41d65"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 30V Vds, 7.3mOhm Rds, N-Channel MOSFET, DirectFET SQ"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SQ*"
			(at 0 0 0)
		)
	)
	(symbol "IRFI4020H"
		(extends "IRFI4019H")
		(property "Reference" "Q"
			(at 5.08 4.445 0)
		)
		(property "Value" "IRFI4020H"
			(at 5.08 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfi4020h-117p.pdf?fileId=5546d462533600a401535623e7271f73"
			(at 5.08 -3.81 0)
		)
		(property "Description" "9.1A Id, 200V Vds, 80mOhm Rds, Dual Half Bridge N-Channel MOSFET, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET Half-Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*P3.4x2.06mm*StaggerEven*Lead1.86mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRFI4212H"
		(extends "IRFI4019H")
		(property "Reference" "Q"
			(at 5.08 4.445 0)
		)
		(property "Value" "IRFI4212H"
			(at 5.08 2.54 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfi4212h-117p.pdf?fileId=5546d462533600a401535623fc841f7a"
			(at 5.08 -3.81 0)
		)
		(property "Description" "11A Id, 100V Vds, 58mOhm Rds, Dual Half Bridge N-Channel MOSFET, TO-220-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET Half-Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220F*P3.4x2.06mm*StaggerEven*Lead1.86mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRFP4468PbF"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFP4468PbF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfp4468pbf.pdf?fileId=5546d462533600a40153562c73472019"
			(at 5.08 -3.81 0)
		)
		(property "Description" "195A Id, 100V Vds, N-Channel Power MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "IRFP4668PbF"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFP4668PbF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-247-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfp4668pbf.pdf?fileId=5546d462533600a40153562c8528201d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "130A Id, 200V Vds, N-Channel Power MOSFET, TO-247"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?247*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4115"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4115"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfs4115pbf.pdf?fileId=5546d462533600a401535636e5d2218f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "99A Id, 150V Vds, 10.3mOhm Rds, N-Channel HEXFET Power MOSFET, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4127"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4127"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfs4127pbf.pdf?fileId=5546d462533600a401535636ee7b2192"
			(at 5.08 -3.81 0)
		)
		(property "Description" "72A Id, 200V Vds, 18.6mOhm Rds, N-Channel MOSFET, 18.6mOhm Ron, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4227"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4227"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfs4227pbf.pdf?fileId=5546d462533600a401535639ef64219b"
			(at 5.08 -3.81 0)
		)
		(property "Description" "130A Id, 200V Vds, 22mOhm Rds, N-Channel MOSFET, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4229"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4229"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfs4229pbf.pdf?fileId=5546d462533600a401535639fdc421a1"
			(at 5.08 -3.81 0)
		)
		(property "Description" "91A Id, 250V Vds, 42mOhm Rds, N-Channel MOSFET, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4310Z"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4310Z"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfb4310zpbf.pdf?fileId=5546d462533600a4015356161b4d1e2d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "120A Id, 100V Vds, 4.8mOhm Rds, N-Channel HEXFET Power MOSFET, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRFS4321"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRFS4321"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irfs4321pbf.pdf?fileId=5546d462533600a40153563a20dd21ad"
			(at 5.08 -3.81 0)
		)
		(property "Description" "85A Id, 150V Vds, 12mOhm Rds, N-Channel HEXFET Power MOSFET, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET HEXFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "IRL6297SD"
		(extends "IRF6802SD")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRL6297SD"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_SA"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irl6297sdpbf.pdf?fileId=5546d462533600a40153565ff22f2575"
			(at 5.08 -3.81 0)
		)
		(property "Description" "15A Id, 20V Vds, 4.9mOhm Rds, Dual N-Channel HEXFET Power MOSFET, DirectFET SA"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*SA*"
			(at 0 0 0)
		)
	)
	(symbol "IRL7472L1"
		(extends "IRF7739L1")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRL7472L1"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DirectFET:DirectFET_L8"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRL7472L1-DS-v02_00-EN.pdf?fileId=5546d46254e133b401555d17178250d8"
			(at 5.08 -3.81 0)
		)
		(property "Description" "375A Id, 40V Vds, 0.45mOhm Rds, N-Channel HEXFET Power MOSFET, DirectFET L8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level IRFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DirectFET*L8*"
			(at 0 0 0)
		)
	)
	(symbol "IRLB8721PBF"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLB8721PBF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irlb8721pbf.pdf?fileId=5546d462533600a40153566056732591"
			(at 5.08 -3.81 0)
		)
		(property "Description" "62A Id, 30V Vds, 8.7 mOhm Rds, N-Channel HEXFET Power MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML0030"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML0030"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml0030pbf.pdf?fileId=5546d462533600a401535664773825df"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.3A Id, 30V Vds, 27mOhm Rds, N-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML2060"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML2060"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml2060pbf.pdf?fileId=5546d462533600a401535664b7fb25ee"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.2A Id, 60V Vds, 480mOhm Rds, N-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML5203"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML5203"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml5203pbf.pdf?fileId=5546d462533600a40153566868da261d"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.0A Id, -30V Vds, 98mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel HEXFET MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML6244"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML6244"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRLML6244-DataSheet-v01_01-EN.pdf?fileId=5546d462533600a4015356686fed261f"
			(at 5.08 -3.81 0)
		)
		(property "Description" "6.3A Id, 20V Vds, 21mOhm Rds, N-Channel StrongIRFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel StrongIRFET MOSFET Load switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML6401"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML6401"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml6401pbf.pdf?fileId=5546d462533600a401535668b96d2634"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-4.3A Id, -12V Vds, 50mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML6402"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML6402"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml6402pbf.pdf?fileId=5546d462533600a401535668d5c2263c"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.7A Id, -20V Vds, 65mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel HEXFET MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLML9301"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLML9301"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml9301pbf.pdf?fileId=5546d462533600a401535668e5e42640"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.6A Id, -30V Vds, 64mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "IRLZ24"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLZ24"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/91326/sihlz24.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "17A Id, 60V Vds, N-Channel Power MOSFET, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRLZ34N"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLZ34N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irlz34npbf.pdf?fileId=5546d462533600a40153567206892720"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30A Id, 55V Vds, 35mOhm Rds, N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "IRLZ44N"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "IRLZ44N"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.irf.com/product-info/datasheets/data/irlz44n.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "47A Id, 55V Vds, 22mOhm Rds Single N-Channel HEXFET Power MOSFET, TO-220AB"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel HEXFET MOSFET Logic-Level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "JFE150DCK"
		(extends "JFE150DBV")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "JFE150DCK"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/jfe150.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra-Low-Noise, Low-Gate-Current, Audio, N-Channel JFET, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "low noise n-channel jfet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70?5*"
			(at 0 0 0)
		)
	)
	(symbol "MMBF170"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBF170"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30104.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.5A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBF4391"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBF4391"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBF4391LT1-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "50mA min, 30V, 30mOhm max, 4-10V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBF4392"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBF4392"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBF4391LT1-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "25mA min, 30V, 60mOhm max, 2-5V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBF4393"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBF4393"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBF4391LT1-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5mA min, 30V, 100mOhm max, 0.5-3V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBFJ111"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBFJ111"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBFJ113-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "20mA min, 35V, 30mOhm max, 3-10V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBFJ112"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBFJ112"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBFJ113-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5mA min, 35V, 50mOhm max, 1-5V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MMBFJ113"
		(extends "BSR56")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "MMBFJ113"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MMBFJ113-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2mA min, 35V, 100mOhm max, 0.5-3V Vgs(off), N-Channel JFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel FET Transistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "NDT3055L"
		(extends "BSP89")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "NDT3055L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ndt3055l-d.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 60V Vds, N-Channel Logic Level Enhancement Mode MOSFET, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "n channel fet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "NTR2101P"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "NTR2101P"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NTR2101P-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.7A Id, -8V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "PGA26E19BA"
		(extends "PGA26E07BA")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PGA26E19BA"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:Panasonic_HSON-8_8x8mm_P2.00mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/PGA26E19BA_E.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "13A Id, 600V Vds, 140mOhm, N-Channel GaN MOSFET, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel GaN MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Panasonic*HSON*8x8mm*P2.00mm*"
			(at 0 0 0)
		)
	)
	(symbol "PMDT290UCE"
		(extends "BSD235C")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "PMDT290UCE"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-666"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PMDT290UCE.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Nexperia 20 / 20 V, 800 / 550 mA N/P-channel Trench MOSFET, SOT-666"
			(at 0 0 0)
		)
		(property "ki_keywords" "Trench MOSFET complementary nmos pmos nexperia"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?666*"
			(at 0 0 0)
		)
	)
	(symbol "QM6006D"
		(extends "IPD50R380CE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "QM6006D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.jaolen.com/images/pdf/QM6006D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "35A Id, 60V Vds, N-Channel Power MOSFET, 18mOhm Ron, 19.3nC Qg (typ), TO252"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "RQ6E080AJ"
		(extends "DMN3033LDM")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "RQ6E080AJ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/mosfet/rq6e080ajtcr-e.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "8A Id, 30V Vds, 16.5 mOhm RdsOn, N-Channel Small-Signal MOSFET, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET Low-Threshold sot-457t sc-95 tsmt6"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "RS9N50D"
		(extends "IPD50R380CE")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "RS9N50D"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.denovocn.com/sites/default/files/RS9N50D.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "9A Id, 500V Vds, N-Channel Power MOSFET, 650mOhm Ron, 22nC Qg (typ), TO252"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFET high voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ100E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ100E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/71828/sqjq100e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "200A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.5mOhm Ron, 13nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ100EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ100EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/68443/sqjq100el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "200A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.5mOhm Ron, 20nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ112E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ112E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/79384/sqjq112e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "296A Id, 100V Vds, N-Channel TrenchFET MOSFET, 2.53mOhm Ron, 37nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ114EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ114EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62161/sqjq114el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "136A Id, 100V Vds, N-Channel TrenchFET MOSFET, 6.2mOhm Ron, 14nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ116EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ116EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62252/sqjq116el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "61A Id, 100V Vds, N-Channel TrenchFET MOSFET, 10.3mOhm Ron, 12nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ130EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ130EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/78005/sqjq130el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "445A Id, 30V Vds, N-Channel TrenchFET MOSFET, 0.7mOhm Ron, 56nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ140E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ140E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/79764/sqjq140e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "701A Id, 40V Vds, N-Channel TrenchFET MOSFET, 0.53mOhm Ron, 41nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ142E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ142E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/77320/sqjq142e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "345A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.24mOhm Ron, 20.1nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ144AE"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ144AE"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/77170/sqjq144ae.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "575A Id, 40V Vds, N-Channel TrenchFET MOSFET, 0.9mOhm Ron, 25nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ146E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ146E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62374/sqjq146e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "487A Id, 40V Vds, N-Channel TrenchFET MOSFET, 0.7mOhm Ron, 33nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ148E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ148E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/77269/sqjq148e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "375A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.6mOhm Ron, 24nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L LFPAK88"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ150E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ150E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/77649/sqjq150e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "233A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.9mOhm Ron, 17nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ160EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ160EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62138/sqjq160el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "461A Id, 60V Vds, N-Channel TrenchFET MOSFET, 1.1mOhm Ron, 31nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ184E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ184E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/77102/sqjq184e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "430A Id, 80V Vds, N-Channel TrenchFET MOSFET, 1.4mOhm Ron, 36nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ186E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ186E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62006/sqjq186e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "245A Id, 80V Vds, N-Channel TrenchFET MOSFET, 2.3mOhm Ron, 26nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ402E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ402E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62748/sqjq402e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "200A Id, 40V Vds, N-Channel TrenchFET MOSFET, 2mOhm Ron, 29nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ404E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ404E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/76570/sqjq404e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "200A Id, 40V Vds, N-Channel TrenchFET MOSFET, 1.72mOhm Ron, 27nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ410EL"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ410EL"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/76643/sqjq410el.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "135A Id, 100V Vds, N-Channel TrenchFET MOSFET, 4mOhm Ron, 20nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 Logic-Level PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ466E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ466E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/75138/sqjq466e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "200A Id, 60V Vds, N-Channel TrenchFET MOSFET, 1.9mOhm Ron, 14nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "SQJQ480E"
		(extends "SQJQ160E")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SQJQ480E"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:LFPAK88"
			(at 5.08 -3.81 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/76718/sqjq480e.pdf"
			(at 5.08 -6.35 0)
		)
		(property "Description" "150A Id, 80V Vds, N-Channel TrenchFET MOSFET, 3mOhm Ron, 21nC Qqd, -55 to 175 °C, LFPAK88"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power MOSFET N-MOS Automotive AEC-Q101 PowerPAK 8x8L"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFPAK88*"
			(at 0 0 0)
		)
	)
	(symbol "STB33N65M2"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "STB33N65M2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stb33n65m2.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "24A Id, 650V Vds, N-Channel MDmesh M2 MOSFET, 140mOhm Ron, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "STB40N60M2"
		(extends "STB15N80K5")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "STB40N60M2"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-263-2"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp40n60m2.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "34A Id, 600V Vds, N-Channel MDmesh M2 MOSFET, 78mOhm Ron, D2PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?263*"
			(at 0 0 0)
		)
	)
	(symbol "STS2DNE60"
		(extends "FDS6890A")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "STS2DNE60"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/CD00001537.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2A Id, 60V Vds, Dual N-Channel MOSFET, 180mOhm Ron, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SUD08P06-155L"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD08P06-155L"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62843/sud08p06-155l-ge3.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-8.4A Id, -60V Vds, TrenchFET P-Channel Power MOSFET, 155mOhm Ron, 19nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD09P10-195"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD09P10-195"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65903/SUD09P10.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-8.8A Id, -100V Vds, TrenchFET P-Channel Power MOSFET, 195mOhm Ron, 34.8nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD45P03-09"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD45P03-09"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65595/sud45p03.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-45A Id, -30V Vds, TrenchFET P-Channel Power MOSFET, 8.7mOhm Ron, 90nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD50P04-08"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD50P04-08"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65594/sud50p04-08.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-50A Id, -40V Vds, TrenchFET P-Channel Power MOSFET, 8.1mOhm Ron, 159nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD50P06-15"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD50P06-15"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/68940/sud50p06.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-50A Id, -60V Vds, TrenchFET P-Channel Power MOSFET, 15mOhm Ron, 165nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD50P08-25L"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD50P08-25L"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/73443/sud50p08.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-50A Id, -80V Vds, TrenchFET P-Channel Power MOSFET, 25.2mOhm Ron, 160nC Qg, -55 to 175 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "SUD50P10-43L"
		(extends "SUD19P06-60")
		(property "Reference" "Q"
			(at 4.953 1.905 0)
		)
		(property "Value" "SUD50P10-43L"
			(at 4.953 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 4.953 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/62504/sud50p10-43l-ge3.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-37A Id, -100V Vds, TrenchFET P-Channel Power MOSFET, 43mOhm Ron, 160nC Qg, -55 to 150 °C, TO-252-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TrenchFET P-Channel Power MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
	)
	(symbol "Si1308EDL"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si1308EDL"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/63399/si1308edl.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "30V Vds, 1.4A Id, N-Channel MOSFET, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?323*"
			(at 0 0 0)
		)
	)
	(symbol "Si2319CDS"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si2319CDS"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/66709/si2319cd.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-4.4A Id, -40V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "Si2371EDS"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si2371EDS"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/63924/si2371eds.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-3.6A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "Si4162DY"
		(extends "IRF8721PBF-1")
		(property "Reference" "Q"
			(at 5.08 2.54 0)
		)
		(property "Value" "Si4162DY"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/68967/si4162dy.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "19.3A Id, 30V Vds, TrenchFET N-Channel Power MOSFET, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4532DY"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si4532DY"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/SI4532DY-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.9A Id, 30V Vds, Dual N and P Channel MOSFET, 65mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si4542DY"
		(extends "IRF7309IPBF")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si4542DY"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/SI4542DY-D.PDF"
			(at 5.08 -3.81 0)
		)
		(property "Description" "Dual N and P Channel MOSFET, 6A Id, 30V Vds, 28mOhm Ron, 10V Vgs, SO8L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual N-Channel P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si7450DP"
		(extends "Si7336ADP")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si7450DP"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:PowerPAK_SO-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/71432/si7450dp.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "5.3A Id, 200V Vds, 80mOhm Ron, PowerPAK-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerPAK*SO*Single*"
			(at 0 0 0)
		)
	)
	(symbol "Si7617DN"
		(extends "Si7141DP")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Si7617DN"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Vishay_PowerPAK_1212-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65164/si7617dn.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-35A Id, -30V Vds, 0.0123 Ohm Ron, PowerPAK-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*1212*Single*"
			(at 0 0 0)
		)
	)
	(symbol "SiA449DJ"
		(extends "SiA453EDJ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiA449DJ"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Vishay_PowerPAK_SC70-6L_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/62644/sia449dj.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-12A Id, -30V Vds, P-Channel MOSFET, PowerPAK SC70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*SC70*Single*"
			(at 0 0 0)
		)
	)
	(symbol "SiR696DP"
		(extends "Si7336ADP")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiR696DP"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:PowerPAK_SO-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/65689/sir696dp.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "60A Id, 125V Vds N-Channel MOSFET, 9.6mOhm Ron, 19.4 nC Qg(typ), PowerPAK-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS NFET Vishay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PowerPAK*SO*Single*"
			(at 0 0 0)
		)
	)
	(symbol "SiS443DN"
		(extends "SiS415DNT")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiS443DN"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Vishay_PowerPAK_1212-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/63253/sis443dn.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-35A Id, -40V Vds, P-Channel MOSFET, PowerPAK 1212-8 Single"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*1212*Single*"
			(at 0 0 0)
		)
	)
	(symbol "SiSS27DN"
		(extends "SiS415DNT")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "SiSS27DN"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_SO:Vishay_PowerPAK_1212-8_Single"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/62847/siss27dn.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-50A Id, -30V Vds, P-Channel MOSFET, PowerPAK 1212-8 Single"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*PowerPAK*1212*Single*"
			(at 0 0 0)
		)
	)
	(symbol "T2N7002AK"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "T2N7002AK"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=29712&prodName=T2N7002AK"
			(at 0 0 0)
		)
		(property "Description" "60V Vds, 0.2A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TSM2301ACX"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TSM2301ACX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.taiwansemi.com/products/datasheet/TSM2301A_C15.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-2.8A Id, -20V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TSM2302CX"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TSM2302CX"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.taiwansemi.com/products/datasheet/TSM2302CX_E1608.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.9A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "VN10LF"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "VN10LF"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/VN10LF.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.15A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "VNP10N07"
		(extends "BUZ11")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "VNP10N07"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/vnp10n07.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "10A Id, 70V Vds, N-Channel Power MOSFET, fully autoprotected, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Power MOSFET OMNIFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "VP0610L"
		(extends "TP0610L")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "VP0610L"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70209/70209.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.18A Id, -60V Vds, P-Channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92L*"
			(at 0 0 0)
		)
	)
	(symbol "VP0610T"
		(extends "TP0610T")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "VP0610T"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70209/70209.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "-0.18A Id, -60V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "P-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZVN3306F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZVN3306F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZVN3306F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.15A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZVN3310F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZVN3310F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZVN3310F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.1A Id, 100V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZVN3320F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZVN3320F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZVN3320F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.06A Id, 200V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZVN4106F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZVN4106F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZVN4106F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.2A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXM61N02F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXM61N02F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXM61N02F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.7A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXM61N03F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXM61N03F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXM61N03F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.4A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN10A07F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN10A07F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN10A07F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "0.76A Id, 100V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2A01F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2A01F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2A01F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2A14F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2A14F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2A14F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.1A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2B01F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2B01F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2B01F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2.4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2B14FH"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2B14FH"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2B14FH.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.3A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2F30FH"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2F30FH"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2F30FH.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.9A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN2F34FH"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN2F34FH"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN2F34FH.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN3A01F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN3A01F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN3A01F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN3A14F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN3A14F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN3A14F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.2A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN3B01F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN3B01F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN3B01F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "2A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN3B14F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN3B14F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN3B14F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3.5A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN3F30FH"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN3F30FH"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN3F30FH.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "4.6A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXMN6A07F"
		(extends "BSS138")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "ZXMN6A07F"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ZXMN6A07F.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "1.4A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "RSQ030N08HZG"
		(extends "RQ6E080AJ")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "RSQ030N08HZG"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/mosfet/rsq030n08hzgtr-e.pdf"
			(at 5.08 -3.81 0)
		)
		(property "Description" "3A Id, 80V Vds, 131 mOhm RdsOn, N-Channel Small-Signal MOSFET, Body and ESD Diode, TSOT-23-6"
			(at 0.254 -14.986 0)
		)
		(property "ki_keywords" "nchan low threshold sot 457t sc 95 tsmt6"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
)
