(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DN2540N3-G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DN2540N3-G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/DN2540%20B060313.pdf"
			(at 0 -12.065 0)
		)
		(property "Description" "150mA Ids, 400 Vds, Depletion-mode N-channel MOSFET, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Depletion-Mode MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "DN2540N3-G_0_1")
		(symbol "DN2540N3-G_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DN2540N5-G"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DN2540N5-G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/DN2540%20B060313.pdf"
			(at 0 -12.065 0)
		)
		(property "Description" "150mA Ids, 400 Vds, Depletion-mode N-channel MOSFET, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Depletion-Mode MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "DN2540N5-G_0_1")
		(symbol "DN2540N5-G_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_DGS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_DGS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET, drain/gate/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_DGS_0_1")
		(symbol "Q_NMOS_Depletion_DGS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_DSG"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_DSG"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET drain/source/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_DSG_0_1")
		(symbol "Q_NMOS_Depletion_DSG_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_GDS"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_GDS"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET gate/drain/source"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_GDS_0_1")
		(symbol "Q_NMOS_Depletion_GDS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_GSD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_GSD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET gate/source/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_GSD_0_1")
		(symbol "Q_NMOS_Depletion_GSD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_SDG"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_SDG"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET source/drain/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_SDG_0_1")
		(symbol "Q_NMOS_Depletion_SDG_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Q_NMOS_Depletion_SGD"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "Q_NMOS_Depletion_SGD"
			(at 5.08 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Depletion-mode N-channel MOSFET source/gate/drain"
			(at 0 0 0)
		)
		(property "ki_keywords" "NMOS"
			(at 0 0 0)
		)
		(symbol "Q_NMOS_Depletion_SGD_0_1")
		(symbol "Q_NMOS_Depletion_SGD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DN2540N8-G"
		(extends "DN2540N5-G")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "DN2540N8-G"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/DN2540%20B060313.pdf"
			(at 0 -12.065 0)
		)
		(property "Description" "150mA Ids, 400 Vds, Depletion-mode N-channel MOSFET, SOT-89"
			(at 0 0 0)
		)
		(property "ki_keywords" "N-Channel Depletion-Mode MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
)
